<?xml version="1.0" encoding="utf-8" ?>
<!DOCTYPE erlref SYSTEM "erlref.dtd" [
  <!ENTITY gen_sctp '<seealso marker="kernel:gen_sctp">gen_sctp(3)</seealso>'>
  <!ENTITY gen_sctp_open1
  '<seealso marker="kernel:gen_sctp#open-1">gen_sctp:open/1</seealso>'>
  <!ENTITY ip_address
  '<seealso marker="kernel:inet#type-ip_address">inet:ip_address()</seealso>'>
  <!ENTITY inet '<seealso marker="kernel:inet">inet(3)</seealso>'>
  <!ENTITY % also SYSTEM "seealso.ent" >
  <!ENTITY % here SYSTEM "seehere.ent" >
  %also;
  %here;
]>

<erlref>
<header>
<copyright>
<year>2011</year>
<year>2016</year>
<holder>Ericsson AB. All Rights Reserved.</holder>
</copyright>
<legalnotice>
Licensed under the Apache License, Version 2.0 (the "License");
you may not use this file except in compliance with the License.
You may obtain a copy of the License at
 
    http://www.apache.org/licenses/LICENSE-2.0

Unless required by applicable law or agreed to in writing, software
distributed under the License is distributed on an "AS IS" BASIS,
WITHOUT WARRANTIES OR CONDITIONS OF ANY KIND, either express or implied.
See the License for the specific language governing permissions and
limitations under the License.

</legalnotice>

<title>diameter_sctp(3)</title>
<prepared>Anders Svensson</prepared>
<responsible></responsible>
<docno></docno>
<approved></approved>
<checked></checked>
<date></date>
<rev></rev>
<file>diameter_sctp.xml</file>
</header>

<module>diameter_sctp</module>
<modulesummary>Diameter transport over SCTP.</modulesummary>

<description>

<p>
This module implements diameter transport over SCTP using &gen_sctp;.
It can be specified as the value of a transport_module option to
&mod_add_transport;
and implements the behaviour documented in
&man_transport;.</p>

<marker id="start"/>
</description>

<!-- ===================================================================== -->

<funcs>

<func>
<name>start({Type, Ref}, Svc, [Opt])
         -> {ok, Pid, [LAddr]} | {error, Reason}</name>
<fsummary>Start a transport process.</fsummary>
<type>
<v>Type = connect | accept</v>
<v>Ref = &mod_transport_ref;</v>
<v>Svc = #diameter_service{}</v>
<v>Opt = OwnOpt | SctpOpt</v>
<v>Pid = pid()</v>
<v>LAddr = &ip_address;</v>
<v>Reason = term()</v>
<v>OwnOpt = {raddr, &ip_address;}
          | {rport, integer()}
          | {accept, Match}</v>
<v>SctpOpt = term()</v>
<v>Match = &ip_address; | string() | [Match]</v>
</type>
<desc>

<p>
The start function required by &man_transport;.</p>

<p>
Options <c>raddr</c> and <c>rport</c> specify the remote address
and port for a connecting transport and not valid for a listening
transport: the former is required while latter defaults to 3868 if
unspecified.
Multiple <c>raddr</c> options can be specified, in which case the
connecting transport in question attempts each in sequence until
an association is established.</p>

<p>
Option <c>accept</c> specifies remote addresses for a listening
transport and is not valid for a connecting transport.
If specified, a remote address that does not match one of the
specified addresses causes the association to be aborted.
Multiple <c>accept</c> options can be specified.
A string-valued <c>Match</c> that does not parse as an address is
interpreted as a regular expression.</p>

<p>
Remaining options are any accepted by &gen_sctp_open1;, with the exception
of options <c>mode</c>, <c>binary</c>, <c>list</c>, <c>active</c>
and <c>sctp_events</c>.
Note that options <c>ip</c> and <c>port</c> specify the local address
and port respectively.</p>

<p>
Multiple <c>ip</c> options can be specified for a multihomed peer.
If none are specified then the values of <c>Host-IP-Address</c>
in the <c>diameter_service</c> record are used.
(In particular, one of these must be specified.)
Option <c>port</c> defaults to 3868 for a listening transport and 0 for a
connecting transport.</p>

<warning>
<p>
An insufficiently large receive buffer may result in a peer having to
resend incoming messages: set the &inet; option <c>recbuf</c> to increase
the buffer size.</p>

<p>
An insufficiently large send buffer may result in outgoing messages
being discarded: set the &inet; option <c>sndbuf</c> to increase
the buffer size.</p>
</warning>

<p>
The <c>transport_data</c> field of record <c>diameter_packet</c>
is used to communicate the stream on which an inbound message
has been received, or on which an outbound message should be sent.
The value will be of the form <c>{stream, Id}</c> for an inbound
message passed to a &app_handle_request; or &app_handle_answer;
callback.
For an outbound message, <c>{outstream, Id}</c> in the return value of
&app_handle_request; or &app_prepare_retransmit; sets the outbound
stream, the stream id being interpreted modulo the number of outbound
streams.
Any other value, or not setting a value, causes successive such sends
to cycle though all outbound streams.</p>
</desc>
</func>

</funcs>

<!-- ===================================================================== -->
<!-- ===================================================================== -->

<section>
<title>SEE ALSO</title>

<p>
&man_main;, &man_transport;, &gen_sctp;, &inet;</p>

</section>

</erlref>
