<?xml version="1.0" encoding="utf-8" ?>
<!DOCTYPE chapter SYSTEM "chapter.dtd">

<chapter>
  <header>
    <copyright>
      <year>1997</year><year>2016</year>
      <holder>Ericsson AB. All Rights Reserved.</holder>
    </copyright>
    <legalnotice>
      Licensed under the Apache License, Version 2.0 (the "License");
      you may not use this file except in compliance with the License.
      You may obtain a copy of the License at
 
          http://www.apache.org/licenses/LICENSE-2.0

      Unless required by applicable law or agreed to in writing, software
      distributed under the License is distributed on an "AS IS" BASIS,
      WITHOUT WARRANTIES OR CONDITIONS OF ANY KIND, either express or implied.
      See the License for the specific language governing permissions and
      limitations under the License.
    
    </legalnotice>

    <title>Definition of Agent Net if</title>
    <prepared></prepared>
    <responsible></responsible>
    <docno></docno>
    <approved></approved>
    <checked></checked>
    <date></date>
    <rev></rev>
    <file>snmp_agent_netif.xml</file>
  </header>
  <p></p>
  <image file="snmp_agent_netif_1.gif">
    <icaption>The Purpose of Agent Net if</icaption>
  </image>
  <p>The Network Interface (Net if) process delivers SNMP PDUs to a
    master agent, and receives SNMP PDUs from the master agent. The most
    common behaviour of a Net if process is that is receives bytes from
    a network, decodes them into an SNMP PDU, which it sends to a master
    agent. When the master agent has processed the PDU, it sends a
    response PDU to the Net if process, which encodes the PDU into bytes
    and transmits the bytes onto the network.
    </p>
  <p>However, that simple behaviour can be modified in numerous
    ways. For example, the Net if process can apply some kind of
    encrypting/decrypting scheme on the bytes or
    act as a proxy filter, which sends some packets to a proxy agent and
    some packets to the master agent.
    </p>
  <p>It is also possible to write your own Net if process. The default
    Net if process is implemented in the module <c>snmpa_net_if</c> and
    it uses UDP as the transport protocol i.e the transport domains
    <c>transportDomainUdpIpv4</c> and/or <c>transportDomainUdpIpv6</c>.
    </p>
  <p>This section describes how to write a Net if process.
    </p>

  <section>
    <marker id="mandatory_functions"></marker>
    <title>Mandatory Functions</title>
    <p>A Net if process must implement the SNMP agent 
      <seealso marker="snmpa_network_interface">network interface behaviour</seealso>.
      </p>
  </section>

  <section>
    <marker id="messages"></marker>
    <title>Messages</title>
    <p>The section <em>Messages</em> describes mandatory messages, which
      Net if must send and be able to receive.     
      </p>
    <p>In this section an <c>Address</c> field is a
    <c>{Domain, Addr}</c> tuple where <c>Domain</c> is
    <c>transportDomainUdpIpv4</c> or <c>transportDomainUdpIpv4</c>,
    and <c>Addr</c> is an
    <c>{</c><seealso marker="kernel:inet#type-ip_address"><c>IpAddr</c></seealso><c>,IpPort}</c> tuple.</p>

    <section>
      <marker id="outgoing_messages"></marker>
      <title>Outgoing Messages</title>
      <p>Net if must send the following message when it receives an
      SNMP PDU from the network that is aimed for the MasterAgent:
      </p>
      <marker id="om_snmp_pdu"></marker>
      <pre>
MasterAgent ! {snmp_pdu, Vsn, Pdu, PduMS, ACMData, From, Extra}
      </pre>
      <list type="bulleted">
        <item><c>Vsn</c> is either <c>'version-1'</c>,
        <c>'version-2'</c>, or <c>'version-3'</c>.
        </item>
        <item><c>Pdu</c> is an SNMP PDU record, as defined in
        <c>snmp_types.hrl</c>, with the SNMP request.
        </item>
        <item><c>PduMS</c> is the Maximum Size of the response Pdu
         allowed.  Normally this is returned from
        <c>snmpa_mpd:process_packet</c> (see Reference Manual).
        </item>
        <item><c>ACMData</c> is data used by the Access Control Module
         in use.  Normally this is returned from
        <c>snmpa_mpd:process_packet</c> (see Reference Manual).
        </item>
        <item><c>From</c> is the source <c>Address</c>.
        </item>
        <item><c>Extra</c> is any term the Net if process wishes to
         send to the agent. This term can be retrieved by the
         instrumentation functions by calling
        <c>snmp:current_net_if_data()</c>. This data is also sent back
         to the Net if process when the agent generates a response to
         the request.</item>
      </list>
      <p>The following message is used to report that a response to a
      request has been received.  The only request an agent can send
      is an Inform-Request.
      </p>
      <marker id="om_snmp_response_received"></marker>
      <pre>
Pid ! {snmp_response_received, Vsn, Pdu, From}
      </pre>
      <list type="bulleted">
        <item><c>Pid</c> is the Process that waits for the response
         for the request.  The Pid was specified in the
        <c>send_pdu_req</c> message 
	<seealso marker="#im_send_pdu_req">(see below)</seealso>.
        </item>
        <item><c>Vsn</c> is either <c>'version-1'</c>, <c>'version-2'</c>, or
        <c>'version-3'</c>.
        </item>
        <item><c>Pdu</c> is the SNMP Pdu received
        </item>
        <item><c>From</c> is the source <c>Address</c>.
        </item>
      </list>
    </section>

    <section>
      <marker id="incoming_messages"></marker>
      <title>Incoming Messages</title>
      <p>This section describes the incoming messages which a Net if
      process must be able to receive.
      </p>
      <list type="bulleted">
        <item>
	  <marker id="im_snmp_response"></marker>
          <p><c>{snmp_response, Vsn, Pdu, Type, ACMData, To, Extra}</c></p>
          <p>This message is sent to the Net if process from a master
            agent as a response to a previously received request.
            </p>
          <list type="bulleted">
            <item>
	      <p><c>Vsn</c> is either <c>'version-1'</c>,
	      <c>'version-2'</c>, or <c>'version-3'</c>. </p>
            </item>
            <item>
	      <p><c>Pdu</c> is an SNMP PDU record (as defined in
	      snmp_types.hrl) with the SNMP response. </p>
            </item>
            <item>
	      <p><c>Type</c> is the <c>#pdu.type</c> 
	      of the original request. </p>
            </item>
            <item>
	      <p><c>ACMData</c> is data used by the Access Control
	      Module in use.  Normally this is just sent to
	      <c>snmpa_mpd:generate_response_message</c> 
	      (see Reference Manual). </p>
            </item>
            <item>
	      <p><c>To</c> is the destination <c>Address</c> that comes
	      from the <c>From</c> field in the corresponding <c>snmp_pdu</c>
	      message previously sent to the MasterAgent.</p>
            </item>
            <item>
	      <p><c>Extra</c> is the term that the Net if process
	      sent to the agent when the request was sent to the agent. </p>
            </item>
          </list>
        </item>
        <item>
	  <marker id="im_discarded_pdu"></marker>
          <p><c>{discarded_pdu, Vsn, ReqId, ACMData, Variable, Extra}</c></p>
          <p>This message is sent from a master agent if it for some
	  reason decided to discard the pdu. </p>
          <list type="bulleted">
            <item>
	      <p><c>Vsn</c> is either <c>'version-1'</c>,
	      <c>'version-2'</c>, or <c>'version-3'</c>. </p>
            </item>
            <item>
	      <p><c>ReqId</c> is the request id of the original request. </p>
            </item>
            <item>
	      <p><c>ACMData</c> is data used by the Access Control
	      Module in use. Normally this is just sent to
	      <c>snmpa_mpd:generate_response_message</c> 
	      (see Reference Manual). </p>
            </item>
            <item>
	      <p><c>Variable</c> is the name of an snmp counter that
	      represents the error, e.g. <c>snmpInBadCommunityUses</c>. </p>
            </item>
            <item>
	      <p><c>Extra</c> is the term that the Net if process
	      sent to the agent when the request was sent to the agent. </p>
            </item>
          </list>
        </item>
        <item>
	  <marker id="im_send_pdu"></marker>
          <p><c>{send_pdu, Vsn, Pdu, MsgData, To, Extra}</c></p>
          <p>This message is sent from a master agent when a trap is
            to be sent. </p>
          <list type="bulleted">
            <item>
	      <p><c>Vsn</c> is either <c>'version-1'</c>,
	      <c>'version-2'</c>, or <c>'version-3'</c>.</p>
            </item>
	    <item>
	      <p><c>Pdu</c> is an SNMP PDU record (as defined in
	      snmp_types.hrl) with the SNMP response. </p>
	    </item>
            <item>
	      <p><c>MsgData</c> is the message specific data used in
	      the SNMP message.  This value is normally sent to
	      <c>snmpa_mpd:generate_message/4</c>.  In SNMPv1 and
	      SNMPv2c, this message data is the community string.  In
	      SNMPv3, it is the context information. </p>
            </item>
            <item>
	      <p><c>To</c> is a list of <c>{Address, SecData}</c>
	      tuples i.e the destination addresses and
	      their corresponding security parameters.  This value is
	      normally sent to <c>snmpa_mpd:generate_message/4</c>. </p>
            </item>
            <item>
	      <p><c>Extra</c> is any term that the notification sender
	      wishes to pass to the Net if process when sending a notification 
	      (see 
	      <seealso marker="snmpa#send_notification2">send notification
	      </seealso> for more info). </p>
            </item>
          </list>
        </item>
        <item>
	  <marker id="im_send_pdu_req"></marker>
          <p><c>{send_pdu_req, Vsn, Pdu, MsgData, To, Pid, Extra}</c></p>
          <p>This message is sent from a master agent when a request is to 
	  be sent.  The only request an agent can send is Inform-Request.  
	  The net if process needs to remember the request id and the Pid, 
	  and when a response is received for the request id, send it to Pid, 
	  using a <c>snmp_response_received</c> message. </p>
	  <list type="bulleted">
	    <item>
	      <p><c>Vsn</c> is either <c>'version-1'</c>,
	      <c>'version-2'</c>,  or <c>'version-3'</c>.</p>
	    </item>
	    <item>
	      <p><c>Pdu</c> is an SNMP PDU record (as defined in
	      snmp_types.hrl) with the SNMP response. </p>
	    </item>
	    <item>
	      <p><c>MsgData</c> is the message specific data used in
	      the SNMP message.  This value is normally sent to
	      <c>snmpa_mpd:generate_message/4</c>. In SNMPv1 and
	      SNMPv2c, this message data is the community string. In
	      SNMPv3, it is the context information. </p>
	    </item>
	    <item>
	      <p><c>To</c> is a list of <c>{Address, SecData}</c>
	      tuples i.e the destination addresses and
	      their corresponding security parameters. This value is
	      normally sent to <c>snmpa_mpd:generate_message/4</c>. </p>
	    </item>
	    <item>
	      <p><c>Pid</c> is a process identifier. </p>
	    </item>
            <item>
	      <p><c>Extra</c> is any term that the notification sender
	      wishes to pass to the Net if process when sending a notification 
	      (see 
	      <seealso marker="snmpa#send_notification2">send notification
	      </seealso> for more info). </p>
            </item>
	  </list>
        </item>
      </list>
    </section>

    <section>
      <title>Notes</title>
      <p>Since the Net if process is responsible for encoding and
        decoding of SNMP messages, it must also update the relevant
        counters in the SNMP group in MIB-II. It can use the functions
        in the module <c>snmpa_mpd</c> for this purpose (refer to the 
        Reference Manual, section <c>snmp</c>, 
        module <seealso marker="snmp_pdus">snmpa_mpd</seealso>
        for more details.)
        </p>
      <p>There are also some useful functions for encoding and
        decoding of SNMP messages in the module 
        <seealso marker="snmp_pdus">snmp_pdus</seealso>.
        </p>
    </section>
  </section>
</chapter>

