Configuration Variables for sctp
================================

                  [ this file is autogenerated, do not edit ]


 1. sctp.socket_rcvbuf
        socket receive buffer size (read-only).
        Range: 512 - 102400.
        Type: integer. Read-only.

 2. sctp.socket_sndbuf
        socket send buffer size (read-only).
        Range: 512 - 102400.
        Type: integer. Read-only.

 3. sctp.autoclose
        seconds before closing and idle connection (must be non-zero).
        Range: 1 - 1073741824.
        Type: integer.

 4. sctp.send_ttl
        milliseconds before aborting a send.
        Range: 0 - 1073741824.
        Type: integer.

 5. sctp.send_retries
        re-send attempts on failure.
        Range: 0 - 9.
        Type: integer.

 6. sctp.assoc_tracking
        connection/association tracking (see also assoc_reuse).
        Range: 0 - 1.
        Type: integer.

 7. sctp.assoc_reuse
        connection/association reuse (for now used only for replies),
        depends on assoc_tracking being set.
        Range: 0 - 1.
        Type: integer.

 8. sctp.max_assocs
        maximum allowed open associations (-1 = disable, as many as
        allowed by the OS).
        Type: integer.

 9. sctp.srto_initial
        initial value of the retr. timeout, used in RTO calculations,
        in msecs.
        Range: 0 - 1073741824.
        Type: integer.

10. sctp.srto_max
        maximum value of the retransmission timeout (RTO), in msecs.
        Range: 0 - 1073741824.
        Type: integer.

11. sctp.srto_min
        minimum value of the retransmission timeout (RTO), in msecs.
        Range: 0 - 1073741824.
        Type: integer.

12. sctp.asocmaxrxt
        maximum retransmission attempts per association.
        Range: 0 - 1024.
        Type: integer.

13. sctp.init_max_attempts
        max INIT retransmission attempts.
        Range: 0 - 1024.
        Type: integer.

14. sctp.init_max_timeo
        max INIT retransmission timeout (RTO max for INIT), in msecs.
        Range: 0 - 1073741824.
        Type: integer.

15. sctp.hbinterval
        heartbeat interval in msecs.
        Range: 0 - 1073741824.
        Type: integer.

16. sctp.pathmaxrxt
        maximum retransmission attempts per path.
        Range: 0 - 1024.
        Type: integer.

17. sctp.sack_delay
        time since the last received packet before sending a SACK, in
        msecs.
        Range: 0 - 1073741824.
        Type: integer.

18. sctp.sack_freq
        number of received packets that trigger the sending of a SACK.
        Range: 0 - 1024.
        Type: integer.

19. sctp.max_burst
        maximum burst of packets that can be emitted by an association.
        Range: 0 - 1024.
        Type: integer.

