Things to look into:

* RFC3261, section 12.1.1 requires UAS to copy Record-Route
* Check to see if any memory leaks.
* Should probably respond when caller says BYE after queue says BYE.
* check RAck number
