# $Id$
#
# History:
# --------
#  2009-05-07  created by Andrei Pelinescu-Onciul <andrei@iptel.org>


Overview
========

kamcmd is a unix tool for interfacing with Kamailio using exported RPCs.
It uses binrpc (a proprietary protocol, designed for minimal packet size and
fast parsing) over a variety of transports (unix stream sockets, unix datagram
 sockets, udp or tcp).
For more details on binrpc see the ctl module documentation
(modules/ctl/README).

kamcmd can work in command line mode (the RPC or command name is just another
command line parameter) or in interactive mode. The interactive mode supports
history and tab-completion (if kamcmd was compiled with libreadline support).

On Kamailio side the ctl module must be loaded.

Usage
=====

	kamcmd [options][-s address] [ cmd ]

Options:
    -s address  unix socket name or host name to send the commands on
    -R name     force reply socket name, for the unix datagram socket mode
    -D dir      create the reply socket in the directory <dir> if no reply
                socket is forced (-R) and a unix datagram socket is selected
                as the transport
    -f format   print the result using format. Format is a string containing
                %v at the places where values read from the reply should be
                substituted. To print '%v', escape it using '%': %%v.
    -v          Verbose 
    -V          Version number
    -h          Help message
address:
    [proto:]name[:port]   where proto is one of tcp, udp, unixs, unix or unixd
                          e.g.:  tcp:localhost:2049 , unixs:/tmp/ser_ctl
                          If the protocol is not specified, unixs will be
                          used if name is a filesystem path and udp if not.
                          "unixs" or "unix" stand for unix stream sockets
                          and "unixd" for unix datagram sockets.
cmd:
    method  [arg1 [arg2...]]
arg:
     string or number; to force a number to be interpreted as string 
     prefix it by "s:", e.g. s:1

If no address is specified (no -s), kamcmd will use  by default
unixs:/tmp/ser_ctl. This is also the default for the ctl module (if no
 "binrpc" module parameters are present in the config).


Command Types
=============

There are 3 types of commands: "raw" RPC, kamcmd aliases and kamcmd
 builtins.

The "raw" RPC commands work directly with ser with no change on the input or
 the output.
To list available RPC commands, use "kamcmd help".

The aliases are just easier to remember names for some RPCs, which
some time include nicer formatting of the RPC result.
One can see all the defined aliases using: kamcmd help|grep alias: .
Example:
 ps is an alias for core.ps with the output formatted in a more readable way.
 kamcmd ps is equivalent to kamcmd -f"%v\t%v\n" core.ps.
 Without the formatting, the output of kamcmd core.ps looks like:

11262
attendant
11268
udp receiver child=0 sock=127.0.0.1:5060
...
 Using kamcmd ps (or  kamcmd -f"%v\t%v\n" core.ps) the output looks like:

11262	attendant
11268	udp receiver child=0 sock=127.0.0.1:5060
...

The built-in commands can combine several different rpcs.
One can see all the built-in commands using: kamcmd help|grep builtin: .

Getting help on a command
=========================

To get the help message associated with a command use 
kamcmd help <command_name>.
Example:
$ kamcmd help ps
ps is an alias for core.ps with reply formatting: "%v\t%v\n"
$ kamcmd help core.ps
Returns the description of running Kamailio processes.


Listing all the commands
========================

To see all the available commands (ser RPCs, aliases and bultins) use
 kamcmd help.
To see only the "raw" RPCs, user kamcmd ls.
Note: since each module can define its own RPCs, the available RPCs depend
 on the loaded modules.


Examples
========

Using the default socket (requires only loadmodule "ctl" in ser.cfg):

$ kamcmd ps
11262	attendant
11268	udp receiver child=0 sock=127.0.0.1:5060
11269	udp receiver child=1 sock=127.0.0.1:5060
11270	udp receiver child=0 sock=192.168.1.101:5060
11271	udp receiver child=1 sock=192.168.1.101:5060
11272	slow timer
11273	timer
11274	ctl handler
11275	tcp receiver child=0
11276	tcp receiver child=1
11277	tcp main process

$ kamcmd help  # list all the supported commands
dst_blocklist.add
ctl.who
...

$ kamcmd help core.uptime # help for the core.uptime rpc
Returns uptime of the Kamailio server.

$ kamcmd cfg.cfg_set_int_now debug 5 # turn debug level to 5 (needs cfg)

$ kamcmd # enters interactive mode

Using a tcp socket
(assumes modparam("ctl", "binrpc", "tcp:localhost:2049") in kamailio.cfg)

$ kamcmd -s tcp:localhost:2049 core.version
Server: Kamailio (3.3.2 (i386/linux))

$ kamcmd -s tcp:localhost:2049 SRV _sip._udp.iptel.org
    name: _sip._udp.iptel.org
    type: SRV
    size (bytes): 104
    reference counter: 2
    expires in (s): 67693
    last used (s): 0
    error flags: 0
    rr name: sip.iptel.org
    rr port: 5060
    rr priority: 0
    rr weight: 0
    rr expires in (s): 67693
    rr error flags: 0

kamcmd -s tcp:127.0.0.1:2049  # enters interactive mode over tcp

For more examples see utils/kamcmd/EXAMPLES
 [http://git.sip-router.org/cgi-bin/gitweb.cgi?p=sip-router;a=blob;f=utils/kamcmd/EXAMPLES].


Interactive Mode
================

To enter the interactive mode start kamcmd without specifying a command name
 on the command line.
If kamcmd was compiled with libreadline support (automatically if
libreadline dev files are installed), the interactive mode will have tab
completion and history support.

Example:

$ kamcmd
kamcmd 0.2
Copyright 2006 iptelorg GmbH
This is free software with ABSOLUTELY NO WARRANTY.
For details type `warranty'.
kamcmd> core.s<tab>
core.sctp_info     core.sctp_options  core.shmmem
kamcmd> help core.shmmem 
Returns shared memory info.
kamcmd> core.shmmem
{
	total: 33554432
	free: 33147816
	used: 190644
	real_used: 406616
	max_used: 406616
	fragments: 2
}
kamcmd> quit


Related Stuff
=============

* ctl module: required, implements binrpc on Kamailio side, without it kamcmd doesn't work.

See modules/ctl/README
 [http://git.sip-router.org/cgi-bin/gitweb.cgi?p=sip-router;a=blob;f=modules_s/ctl/README].

* cfg_rpc module: allows setting or reading configuration parameters on-the-fly.
	For example one could change the tcp connection lifetime to 180s using:
	$ kamcmd cfg.set_now_int tcp.connection_lifetime 180
	See modules/cfg_rpc/README
 	[http://git.sip-router.org/cgi-bin/gitweb.cgi?p=sip-router;a=blob;f=modules_s/cfg_rpc/README].
