<?xml version="1.0" encoding="ISO-8859-1"?>
<!DOCTYPE book PUBLIC "-//OASIS//DTD DocBook XML V4.4//EN"
"http://www.oasis-open.org/docbook/xml/4.4/docbookx.dtd" [
<!-- Include general documentation entities -->
<!ENTITY % docentities SYSTEM "../../../../doc/docbook/entities.xml">
%docentities;
]>
<!-- Auth_db Module User's Guide -->
<chapter>
  <title>&adminguide;</title>

  <section>
    <title>Overview</title>

    <para>This module contains all method related to the IMS policy and
    charging control functions performed by an Application Function (e.g.
    P-CSCF) over the Rx interface. This module is dependent on the CDP (C
    Diameter Peer) modules for communicating with PCRF as specified in 3GPP
    specification TS 29.214.</para>
  </section>

  <section>
    <title>Dependencies</title>

    <section>
      <title>&kamailio; Modules</title>

      <para>The Following modules must be loaded before this module:</para>

      <itemizedlist>
        <listitem>
          <para>IMS Dialog</para>
        </listitem>

        <listitem>
          <para>Usrloc PCSCF</para>
        </listitem>

        <listitem>
          <para>TM - Transaction Manager</para>
        </listitem>

        <listitem>
          <para>CDP - C Diameter Peer</para>
        </listitem>

        <listitem>
          <para>CDP_AVP - CDP AVP Applications</para>
        </listitem>
      </itemizedlist>
    </section>

    <section>
      <title>External Libraries or Applications</title>

      <para>This module requires the internal IMS library.</para>
    </section>
  </section>

  <section>
    <title>Parameters</title>

    <section>
      <title><varname>rx_dest_realm</varname> (string)</title>

      <para>This is the name of the Diameter realm of the Diameter server
      (typically a PCRF).</para>

      <para><emphasis> Default value is 'ims.smilecoms.com'.
      </emphasis></para>

      <example>
        <title><varname>rx_dest_realm</varname> parameter usage</title>

        <programlisting format="linespecific">
...
modparam("ims_qos", "rx_dest_realm", "ims.smilecoms.com")
...
        </programlisting>
      </example>
    </section>

    <section>
      <title><varname>rx_forced_peer</varname> (string)</title>

      <para>FQDN of the Diameter server (typically a PCRF) to communicate
      with. If not set then realm routing is used. If you use this, the
      routing defined in your diameter xml configuration file (CDP) will be
      ignored and as a result you will lose the benefits of load balancing and
      failover. </para>

      <para><emphasis> Default value is ''. </emphasis></para>

      <example>
        <title><varname>rx_forced_peer</varname> parameter usage</title>

        <programlisting format="linespecific">
...
modparam("ims_qos", "rx_forced_peer", "pcrf.ims.smilecoms.com")
...
        </programlisting>
      </example>
    </section>

    <section>
      <title><varname>rx_auth_expiry</varname> (integer)</title>

      <para>This is the expiry length in seconds of the initiated Diameter
      sessions.</para>

      <para><emphasis> Default value is 7200. </emphasis></para>

      <example>
        <title><varname>rx_auth_expiry</varname> parameter usage</title>

        <programlisting format="linespecific">
...
modparam("ims_qos", "rx_auth_expiry", 14400)
...
        </programlisting>
      </example>
    </section>

    <section>
      <title><varname>cdp_event_latency</varname> (integer)</title>

      <para>This is a flag to determine whether or slow CDP responses should
      be reported in the log file. 1 is enabled and 0 is disabled.</para>

      <para><emphasis> Default value is 1. </emphasis></para>

      <example>
        <title><varname>cdp_event_latency</varname> parameter usage</title>

        <programlisting format="linespecific">
...
modparam("ims_qos", "cdp_event_latency", 1)
...
        </programlisting>
      </example>
    </section>

    <section>
      <title><varname>cdp_event_threshold</varname> (integer)</title>

      <para>This time in milliseconds is the limit we should report a CDP
      response as slow. i.e. if a CDP response exceeds this limit it will be
      reported in the log file. This is only relevant is cdp_event_latency is
      enabled (set to 0).</para>

      <para><emphasis> Default value is 500. </emphasis></para>

      <example>
        <title><varname>cdp_event_threshold</varname> parameter usage</title>

        <programlisting format="linespecific">
...
modparam("ims_qos", "cdp_event_threshold", 500)
...
        </programlisting>
      </example>
    </section>

    <section>
      <title><varname>cdp_event_latency_log</varname> (integer)</title>

      <para>This time log level at which we should report slow CDP responses.
      0 is ERROR, 1 is WARN, 2 is INFO and 3 is DEBUG. This is only relevant
      is cdp_event_latency is enabled (set to 0)</para>

      <para><emphasis> Default value is 0. </emphasis></para>

      <example>
        <title><varname>cdp_event_latency_log</varname> parameter
        usage</title>

        <programlisting format="linespecific">
...
modparam("ims_qos", "cdp_event_latency_log", 1)
...
        </programlisting>
      </example>
    </section>
    <section>
      <title><varname>authorize_video_flow</varname> (integer)</title>

      <para>This is a flag that specifies whether or not to authorize video flows.
      1 means video flows will be authorized over Rx and
      0 means video flows will not be authorized over Rx</para>

      <para><emphasis> Default value is 1. </emphasis></para>

      <example>
        <title><varname>authorize_video_flow</varname> parameter
        usage</title>

        <programlisting format="linespecific">
...
modparam("ims_qos", "authorize_video_flow", 0)
...
        </programlisting>
      </example>
    </section>
    <section>
      <title><varname>cdp_event_list_size_threshold</varname> (integer)</title>

      <para>This is a threshold on the size of the cdp event list.  Once the
	queue exceeds this length a warning is logged.  0 disables this feature</para>

      <para><emphasis> Default value is 0. </emphasis></para>

      <example>
        <title><varname>cdp_event_list_size_threshold</varname> parameter
        usage</title>

        <programlisting format="linespecific">
...
modparam("ims_qos", "cdp_event_list_size_threshold", 10)
...
        </programlisting>
      </example>
    </section>
    <section>
      <title><varname>audio_default_bandwidth</varname> (integer)</title>

      <para>This parameters defines the default bandwidth for Audio,
            if no "b=AS"-Parameter is found in the SDP.</para>

      <para><emphasis> Default value is 64 (64 kBit)</emphasis></para>

      <example>
        <title><varname>audio_default_bandwidth</varname> parameter
        usage</title>

        <programlisting format="linespecific">
...
modparam("ims_qos", "audio_default_bandwidth", 32)
...
        </programlisting>
      </example>
    </section>
    <section>
      <title><varname>video_default_bandwidth</varname> (integer)</title>

      <para>This parameters defines the default bandwidth for Video,
            if no "b=AS"-Parameter is found in the SDP.</para>

      <para><emphasis> Default value is 128 (128 kBit)</emphasis></para>

      <example>
        <title><varname>video_default_bandwidth</varname> parameter
        usage</title>

        <programlisting format="linespecific">
...
modparam("ims_qos", "video_default_bandwidth", 256)
...
        </programlisting>
      </example>
    </section>
    <section>
      <title><varname>early_qosrelease_reason</varname> (String)</title>

      <para>This sets the default Reason, when a call is terminated in
            early stage due to QoS-failure.</para>

      <para><emphasis> Default value is "QoS released", a call in early stage
		       would be released with "488 QoS released".</emphasis></para>

      <example>
        <title><varname>early_qosrelease_reason</varname> parameter
        usage</title>

        <programlisting format="linespecific">
...
modparam("ims_qos", "early_qosrelease_reason", "Sorry - QoS failed")
...
        </programlisting>
      </example>
    </section>
    <section>
      <title><varname>confirmed_qosrelease_headers</varname> (String)</title>

      <para>These headers are added to the BYE-Message, when a confirmed call
	    is terminated due to a QoS failure.</para>

      <para><emphasis> Default value is "", no Extra-Headers</emphasis></para>

      <para><emphasis> The headers must end with CRLF.</emphasis></para>

      <example>
        <title><varname>confirmed_qosrelease_headers</varname> parameter
        usage</title>

        <programlisting format="linespecific">
...
modparam("ims_qos", "confirmed_qosrelease_headers", "X-Reason: QoS failed\r\n")
...
        </programlisting>
      </example>
    </section>

    <section>
      <title><varname>regex_sdp_ip_prefix_to_maintain_in_fd</varname> (String)</title>

      <para>The flow-description AVP is typically populated using IP:port information
          present in the SDP.  Certain (buggy) UEs can change ports midway during
          calls which causes the flow-description to no longer match the
          traffic.  This parameter allows the flow-description AVP to use to the
          any keyword instead of certain IP:port combinations in the SDP. The
          parameter is a regex that if set adds an extra filter for all IPs that do not match
          the regex with the any keyword in the flow-description AVP</para>

      <para><emphasis> Default value is "", no extra filters added</emphasis></para>

      <example>
        <title><varname>regex_sdp_ip_prefix_to_maintain_in_fd</varname> parameter
        usage</title>

        <programlisting format="linespecific">
...
modparam("ims_qos", "regex_sdp_ip_prefix_to_maintain_in_fd", "10.21.0.1")
...
        </programlisting>
      </example>
    </section>

    <section>
      <title><varname>terminate_dialog_on_rx_failure</varname> integer</title>

      <para>If set then active dialogs associated with an Rx session are
      torn down in the Rx session fails</para>

      <para><emphasis> Default value is 1, dialogs are torn down</emphasis></para>

      <example>
        <title><varname>terminate_dialog_on_rx_failure</varname> parameter
        usage</title>

        <programlisting format="linespecific">
...
modparam("ims_qos", "terminate_dialog_on_rx_failure", 0)
...
        </programlisting>
      </example>
    </section>

    <section>
      <title><varname>delete_contact_on_rx_failure</varname> integer</title>

      <para>If set then contacts associated with signalling Rx sessions are deleted
if the Rx session fails</para>

      <para><emphasis> Default value is 1, contacts are deleted</emphasis></para>

      <example>
        <title><varname>delete_contact_on_rx_failure</varname> parameter
        usage</title>

        <programlisting format="linespecific">
...
modparam("ims_qos", "delete_contact_on_rx_failure", 0)
...
        </programlisting>
      </example>
    </section>

    <section>
      <title><varname>include_rtcp_fd</varname> integer</title>

      <para>If set then a flow description is added for media flows - next available odd port
          is used as the default for RTCP traffic</para>

      <para><emphasis> Default value is 0, RTCP flow description not added</emphasis></para>

      <example>
        <title><varname>include_rtcp_fd</varname> parameter
        usage</title>

        <programlisting format="linespecific">
...
modparam("ims_qos", "include_rtcp_fd", 1)
...
        </programlisting>
      </example>
    </section>

    <section>
      <title><varname>af_signaling_ip</varname> (String)</title>

      <para>Set P-CSCF IPv4 address to generate the flows for the UE - PCSCF signaling path. Used only for AAR register, Flow-Description AVP (507)</para>

      <para><emphasis> Default value is 127.0.0.1</emphasis></para>

      <example>
        <title><varname>af_signaling_ip</varname> parameter
        usage</title>

        <programlisting format="linespecific">
...
modparam("ims_qos", "af_signaling_ip", "127.0.0.1")
...
        </programlisting>
      </example>
    </section>

    <section>
      <title><varname>af_signaling_ip6</varname> (String)</title>

      <para>Set P-CSCF IPv6 address to generate the flows for the UE - PCSCF signaling path. Used only for AAR register, Flow-Description AVP (507)</para>

      <para><emphasis> Default value is ""</emphasis></para>

      <example>
        <title><varname>af_signaling_ip6</varname> parameter
        usage</title>

        <programlisting format="linespecific">
...
modparam("ims_qos", "af_signaling_ip6", "fd16::205:2dee:ce4a:ab22")
...
        </programlisting>
      </example>
    </section>

    <section>
      <title><varname>media_type</varname> (String)</title>

      <para>Describe Media Type AVP(520) for AAR register</para>

      <para><emphasis> Default value is 'control'</emphasis></para>

      <example>
        <title><varname>media_type</varname> parameter
        usage</title>

        <programlisting format="linespecific">
...
modparam("ims_qos", "media_type", "audio")
...
        </programlisting>
      </example>
    </section>

    <section>
      <title><varname>flow_protocol</varname> (String)</title>

      <para>Describe Flow protocol for Flow-Description AVP (507). Used only for AAR register</para>

      <para><emphasis> Default value is 'IP'</emphasis></para>

      <example>
        <title><varname>flow_protocol</varname> parameter
        usage</title>

        <programlisting format="linespecific">
...
modparam("ims_qos", "flow_protocol", "UDP")
...
        </programlisting>
      </example>
    </section>

    <section>
      <title><varname>omit_flow_ports</varname> integer</title>

      <para>If set to 1 ommit ports for Flow-Description AVP (507). Used only for AAR register</para>

      <para><emphasis> Default value is 0, Add ports to Flow-Description AVP (507)</emphasis></para>

      <example>
        <title><varname>omit_flow_ports</varname> parameter
        usage</title>

        <programlisting format="linespecific">
...
modparam("ims_qos", "omit_flow_ports", 1)
...
        </programlisting>
      </example>
    </section>

    <section>
      <title><varname>rs_default_bandwidth</varname> integer</title>

      <para>Describe default RS-Bandwidth AVP(522) for AAR</para>

      <para><emphasis> Default value is 0</emphasis></para>

      <example>
        <title><varname>rs_default_bandwidth</varname> parameter
        usage</title>

        <programlisting format="linespecific">
...
modparam("ims_qos", "rs_default_bandwidth", 600)
...
        </programlisting>
      </example>
    </section>

    <section>
      <title><varname>rr_default_bandwidth</varname> integer</title>

      <para>Describe default RR-Bandwidth AVP(521) for AAR</para>

      <para><emphasis> Default value is 0</emphasis></para>

      <example>
        <title><varname>rr_default_bandwidth</varname> parameter
        usage</title>

        <programlisting format="linespecific">
...
modparam("ims_qos", "rr_default_bandwidth", 2000)
...
        </programlisting>
      </example>
    </section>

    <section>
      <title><varname>suspend_transaction</varname> integer</title>

      <para>If enabled, suspends the tm transaction while doing the AAR.</para>

      <para><emphasis> Default value is 1 (enabled)</emphasis></para>

      <example>
        <title><varname>suspend_transaction</varname> parameter
        usage</title>

        <programlisting format="linespecific">
...
modparam("ims_qos", "suspend_transaction", 0)
...
        </programlisting>
      </example>
    </section>

    <section>
      <title><varname>recv_mode</varname> integer</title>

	  <para>If set to 0, rx_aar_register() takes the received-from address values
	  (IP, port, proto) from the IP frame. If set to 1, it takes them from
      Via header. </para>

      <para><emphasis> Default value is 0</emphasis></para>

      <example>
        <title><varname>recv_mode</varname> parameter
        usage</title>

        <programlisting format="linespecific">
...
modparam("ims_qos", "recv_mode", 1)
...
        </programlisting>
      </example>
    </section>

    <section>
      <title><varname>dialog_direction</varname> integer</title>

	  <para>If set to 1, DLG_MOBILE_ORIGINATING is set to
	  rx_add_media_component_description_avp() instead of DLG_MOBILE_REGISTER
	  (which corresponds to value 3).
      </para>

      <para><emphasis> Default value is 3</emphasis></para>

      <example>
        <title><varname>dialog_direction</varname> parameter
        usage</title>

        <programlisting format="linespecific">
...
modparam("ims_qos", "dialog_direction", 1)
...
        </programlisting>
      </example>
    </section>
  </section>

  <section>
    <title>Functions</title>

    <section>
      <title><function moreinfo="none">Rx_AAR_Register(route_block,
      domain)</function></title>

      <para>Perform an AAR on Diameter RX interface to subscribe to signalling
      status. This purpose of this is tell a Diameter server (typically a
      PCRF) to inform the requesting Diameter client on changes to the status
      of signalling bearer for the same framed IP address. For more details
      see 3GGP TS 29.214.</para>

      <para>Meaning of the parameters is as follows:</para>

      <itemizedlist>
        <listitem>
          <para>Route block to resume after async UAR Diameter reply.</para>
        </listitem>

        <listitem>
          <para><emphasis>domain</emphasis> that usrloc_pcscf uses to store
          user information.</para>
        </listitem>
      </itemizedlist>

	<para>Return codes:</para>
		<itemizedlist>
		<listitem>
			<para>
			<emphasis>-1</emphasis> - error: There was an error, so we must either ignore it (no subscription) or send 403 (depends on behaviour you want)
			</para>
			<para>
			<emphasis>0</emphasis> - Success: AAR-Request sent, reply is processed asynchronously.
			</para>
			<para>
			<emphasis>1</emphasis> - Success: No need to send AAR-Request, as a subscription still exists (continue as normal)
			</para>
		</listitem>
		</itemizedlist>


      <para>This function can be used from REQUEST_ROUTE.</para>

      <para>p.s. this is executed asynchronously. See example on how to
      retrieve return value</para>

      <example>
        <title>Rx_AAR_Register</title>

        <programlisting format="linespecific">
...
if(Rx_AAR_Register("REG_AAR_REPLY","location")==0){
    exit;
}
...
route[REG_AAR_REPLY]
{
    switch ($avp(s:aar_return_code)) {
        case 1:
            xlog("L_DBG", "Diameter: AAR success on subscription to signalling\n");
            break;
        default:
            xlog("L_ERR", "Diameter: AAR failed on subscription to signalling\n");
            t_reply("403", "Can't register to QoS for signalling");
            exit;
    }
...
</programlisting>
      </example>
    </section>

    <section>
      <title><function moreinfo="none">Rx_AAR(route_block,
      direction, subscription_id, subscription_id_type)</function></title>

      <para>Perform an AAR on Diameter RX interface to request resource
      authorisation from a Diameter server (typically a PCRF). For more
      details see 3GGP TS 29.214.</para>

      <para>Meaning of the parameters is as follows:</para>

      <itemizedlist>
        <listitem>
          <para><emphasis>Route block</emphasis> to resume after async UAR Diameter reply.</para>
        </listitem>

        <listitem>
          <para><emphasis>direction</emphasis> of this message -
          orig, term, etc.</para>
        </listitem>

	<listitem>
          <para><emphasis>subscription_id</emphasis> to hard code subscription ID for AAR.
	  Used for some broken PCRFs.  Leave blank to use default</para>
        </listitem>

	<listitem>
          <para><emphasis>subscription_id_type</emphasis> to hard code subscription ID type
	  for AAR. Only applicable if subscription_id is set. Set to -1 to use default.
	  This is as per RFC 4006:
	  END_USER_E164 0, END_USER_IMSI 1, END_USER_SIP_URI 2, END_USER_NAI 3,
	  END_USER_PRIVATE 4</para>
	</listitem>
	</itemizedlist>

	<para>This function can be used only from ONREPLY_ROUTE, only for replies to INVITE, UPDATE, PRACK.
	The reply and request must have SDP, for this function to work properly.</para>

      <para>p.s. this is executed asynchronously. See example on how to
      retrieve return value</para>

      <example>
        <title>Rx_AAR</title>

        <programlisting format="linespecific">
...
if(Rx_AAR("ORIG_SESSION_AAR_REPLY","orig","",-1)==0){
    exit;
}
...
route[ORIGN_SESSION_AAR_REPLY]
{
    if ($avp(s:aar_return_code) != 1) {
        xlog("L_ERR", "IMS: AAR failed Orig\n");
        dlg_terminate("all", "Sorry no QoS available");
    } else {
        xlog("L_DBG", "Diameter: Orig AAR success on media authorization\n");
    }
}
...
</programlisting>
      </example>
    </section>
  </section>

  <section>
    <title>Statistics</title>

    <section>
      <title>AAR Timeouts (aar_timeouts)</title>

      <para>The number of timeouts on sending an AAR. i.e. no response to
      AAR.</para>
    </section>

    <section>
      <title>Average AAR Response Time (aar_avg_response_time)</title>

      <para>The average response time in milliseconds for AAR-AAA
      transaction.</para>
    </section>
  </section>
</chapter>
