<?xml version="1.0" encoding="UTF-8"?>
<!-- this file is autogenerated, do not edit! -->
<!DOCTYPE section PUBLIC "-//OASIS//DTD DocBook XML V4.2//EN"
	"http://www.oasis-open.org/docbook/xml/4.2/docbookx.dtd">
<chapter id="config_vars.sctp">
	<title> Configuration Variables for sctp</title>


<section id="sctp.socket_rcvbuf">
    <title>sctp.socket_rcvbuf</title>
    <para>
        socket receive buffer size (read-only).
    </para>
    <para>Range: 512 - 102400.</para>
    <para>Type: integer.</para>
    <para>
        Read-only.
    </para>
</section>

<section id="sctp.socket_sndbuf">
    <title>sctp.socket_sndbuf</title>
    <para>
        socket send buffer size (read-only).
    </para>
    <para>Range: 512 - 102400.</para>
    <para>Type: integer.</para>
    <para>
        Read-only.
    </para>
</section>

<section id="sctp.autoclose">
    <title>sctp.autoclose</title>
    <para>
        seconds before closing and idle connection (must be non-zero).
    </para>
    <para>Range: 1 - 1073741824.</para>
    <para>Type: integer.</para>
    <para>
    </para>
</section>

<section id="sctp.send_ttl">
    <title>sctp.send_ttl</title>
    <para>
        milliseconds before aborting a send.
    </para>
    <para>Range: 0 - 1073741824.</para>
    <para>Type: integer.</para>
    <para>
    </para>
</section>

<section id="sctp.send_retries">
    <title>sctp.send_retries</title>
    <para>
        re-send attempts on failure.
    </para>
    <para>Range: 0 - 9.</para>
    <para>Type: integer.</para>
    <para>
    </para>
</section>

<section id="sctp.assoc_tracking">
    <title>sctp.assoc_tracking</title>
    <para>
        connection/association tracking (see also assoc_reuse).
    </para>
    <para>Range: 0 - 1.</para>
    <para>Type: integer.</para>
    <para>
    </para>
</section>

<section id="sctp.assoc_reuse">
    <title>sctp.assoc_reuse</title>
    <para>
        connection/association reuse (for now used only for replies),
        depends on assoc_tracking being set.
    </para>
    <para>Range: 0 - 1.</para>
    <para>Type: integer.</para>
    <para>
    </para>
</section>

<section id="sctp.max_assocs">
    <title>sctp.max_assocs</title>
    <para>
        maximum allowed open associations (-1 = disable, as many as
        allowed by the OS).
    </para>
    <para>Type: integer.</para>
    <para>
    </para>
</section>

<section id="sctp.srto_initial">
    <title>sctp.srto_initial</title>
    <para>
        initial value of the retr. timeout, used in RTO calculations,
        in msecs.
    </para>
    <para>Range: 0 - 1073741824.</para>
    <para>Type: integer.</para>
    <para>
    </para>
</section>

<section id="sctp.srto_max">
    <title>sctp.srto_max</title>
    <para>
        maximum value of the retransmission timeout (RTO), in msecs.
    </para>
    <para>Range: 0 - 1073741824.</para>
    <para>Type: integer.</para>
    <para>
    </para>
</section>

<section id="sctp.srto_min">
    <title>sctp.srto_min</title>
    <para>
        minimum value of the retransmission timeout (RTO), in msecs.
    </para>
    <para>Range: 0 - 1073741824.</para>
    <para>Type: integer.</para>
    <para>
    </para>
</section>

<section id="sctp.asocmaxrxt">
    <title>sctp.asocmaxrxt</title>
    <para>
        maximum retransmission attempts per association.
    </para>
    <para>Range: 0 - 1024.</para>
    <para>Type: integer.</para>
    <para>
    </para>
</section>

<section id="sctp.init_max_attempts">
    <title>sctp.init_max_attempts</title>
    <para>
        max INIT retransmission attempts.
    </para>
    <para>Range: 0 - 1024.</para>
    <para>Type: integer.</para>
    <para>
    </para>
</section>

<section id="sctp.init_max_timeo">
    <title>sctp.init_max_timeo</title>
    <para>
        max INIT retransmission timeout (RTO max for INIT), in msecs.
    </para>
    <para>Range: 0 - 1073741824.</para>
    <para>Type: integer.</para>
    <para>
    </para>
</section>

<section id="sctp.hbinterval">
    <title>sctp.hbinterval</title>
    <para>
        heartbeat interval in msecs.
    </para>
    <para>Range: 0 - 1073741824.</para>
    <para>Type: integer.</para>
    <para>
    </para>
</section>

<section id="sctp.pathmaxrxt">
    <title>sctp.pathmaxrxt</title>
    <para>
        maximum retransmission attempts per path.
    </para>
    <para>Range: 0 - 1024.</para>
    <para>Type: integer.</para>
    <para>
    </para>
</section>

<section id="sctp.sack_delay">
    <title>sctp.sack_delay</title>
    <para>
        time since the last received packet before sending a SACK, in
        msecs.
    </para>
    <para>Range: 0 - 1073741824.</para>
    <para>Type: integer.</para>
    <para>
    </para>
</section>

<section id="sctp.sack_freq">
    <title>sctp.sack_freq</title>
    <para>
        number of received packets that trigger the sending of a SACK.
    </para>
    <para>Range: 0 - 1024.</para>
    <para>Type: integer.</para>
    <para>
    </para>
</section>

<section id="sctp.max_burst">
    <title>sctp.max_burst</title>
    <para>
        maximum burst of packets that can be emitted by an association.
    </para>
    <para>Range: 0 - 1024.</para>
    <para>Type: integer.</para>
    <para>
    </para>
</section>

</chapter>
