Minimal control plane for Istio. Pilot and mesh config are included.

MCP and injector should optionally be installed in the same namespace. Alternatively remote
address of an MCP server can be set.

