// Copyright 2015-2021 The Khronos Group, Inc.
//
// SPDX-License-Identifier: CC-BY-4.0

[[formats]]
= Formats

Supported buffer and image formats may: vary across implementations.
A minimum set of format features are guaranteed, but others must: be
explicitly queried before use to ensure they are supported by the
implementation.

The features for the set of formats (elink:VkFormat) supported by the
implementation are queried individually using the
flink:vkGetPhysicalDeviceFormatProperties command.


[[formats-definition]]
== Format Definition

[open,refpage='VkFormat',desc='Available image formats',type='enums']
--
The following image formats can: be passed to, and may: be returned from
Vulkan commands.
The memory required to store each format is discussed with that format, and
also summarized in the <<texel-block-size, Representation and Texel Block
Size>> section and the <<formats-compatibility, Compatible formats>> table.

include::{generated}/api/enums/VkFormat.txt[]

  * ename:VK_FORMAT_UNDEFINED specifies that the format is not specified.
  * ename:VK_FORMAT_R4G4_UNORM_PACK8 specifies a two-component, 8-bit packed
    unsigned normalized format that has a 4-bit R component in bits 4..7,
    and a 4-bit G component in bits 0..3.
  * ename:VK_FORMAT_R4G4B4A4_UNORM_PACK16 specifies a four-component, 16-bit
    packed unsigned normalized format that has a 4-bit R component in bits
    12..15, a 4-bit G component in bits 8..11, a 4-bit B component in bits
    4..7, and a 4-bit A component in bits 0..3.
  * ename:VK_FORMAT_B4G4R4A4_UNORM_PACK16 specifies a four-component, 16-bit
    packed unsigned normalized format that has a 4-bit B component in bits
    12..15, a 4-bit G component in bits 8..11, a 4-bit R component in bits
    4..7, and a 4-bit A component in bits 0..3.
ifdef::VK_EXT_4444_formats[]
  * ename:VK_FORMAT_A4R4G4B4_UNORM_PACK16_EXT specifies a four-component,
    16-bit packed unsigned normalized format that has a 4-bit A component in
    bits 12..15, a 4-bit R component in bits 8..11, a 4-bit G component in
    bits 4..7, and a 4-bit B component in bits 0..3.
  * ename:VK_FORMAT_A4B4G4R4_UNORM_PACK16_EXT specifies a four-component,
    16-bit packed unsigned normalized format that has a 4-bit A component in
    bits 12..15, a 4-bit B component in bits 8..11, a 4-bit G component in
    bits 4..7, and a 4-bit R component in bits 0..3.
endif::VK_EXT_4444_formats[]
  * ename:VK_FORMAT_R5G6B5_UNORM_PACK16 specifies a three-component, 16-bit
    packed unsigned normalized format that has a 5-bit R component in bits
    11..15, a 6-bit G component in bits 5..10, and a 5-bit B component in
    bits 0..4.
  * ename:VK_FORMAT_B5G6R5_UNORM_PACK16 specifies a three-component, 16-bit
    packed unsigned normalized format that has a 5-bit B component in bits
    11..15, a 6-bit G component in bits 5..10, and a 5-bit R component in
    bits 0..4.
  * ename:VK_FORMAT_R5G5B5A1_UNORM_PACK16 specifies a four-component, 16-bit
    packed unsigned normalized format that has a 5-bit R component in bits
    11..15, a 5-bit G component in bits 6..10, a 5-bit B component in bits
    1..5, and a 1-bit A component in bit 0.
  * ename:VK_FORMAT_B5G5R5A1_UNORM_PACK16 specifies a four-component, 16-bit
    packed unsigned normalized format that has a 5-bit B component in bits
    11..15, a 5-bit G component in bits 6..10, a 5-bit R component in bits
    1..5, and a 1-bit A component in bit 0.
  * ename:VK_FORMAT_A1R5G5B5_UNORM_PACK16 specifies a four-component, 16-bit
    packed unsigned normalized format that has a 1-bit A component in bit
    15, a 5-bit R component in bits 10..14, a 5-bit G component in bits
    5..9, and a 5-bit B component in bits 0..4.
  * ename:VK_FORMAT_R8_UNORM specifies a one-component, 8-bit unsigned
    normalized format that has a single 8-bit R component.
  * ename:VK_FORMAT_R8_SNORM specifies a one-component, 8-bit signed
    normalized format that has a single 8-bit R component.
  * ename:VK_FORMAT_R8_USCALED specifies a one-component, 8-bit unsigned
    scaled integer format that has a single 8-bit R component.
  * ename:VK_FORMAT_R8_SSCALED specifies a one-component, 8-bit signed
    scaled integer format that has a single 8-bit R component.
  * ename:VK_FORMAT_R8_UINT specifies a one-component, 8-bit unsigned
    integer format that has a single 8-bit R component.
  * ename:VK_FORMAT_R8_SINT specifies a one-component, 8-bit signed integer
    format that has a single 8-bit R component.
  * ename:VK_FORMAT_R8_SRGB specifies a one-component, 8-bit unsigned
    normalized format that has a single 8-bit R component stored with sRGB
    nonlinear encoding.
  * ename:VK_FORMAT_R8G8_UNORM specifies a two-component, 16-bit unsigned
    normalized format that has an 8-bit R component in byte 0, and an 8-bit
    G component in byte 1.
  * ename:VK_FORMAT_R8G8_SNORM specifies a two-component, 16-bit signed
    normalized format that has an 8-bit R component in byte 0, and an 8-bit
    G component in byte 1.
  * ename:VK_FORMAT_R8G8_USCALED specifies a two-component, 16-bit unsigned
    scaled integer format that has an 8-bit R component in byte 0, and an
    8-bit G component in byte 1.
  * ename:VK_FORMAT_R8G8_SSCALED specifies a two-component, 16-bit signed
    scaled integer format that has an 8-bit R component in byte 0, and an
    8-bit G component in byte 1.
  * ename:VK_FORMAT_R8G8_UINT specifies a two-component, 16-bit unsigned
    integer format that has an 8-bit R component in byte 0, and an 8-bit G
    component in byte 1.
  * ename:VK_FORMAT_R8G8_SINT specifies a two-component, 16-bit signed
    integer format that has an 8-bit R component in byte 0, and an 8-bit G
    component in byte 1.
  * ename:VK_FORMAT_R8G8_SRGB specifies a two-component, 16-bit unsigned
    normalized format that has an 8-bit R component stored with sRGB
    nonlinear encoding in byte 0, and an 8-bit G component stored with sRGB
    nonlinear encoding in byte 1.
  * ename:VK_FORMAT_R8G8B8_UNORM specifies a three-component, 24-bit
    unsigned normalized format that has an 8-bit R component in byte 0, an
    8-bit G component in byte 1, and an 8-bit B component in byte 2.
  * ename:VK_FORMAT_R8G8B8_SNORM specifies a three-component, 24-bit signed
    normalized format that has an 8-bit R component in byte 0, an 8-bit G
    component in byte 1, and an 8-bit B component in byte 2.
  * ename:VK_FORMAT_R8G8B8_USCALED specifies a three-component, 24-bit
    unsigned scaled format that has an 8-bit R component in byte 0, an 8-bit
    G component in byte 1, and an 8-bit B component in byte 2.
  * ename:VK_FORMAT_R8G8B8_SSCALED specifies a three-component, 24-bit
    signed scaled format that has an 8-bit R component in byte 0, an 8-bit G
    component in byte 1, and an 8-bit B component in byte 2.
  * ename:VK_FORMAT_R8G8B8_UINT specifies a three-component, 24-bit unsigned
    integer format that has an 8-bit R component in byte 0, an 8-bit G
    component in byte 1, and an 8-bit B component in byte 2.
  * ename:VK_FORMAT_R8G8B8_SINT specifies a three-component, 24-bit signed
    integer format that has an 8-bit R component in byte 0, an 8-bit G
    component in byte 1, and an 8-bit B component in byte 2.
  * ename:VK_FORMAT_R8G8B8_SRGB specifies a three-component, 24-bit unsigned
    normalized format that has an 8-bit R component stored with sRGB
    nonlinear encoding in byte 0, an 8-bit G component stored with sRGB
    nonlinear encoding in byte 1, and an 8-bit B component stored with sRGB
    nonlinear encoding in byte 2.
  * ename:VK_FORMAT_B8G8R8_UNORM specifies a three-component, 24-bit
    unsigned normalized format that has an 8-bit B component in byte 0, an
    8-bit G component in byte 1, and an 8-bit R component in byte 2.
  * ename:VK_FORMAT_B8G8R8_SNORM specifies a three-component, 24-bit signed
    normalized format that has an 8-bit B component in byte 0, an 8-bit G
    component in byte 1, and an 8-bit R component in byte 2.
  * ename:VK_FORMAT_B8G8R8_USCALED specifies a three-component, 24-bit
    unsigned scaled format that has an 8-bit B component in byte 0, an 8-bit
    G component in byte 1, and an 8-bit R component in byte 2.
  * ename:VK_FORMAT_B8G8R8_SSCALED specifies a three-component, 24-bit
    signed scaled format that has an 8-bit B component in byte 0, an 8-bit G
    component in byte 1, and an 8-bit R component in byte 2.
  * ename:VK_FORMAT_B8G8R8_UINT specifies a three-component, 24-bit unsigned
    integer format that has an 8-bit B component in byte 0, an 8-bit G
    component in byte 1, and an 8-bit R component in byte 2.
  * ename:VK_FORMAT_B8G8R8_SINT specifies a three-component, 24-bit signed
    integer format that has an 8-bit B component in byte 0, an 8-bit G
    component in byte 1, and an 8-bit R component in byte 2.
  * ename:VK_FORMAT_B8G8R8_SRGB specifies a three-component, 24-bit unsigned
    normalized format that has an 8-bit B component stored with sRGB
    nonlinear encoding in byte 0, an 8-bit G component stored with sRGB
    nonlinear encoding in byte 1, and an 8-bit R component stored with sRGB
    nonlinear encoding in byte 2.
  * ename:VK_FORMAT_R8G8B8A8_UNORM specifies a four-component, 32-bit
    unsigned normalized format that has an 8-bit R component in byte 0, an
    8-bit G component in byte 1, an 8-bit B component in byte 2, and an
    8-bit A component in byte 3.
  * ename:VK_FORMAT_R8G8B8A8_SNORM specifies a four-component, 32-bit signed
    normalized format that has an 8-bit R component in byte 0, an 8-bit G
    component in byte 1, an 8-bit B component in byte 2, and an 8-bit A
    component in byte 3.
  * ename:VK_FORMAT_R8G8B8A8_USCALED specifies a four-component, 32-bit
    unsigned scaled format that has an 8-bit R component in byte 0, an 8-bit
    G component in byte 1, an 8-bit B component in byte 2, and an 8-bit A
    component in byte 3.
  * ename:VK_FORMAT_R8G8B8A8_SSCALED specifies a four-component, 32-bit
    signed scaled format that has an 8-bit R component in byte 0, an 8-bit G
    component in byte 1, an 8-bit B component in byte 2, and an 8-bit A
    component in byte 3.
  * ename:VK_FORMAT_R8G8B8A8_UINT specifies a four-component, 32-bit
    unsigned integer format that has an 8-bit R component in byte 0, an
    8-bit G component in byte 1, an 8-bit B component in byte 2, and an
    8-bit A component in byte 3.
  * ename:VK_FORMAT_R8G8B8A8_SINT specifies a four-component, 32-bit signed
    integer format that has an 8-bit R component in byte 0, an 8-bit G
    component in byte 1, an 8-bit B component in byte 2, and an 8-bit A
    component in byte 3.
  * ename:VK_FORMAT_R8G8B8A8_SRGB specifies a four-component, 32-bit
    unsigned normalized format that has an 8-bit R component stored with
    sRGB nonlinear encoding in byte 0, an 8-bit G component stored with sRGB
    nonlinear encoding in byte 1, an 8-bit B component stored with sRGB
    nonlinear encoding in byte 2, and an 8-bit A component in byte 3.
  * ename:VK_FORMAT_B8G8R8A8_UNORM specifies a four-component, 32-bit
    unsigned normalized format that has an 8-bit B component in byte 0, an
    8-bit G component in byte 1, an 8-bit R component in byte 2, and an
    8-bit A component in byte 3.
  * ename:VK_FORMAT_B8G8R8A8_SNORM specifies a four-component, 32-bit signed
    normalized format that has an 8-bit B component in byte 0, an 8-bit G
    component in byte 1, an 8-bit R component in byte 2, and an 8-bit A
    component in byte 3.
  * ename:VK_FORMAT_B8G8R8A8_USCALED specifies a four-component, 32-bit
    unsigned scaled format that has an 8-bit B component in byte 0, an 8-bit
    G component in byte 1, an 8-bit R component in byte 2, and an 8-bit A
    component in byte 3.
  * ename:VK_FORMAT_B8G8R8A8_SSCALED specifies a four-component, 32-bit
    signed scaled format that has an 8-bit B component in byte 0, an 8-bit G
    component in byte 1, an 8-bit R component in byte 2, and an 8-bit A
    component in byte 3.
  * ename:VK_FORMAT_B8G8R8A8_UINT specifies a four-component, 32-bit
    unsigned integer format that has an 8-bit B component in byte 0, an
    8-bit G component in byte 1, an 8-bit R component in byte 2, and an
    8-bit A component in byte 3.
  * ename:VK_FORMAT_B8G8R8A8_SINT specifies a four-component, 32-bit signed
    integer format that has an 8-bit B component in byte 0, an 8-bit G
    component in byte 1, an 8-bit R component in byte 2, and an 8-bit A
    component in byte 3.
  * ename:VK_FORMAT_B8G8R8A8_SRGB specifies a four-component, 32-bit
    unsigned normalized format that has an 8-bit B component stored with
    sRGB nonlinear encoding in byte 0, an 8-bit G component stored with sRGB
    nonlinear encoding in byte 1, an 8-bit R component stored with sRGB
    nonlinear encoding in byte 2, and an 8-bit A component in byte 3.
  * ename:VK_FORMAT_A8B8G8R8_UNORM_PACK32 specifies a four-component, 32-bit
    packed unsigned normalized format that has an 8-bit A component in bits
    24..31, an 8-bit B component in bits 16..23, an 8-bit G component in
    bits 8..15, and an 8-bit R component in bits 0..7.
  * ename:VK_FORMAT_A8B8G8R8_SNORM_PACK32 specifies a four-component, 32-bit
    packed signed normalized format that has an 8-bit A component in bits
    24..31, an 8-bit B component in bits 16..23, an 8-bit G component in
    bits 8..15, and an 8-bit R component in bits 0..7.
  * ename:VK_FORMAT_A8B8G8R8_USCALED_PACK32 specifies a four-component,
    32-bit packed unsigned scaled integer format that has an 8-bit A
    component in bits 24..31, an 8-bit B component in bits 16..23, an 8-bit
    G component in bits 8..15, and an 8-bit R component in bits 0..7.
  * ename:VK_FORMAT_A8B8G8R8_SSCALED_PACK32 specifies a four-component,
    32-bit packed signed scaled integer format that has an 8-bit A component
    in bits 24..31, an 8-bit B component in bits 16..23, an 8-bit G
    component in bits 8..15, and an 8-bit R component in bits 0..7.
  * ename:VK_FORMAT_A8B8G8R8_UINT_PACK32 specifies a four-component, 32-bit
    packed unsigned integer format that has an 8-bit A component in bits
    24..31, an 8-bit B component in bits 16..23, an 8-bit G component in
    bits 8..15, and an 8-bit R component in bits 0..7.
  * ename:VK_FORMAT_A8B8G8R8_SINT_PACK32 specifies a four-component, 32-bit
    packed signed integer format that has an 8-bit A component in bits
    24..31, an 8-bit B component in bits 16..23, an 8-bit G component in
    bits 8..15, and an 8-bit R component in bits 0..7.
  * ename:VK_FORMAT_A8B8G8R8_SRGB_PACK32 specifies a four-component, 32-bit
    packed unsigned normalized format that has an 8-bit A component in bits
    24..31, an 8-bit B component stored with sRGB nonlinear encoding in bits
    16..23, an 8-bit G component stored with sRGB nonlinear encoding in bits
    8..15, and an 8-bit R component stored with sRGB nonlinear encoding in
    bits 0..7.
  * ename:VK_FORMAT_A2R10G10B10_UNORM_PACK32 specifies a four-component,
    32-bit packed unsigned normalized format that has a 2-bit A component in
    bits 30..31, a 10-bit R component in bits 20..29, a 10-bit G component
    in bits 10..19, and a 10-bit B component in bits 0..9.
  * ename:VK_FORMAT_A2R10G10B10_SNORM_PACK32 specifies a four-component,
    32-bit packed signed normalized format that has a 2-bit A component in
    bits 30..31, a 10-bit R component in bits 20..29, a 10-bit G component
    in bits 10..19, and a 10-bit B component in bits 0..9.
  * ename:VK_FORMAT_A2R10G10B10_USCALED_PACK32 specifies a four-component,
    32-bit packed unsigned scaled integer format that has a 2-bit A
    component in bits 30..31, a 10-bit R component in bits 20..29, a 10-bit
    G component in bits 10..19, and a 10-bit B component in bits 0..9.
  * ename:VK_FORMAT_A2R10G10B10_SSCALED_PACK32 specifies a four-component,
    32-bit packed signed scaled integer format that has a 2-bit A component
    in bits 30..31, a 10-bit R component in bits 20..29, a 10-bit G
    component in bits 10..19, and a 10-bit B component in bits 0..9.
  * ename:VK_FORMAT_A2R10G10B10_UINT_PACK32 specifies a four-component,
    32-bit packed unsigned integer format that has a 2-bit A component in
    bits 30..31, a 10-bit R component in bits 20..29, a 10-bit G component
    in bits 10..19, and a 10-bit B component in bits 0..9.
  * ename:VK_FORMAT_A2R10G10B10_SINT_PACK32 specifies a four-component,
    32-bit packed signed integer format that has a 2-bit A component in bits
    30..31, a 10-bit R component in bits 20..29, a 10-bit G component in
    bits 10..19, and a 10-bit B component in bits 0..9.
  * ename:VK_FORMAT_A2B10G10R10_UNORM_PACK32 specifies a four-component,
    32-bit packed unsigned normalized format that has a 2-bit A component in
    bits 30..31, a 10-bit B component in bits 20..29, a 10-bit G component
    in bits 10..19, and a 10-bit R component in bits 0..9.
  * ename:VK_FORMAT_A2B10G10R10_SNORM_PACK32 specifies a four-component,
    32-bit packed signed normalized format that has a 2-bit A component in
    bits 30..31, a 10-bit B component in bits 20..29, a 10-bit G component
    in bits 10..19, and a 10-bit R component in bits 0..9.
  * ename:VK_FORMAT_A2B10G10R10_USCALED_PACK32 specifies a four-component,
    32-bit packed unsigned scaled integer format that has a 2-bit A
    component in bits 30..31, a 10-bit B component in bits 20..29, a 10-bit
    G component in bits 10..19, and a 10-bit R component in bits 0..9.
  * ename:VK_FORMAT_A2B10G10R10_SSCALED_PACK32 specifies a four-component,
    32-bit packed signed scaled integer format that has a 2-bit A component
    in bits 30..31, a 10-bit B component in bits 20..29, a 10-bit G
    component in bits 10..19, and a 10-bit R component in bits 0..9.
  * ename:VK_FORMAT_A2B10G10R10_UINT_PACK32 specifies a four-component,
    32-bit packed unsigned integer format that has a 2-bit A component in
    bits 30..31, a 10-bit B component in bits 20..29, a 10-bit G component
    in bits 10..19, and a 10-bit R component in bits 0..9.
  * ename:VK_FORMAT_A2B10G10R10_SINT_PACK32 specifies a four-component,
    32-bit packed signed integer format that has a 2-bit A component in bits
    30..31, a 10-bit B component in bits 20..29, a 10-bit G component in
    bits 10..19, and a 10-bit R component in bits 0..9.
  * ename:VK_FORMAT_R16_UNORM specifies a one-component, 16-bit unsigned
    normalized format that has a single 16-bit R component.
  * ename:VK_FORMAT_R16_SNORM specifies a one-component, 16-bit signed
    normalized format that has a single 16-bit R component.
  * ename:VK_FORMAT_R16_USCALED specifies a one-component, 16-bit unsigned
    scaled integer format that has a single 16-bit R component.
  * ename:VK_FORMAT_R16_SSCALED specifies a one-component, 16-bit signed
    scaled integer format that has a single 16-bit R component.
  * ename:VK_FORMAT_R16_UINT specifies a one-component, 16-bit unsigned
    integer format that has a single 16-bit R component.
  * ename:VK_FORMAT_R16_SINT specifies a one-component, 16-bit signed
    integer format that has a single 16-bit R component.
  * ename:VK_FORMAT_R16_SFLOAT specifies a one-component, 16-bit signed
    floating-point format that has a single 16-bit R component.
  * ename:VK_FORMAT_R16G16_UNORM specifies a two-component, 32-bit unsigned
    normalized format that has a 16-bit R component in bytes 0..1, and a
    16-bit G component in bytes 2..3.
  * ename:VK_FORMAT_R16G16_SNORM specifies a two-component, 32-bit signed
    normalized format that has a 16-bit R component in bytes 0..1, and a
    16-bit G component in bytes 2..3.
  * ename:VK_FORMAT_R16G16_USCALED specifies a two-component, 32-bit
    unsigned scaled integer format that has a 16-bit R component in bytes
    0..1, and a 16-bit G component in bytes 2..3.
  * ename:VK_FORMAT_R16G16_SSCALED specifies a two-component, 32-bit signed
    scaled integer format that has a 16-bit R component in bytes 0..1, and a
    16-bit G component in bytes 2..3.
  * ename:VK_FORMAT_R16G16_UINT specifies a two-component, 32-bit unsigned
    integer format that has a 16-bit R component in bytes 0..1, and a 16-bit
    G component in bytes 2..3.
  * ename:VK_FORMAT_R16G16_SINT specifies a two-component, 32-bit signed
    integer format that has a 16-bit R component in bytes 0..1, and a 16-bit
    G component in bytes 2..3.
  * ename:VK_FORMAT_R16G16_SFLOAT specifies a two-component, 32-bit signed
    floating-point format that has a 16-bit R component in bytes 0..1, and a
    16-bit G component in bytes 2..3.
  * ename:VK_FORMAT_R16G16B16_UNORM specifies a three-component, 48-bit
    unsigned normalized format that has a 16-bit R component in bytes 0..1,
    a 16-bit G component in bytes 2..3, and a 16-bit B component in bytes
    4..5.
  * ename:VK_FORMAT_R16G16B16_SNORM specifies a three-component, 48-bit
    signed normalized format that has a 16-bit R component in bytes 0..1, a
    16-bit G component in bytes 2..3, and a 16-bit B component in bytes
    4..5.
  * ename:VK_FORMAT_R16G16B16_USCALED specifies a three-component, 48-bit
    unsigned scaled integer format that has a 16-bit R component in bytes
    0..1, a 16-bit G component in bytes 2..3, and a 16-bit B component in
    bytes 4..5.
  * ename:VK_FORMAT_R16G16B16_SSCALED specifies a three-component, 48-bit
    signed scaled integer format that has a 16-bit R component in bytes
    0..1, a 16-bit G component in bytes 2..3, and a 16-bit B component in
    bytes 4..5.
  * ename:VK_FORMAT_R16G16B16_UINT specifies a three-component, 48-bit
    unsigned integer format that has a 16-bit R component in bytes 0..1, a
    16-bit G component in bytes 2..3, and a 16-bit B component in bytes
    4..5.
  * ename:VK_FORMAT_R16G16B16_SINT specifies a three-component, 48-bit
    signed integer format that has a 16-bit R component in bytes 0..1, a
    16-bit G component in bytes 2..3, and a 16-bit B component in bytes
    4..5.
  * ename:VK_FORMAT_R16G16B16_SFLOAT specifies a three-component, 48-bit
    signed floating-point format that has a 16-bit R component in bytes
    0..1, a 16-bit G component in bytes 2..3, and a 16-bit B component in
    bytes 4..5.
  * ename:VK_FORMAT_R16G16B16A16_UNORM specifies a four-component, 64-bit
    unsigned normalized format that has a 16-bit R component in bytes 0..1,
    a 16-bit G component in bytes 2..3, a 16-bit B component in bytes 4..5,
    and a 16-bit A component in bytes 6..7.
  * ename:VK_FORMAT_R16G16B16A16_SNORM specifies a four-component, 64-bit
    signed normalized format that has a 16-bit R component in bytes 0..1, a
    16-bit G component in bytes 2..3, a 16-bit B component in bytes 4..5,
    and a 16-bit A component in bytes 6..7.
  * ename:VK_FORMAT_R16G16B16A16_USCALED specifies a four-component, 64-bit
    unsigned scaled integer format that has a 16-bit R component in bytes
    0..1, a 16-bit G component in bytes 2..3, a 16-bit B component in bytes
    4..5, and a 16-bit A component in bytes 6..7.
  * ename:VK_FORMAT_R16G16B16A16_SSCALED specifies a four-component, 64-bit
    signed scaled integer format that has a 16-bit R component in bytes
    0..1, a 16-bit G component in bytes 2..3, a 16-bit B component in bytes
    4..5, and a 16-bit A component in bytes 6..7.
  * ename:VK_FORMAT_R16G16B16A16_UINT specifies a four-component, 64-bit
    unsigned integer format that has a 16-bit R component in bytes 0..1, a
    16-bit G component in bytes 2..3, a 16-bit B component in bytes 4..5,
    and a 16-bit A component in bytes 6..7.
  * ename:VK_FORMAT_R16G16B16A16_SINT specifies a four-component, 64-bit
    signed integer format that has a 16-bit R component in bytes 0..1, a
    16-bit G component in bytes 2..3, a 16-bit B component in bytes 4..5,
    and a 16-bit A component in bytes 6..7.
  * ename:VK_FORMAT_R16G16B16A16_SFLOAT specifies a four-component, 64-bit
    signed floating-point format that has a 16-bit R component in bytes
    0..1, a 16-bit G component in bytes 2..3, a 16-bit B component in bytes
    4..5, and a 16-bit A component in bytes 6..7.
  * ename:VK_FORMAT_R32_UINT specifies a one-component, 32-bit unsigned
    integer format that has a single 32-bit R component.
  * ename:VK_FORMAT_R32_SINT specifies a one-component, 32-bit signed
    integer format that has a single 32-bit R component.
  * ename:VK_FORMAT_R32_SFLOAT specifies a one-component, 32-bit signed
    floating-point format that has a single 32-bit R component.
  * ename:VK_FORMAT_R32G32_UINT specifies a two-component, 64-bit unsigned
    integer format that has a 32-bit R component in bytes 0..3, and a 32-bit
    G component in bytes 4..7.
  * ename:VK_FORMAT_R32G32_SINT specifies a two-component, 64-bit signed
    integer format that has a 32-bit R component in bytes 0..3, and a 32-bit
    G component in bytes 4..7.
  * ename:VK_FORMAT_R32G32_SFLOAT specifies a two-component, 64-bit signed
    floating-point format that has a 32-bit R component in bytes 0..3, and a
    32-bit G component in bytes 4..7.
  * ename:VK_FORMAT_R32G32B32_UINT specifies a three-component, 96-bit
    unsigned integer format that has a 32-bit R component in bytes 0..3, a
    32-bit G component in bytes 4..7, and a 32-bit B component in bytes
    8..11.
  * ename:VK_FORMAT_R32G32B32_SINT specifies a three-component, 96-bit
    signed integer format that has a 32-bit R component in bytes 0..3, a
    32-bit G component in bytes 4..7, and a 32-bit B component in bytes
    8..11.
  * ename:VK_FORMAT_R32G32B32_SFLOAT specifies a three-component, 96-bit
    signed floating-point format that has a 32-bit R component in bytes
    0..3, a 32-bit G component in bytes 4..7, and a 32-bit B component in
    bytes 8..11.
  * ename:VK_FORMAT_R32G32B32A32_UINT specifies a four-component, 128-bit
    unsigned integer format that has a 32-bit R component in bytes 0..3, a
    32-bit G component in bytes 4..7, a 32-bit B component in bytes 8..11,
    and a 32-bit A component in bytes 12..15.
  * ename:VK_FORMAT_R32G32B32A32_SINT specifies a four-component, 128-bit
    signed integer format that has a 32-bit R component in bytes 0..3, a
    32-bit G component in bytes 4..7, a 32-bit B component in bytes 8..11,
    and a 32-bit A component in bytes 12..15.
  * ename:VK_FORMAT_R32G32B32A32_SFLOAT specifies a four-component, 128-bit
    signed floating-point format that has a 32-bit R component in bytes
    0..3, a 32-bit G component in bytes 4..7, a 32-bit B component in bytes
    8..11, and a 32-bit A component in bytes 12..15.
  * ename:VK_FORMAT_R64_UINT specifies a one-component, 64-bit unsigned
    integer format that has a single 64-bit R component.
  * ename:VK_FORMAT_R64_SINT specifies a one-component, 64-bit signed
    integer format that has a single 64-bit R component.
  * ename:VK_FORMAT_R64_SFLOAT specifies a one-component, 64-bit signed
    floating-point format that has a single 64-bit R component.
  * ename:VK_FORMAT_R64G64_UINT specifies a two-component, 128-bit unsigned
    integer format that has a 64-bit R component in bytes 0..7, and a 64-bit
    G component in bytes 8..15.
  * ename:VK_FORMAT_R64G64_SINT specifies a two-component, 128-bit signed
    integer format that has a 64-bit R component in bytes 0..7, and a 64-bit
    G component in bytes 8..15.
  * ename:VK_FORMAT_R64G64_SFLOAT specifies a two-component, 128-bit signed
    floating-point format that has a 64-bit R component in bytes 0..7, and a
    64-bit G component in bytes 8..15.
  * ename:VK_FORMAT_R64G64B64_UINT specifies a three-component, 192-bit
    unsigned integer format that has a 64-bit R component in bytes 0..7, a
    64-bit G component in bytes 8..15, and a 64-bit B component in bytes
    16..23.
  * ename:VK_FORMAT_R64G64B64_SINT specifies a three-component, 192-bit
    signed integer format that has a 64-bit R component in bytes 0..7, a
    64-bit G component in bytes 8..15, and a 64-bit B component in bytes
    16..23.
  * ename:VK_FORMAT_R64G64B64_SFLOAT specifies a three-component, 192-bit
    signed floating-point format that has a 64-bit R component in bytes
    0..7, a 64-bit G component in bytes 8..15, and a 64-bit B component in
    bytes 16..23.
  * ename:VK_FORMAT_R64G64B64A64_UINT specifies a four-component, 256-bit
    unsigned integer format that has a 64-bit R component in bytes 0..7, a
    64-bit G component in bytes 8..15, a 64-bit B component in bytes 16..23,
    and a 64-bit A component in bytes 24..31.
  * ename:VK_FORMAT_R64G64B64A64_SINT specifies a four-component, 256-bit
    signed integer format that has a 64-bit R component in bytes 0..7, a
    64-bit G component in bytes 8..15, a 64-bit B component in bytes 16..23,
    and a 64-bit A component in bytes 24..31.
  * ename:VK_FORMAT_R64G64B64A64_SFLOAT specifies a four-component, 256-bit
    signed floating-point format that has a 64-bit R component in bytes
    0..7, a 64-bit G component in bytes 8..15, a 64-bit B component in bytes
    16..23, and a 64-bit A component in bytes 24..31.
  * ename:VK_FORMAT_B10G11R11_UFLOAT_PACK32 specifies a three-component,
    32-bit packed unsigned floating-point format that has a 10-bit B
    component in bits 22..31, an 11-bit G component in bits 11..21, an
    11-bit R component in bits 0..10.
    See <<fundamentals-fp10>> and <<fundamentals-fp11>>.
  * ename:VK_FORMAT_E5B9G9R9_UFLOAT_PACK32 specifies a three-component,
    32-bit packed unsigned floating-point format that has a 5-bit shared
    exponent in bits 27..31, a 9-bit B component mantissa in bits 18..26, a
    9-bit G component mantissa in bits 9..17, and a 9-bit R component
    mantissa in bits 0..8.
  * ename:VK_FORMAT_D16_UNORM specifies a one-component, 16-bit unsigned
    normalized format that has a single 16-bit depth component.
  * ename:VK_FORMAT_X8_D24_UNORM_PACK32 specifies a two-component, 32-bit
    format that has 24 unsigned normalized bits in the depth component and,
    optionally:, 8 bits that are unused.
  * ename:VK_FORMAT_D32_SFLOAT specifies a one-component, 32-bit signed
    floating-point format that has 32 bits in the depth component.
  * ename:VK_FORMAT_S8_UINT specifies a one-component, 8-bit unsigned
    integer format that has 8 bits in the stencil component.
  * ename:VK_FORMAT_D16_UNORM_S8_UINT specifies a two-component, 24-bit
    format that has 16 unsigned normalized bits in the depth component and 8
    unsigned integer bits in the stencil component.
  * ename:VK_FORMAT_D24_UNORM_S8_UINT specifies a two-component, 32-bit
    packed format that has 8 unsigned integer bits in the stencil component,
    and 24 unsigned normalized bits in the depth component.
  * ename:VK_FORMAT_D32_SFLOAT_S8_UINT specifies a two-component format that
    has 32 signed float bits in the depth component and 8 unsigned integer
    bits in the stencil component.
    There are optionally: 24 bits that are unused.
  * ename:VK_FORMAT_BC1_RGB_UNORM_BLOCK specifies a three-component,
    block-compressed format where each 64-bit compressed texel block encodes
    a 4{times}4 rectangle of unsigned normalized RGB texel data.
    This format has no alpha and is considered opaque.
  * ename:VK_FORMAT_BC1_RGB_SRGB_BLOCK specifies a three-component,
    block-compressed format where each 64-bit compressed texel block encodes
    a 4{times}4 rectangle of unsigned normalized RGB texel data with sRGB
    nonlinear encoding.
    This format has no alpha and is considered opaque.
  * ename:VK_FORMAT_BC1_RGBA_UNORM_BLOCK specifies a four-component,
    block-compressed format where each 64-bit compressed texel block encodes
    a 4{times}4 rectangle of unsigned normalized RGB texel data, and
    provides 1 bit of alpha.
  * ename:VK_FORMAT_BC1_RGBA_SRGB_BLOCK specifies a four-component,
    block-compressed format where each 64-bit compressed texel block encodes
    a 4{times}4 rectangle of unsigned normalized RGB texel data with sRGB
    nonlinear encoding, and provides 1 bit of alpha.
  * ename:VK_FORMAT_BC2_UNORM_BLOCK specifies a four-component,
    block-compressed format where each 128-bit compressed texel block
    encodes a 4{times}4 rectangle of unsigned normalized RGBA texel data
    with the first 64 bits encoding alpha values followed by 64 bits
    encoding RGB values.
  * ename:VK_FORMAT_BC2_SRGB_BLOCK specifies a four-component,
    block-compressed format where each 128-bit compressed texel block
    encodes a 4{times}4 rectangle of unsigned normalized RGBA texel data
    with the first 64 bits encoding alpha values followed by 64 bits
    encoding RGB values with sRGB nonlinear encoding.
  * ename:VK_FORMAT_BC3_UNORM_BLOCK specifies a four-component,
    block-compressed format where each 128-bit compressed texel block
    encodes a 4{times}4 rectangle of unsigned normalized RGBA texel data
    with the first 64 bits encoding alpha values followed by 64 bits
    encoding RGB values.
  * ename:VK_FORMAT_BC3_SRGB_BLOCK specifies a four-component,
    block-compressed format where each 128-bit compressed texel block
    encodes a 4{times}4 rectangle of unsigned normalized RGBA texel data
    with the first 64 bits encoding alpha values followed by 64 bits
    encoding RGB values with sRGB nonlinear encoding.
  * ename:VK_FORMAT_BC4_UNORM_BLOCK specifies a one-component,
    block-compressed format where each 64-bit compressed texel block encodes
    a 4{times}4 rectangle of unsigned normalized red texel data.
  * ename:VK_FORMAT_BC4_SNORM_BLOCK specifies a one-component,
    block-compressed format where each 64-bit compressed texel block encodes
    a 4{times}4 rectangle of signed normalized red texel data.
  * ename:VK_FORMAT_BC5_UNORM_BLOCK specifies a two-component,
    block-compressed format where each 128-bit compressed texel block
    encodes a 4{times}4 rectangle of unsigned normalized RG texel data with
    the first 64 bits encoding red values followed by 64 bits encoding green
    values.
  * ename:VK_FORMAT_BC5_SNORM_BLOCK specifies a two-component,
    block-compressed format where each 128-bit compressed texel block
    encodes a 4{times}4 rectangle of signed normalized RG texel data with
    the first 64 bits encoding red values followed by 64 bits encoding green
    values.
  * ename:VK_FORMAT_BC6H_UFLOAT_BLOCK specifies a three-component,
    block-compressed format where each 128-bit compressed texel block
    encodes a 4{times}4 rectangle of unsigned floating-point RGB texel data.
  * ename:VK_FORMAT_BC6H_SFLOAT_BLOCK specifies a three-component,
    block-compressed format where each 128-bit compressed texel block
    encodes a 4{times}4 rectangle of signed floating-point RGB texel data.
  * ename:VK_FORMAT_BC7_UNORM_BLOCK specifies a four-component,
    block-compressed format where each 128-bit compressed texel block
    encodes a 4{times}4 rectangle of unsigned normalized RGBA texel data.
  * ename:VK_FORMAT_BC7_SRGB_BLOCK specifies a four-component,
    block-compressed format where each 128-bit compressed texel block
    encodes a 4{times}4 rectangle of unsigned normalized RGBA texel data
    with sRGB nonlinear encoding applied to the RGB components.
  * ename:VK_FORMAT_ETC2_R8G8B8_UNORM_BLOCK specifies a three-component,
    ETC2 compressed format where each 64-bit compressed texel block encodes
    a 4{times}4 rectangle of unsigned normalized RGB texel data.
    This format has no alpha and is considered opaque.
  * ename:VK_FORMAT_ETC2_R8G8B8_SRGB_BLOCK specifies a three-component, ETC2
    compressed format where each 64-bit compressed texel block encodes a
    4{times}4 rectangle of unsigned normalized RGB texel data with sRGB
    nonlinear encoding.
    This format has no alpha and is considered opaque.
  * ename:VK_FORMAT_ETC2_R8G8B8A1_UNORM_BLOCK specifies a four-component,
    ETC2 compressed format where each 64-bit compressed texel block encodes
    a 4{times}4 rectangle of unsigned normalized RGB texel data, and
    provides 1 bit of alpha.
  * ename:VK_FORMAT_ETC2_R8G8B8A1_SRGB_BLOCK specifies a four-component,
    ETC2 compressed format where each 64-bit compressed texel block encodes
    a 4{times}4 rectangle of unsigned normalized RGB texel data with sRGB
    nonlinear encoding, and provides 1 bit of alpha.
  * ename:VK_FORMAT_ETC2_R8G8B8A8_UNORM_BLOCK specifies a four-component,
    ETC2 compressed format where each 128-bit compressed texel block encodes
    a 4{times}4 rectangle of unsigned normalized RGBA texel data with the
    first 64 bits encoding alpha values followed by 64 bits encoding RGB
    values.
  * ename:VK_FORMAT_ETC2_R8G8B8A8_SRGB_BLOCK specifies a four-component,
    ETC2 compressed format where each 128-bit compressed texel block encodes
    a 4{times}4 rectangle of unsigned normalized RGBA texel data with the
    first 64 bits encoding alpha values followed by 64 bits encoding RGB
    values with sRGB nonlinear encoding applied.
  * ename:VK_FORMAT_EAC_R11_UNORM_BLOCK specifies a one-component, ETC2
    compressed format where each 64-bit compressed texel block encodes a
    4{times}4 rectangle of unsigned normalized red texel data.
  * ename:VK_FORMAT_EAC_R11_SNORM_BLOCK specifies a one-component, ETC2
    compressed format where each 64-bit compressed texel block encodes a
    4{times}4 rectangle of signed normalized red texel data.
  * ename:VK_FORMAT_EAC_R11G11_UNORM_BLOCK specifies a two-component, ETC2
    compressed format where each 128-bit compressed texel block encodes a
    4{times}4 rectangle of unsigned normalized RG texel data with the first
    64 bits encoding red values followed by 64 bits encoding green values.
  * ename:VK_FORMAT_EAC_R11G11_SNORM_BLOCK specifies a two-component, ETC2
    compressed format where each 128-bit compressed texel block encodes a
    4{times}4 rectangle of signed normalized RG texel data with the first 64
    bits encoding red values followed by 64 bits encoding green values.
  * ename:VK_FORMAT_ASTC_4x4_UNORM_BLOCK specifies a four-component, ASTC
    compressed format where each 128-bit compressed texel block encodes a
    4{times}4 rectangle of unsigned normalized RGBA texel data.
  * ename:VK_FORMAT_ASTC_4x4_SRGB_BLOCK specifies a four-component, ASTC
    compressed format where each 128-bit compressed texel block encodes a
    4{times}4 rectangle of unsigned normalized RGBA texel data with sRGB
    nonlinear encoding applied to the RGB components.
ifdef::VK_EXT_texture_compression_astc_hdr[]
  * ename:VK_FORMAT_ASTC_4x4_SFLOAT_BLOCK_EXT specifies a four-component,
    ASTC compressed format where each 128-bit compressed texel block encodes
    a 4{times}4 rectangle of signed floating-point RGBA texel data.
endif::VK_EXT_texture_compression_astc_hdr[]
  * ename:VK_FORMAT_ASTC_5x4_UNORM_BLOCK specifies a four-component, ASTC
    compressed format where each 128-bit compressed texel block encodes a
    5{times}4 rectangle of unsigned normalized RGBA texel data.
  * ename:VK_FORMAT_ASTC_5x4_SRGB_BLOCK specifies a four-component, ASTC
    compressed format where each 128-bit compressed texel block encodes a
    5{times}4 rectangle of unsigned normalized RGBA texel data with sRGB
    nonlinear encoding applied to the RGB components.
ifdef::VK_EXT_texture_compression_astc_hdr[]
  * ename:VK_FORMAT_ASTC_5x4_SFLOAT_BLOCK_EXT specifies a four-component,
    ASTC compressed format where each 128-bit compressed texel block encodes
    a 5{times}4 rectangle of signed floating-point RGBA texel data.
endif::VK_EXT_texture_compression_astc_hdr[]
  * ename:VK_FORMAT_ASTC_5x5_UNORM_BLOCK specifies a four-component, ASTC
    compressed format where each 128-bit compressed texel block encodes a
    5{times}5 rectangle of unsigned normalized RGBA texel data.
  * ename:VK_FORMAT_ASTC_5x5_SRGB_BLOCK specifies a four-component, ASTC
    compressed format where each 128-bit compressed texel block encodes a
    5{times}5 rectangle of unsigned normalized RGBA texel data with sRGB
    nonlinear encoding applied to the RGB components.
ifdef::VK_EXT_texture_compression_astc_hdr[]
  * ename:VK_FORMAT_ASTC_5x5_SFLOAT_BLOCK_EXT specifies a four-component,
    ASTC compressed format where each 128-bit compressed texel block encodes
    a 5{times}5 rectangle of signed floating-point RGBA texel data.
endif::VK_EXT_texture_compression_astc_hdr[]
  * ename:VK_FORMAT_ASTC_6x5_UNORM_BLOCK specifies a four-component, ASTC
    compressed format where each 128-bit compressed texel block encodes a
    6{times}5 rectangle of unsigned normalized RGBA texel data.
  * ename:VK_FORMAT_ASTC_6x5_SRGB_BLOCK specifies a four-component, ASTC
    compressed format where each 128-bit compressed texel block encodes a
    6{times}5 rectangle of unsigned normalized RGBA texel data with sRGB
    nonlinear encoding applied to the RGB components.
ifdef::VK_EXT_texture_compression_astc_hdr[]
  * ename:VK_FORMAT_ASTC_6x5_SFLOAT_BLOCK_EXT specifies a four-component,
    ASTC compressed format where each 128-bit compressed texel block encodes
    a 6{times}5 rectangle of signed floating-point RGBA texel data.
endif::VK_EXT_texture_compression_astc_hdr[]
  * ename:VK_FORMAT_ASTC_6x6_UNORM_BLOCK specifies a four-component, ASTC
    compressed format where each 128-bit compressed texel block encodes a
    6{times}6 rectangle of unsigned normalized RGBA texel data.
  * ename:VK_FORMAT_ASTC_6x6_SRGB_BLOCK specifies a four-component, ASTC
    compressed format where each 128-bit compressed texel block encodes a
    6{times}6 rectangle of unsigned normalized RGBA texel data with sRGB
    nonlinear encoding applied to the RGB components.
ifdef::VK_EXT_texture_compression_astc_hdr[]
  * ename:VK_FORMAT_ASTC_6x6_SFLOAT_BLOCK_EXT specifies a four-component,
    ASTC compressed format where each 128-bit compressed texel block encodes
    a 6{times}6 rectangle of signed floating-point RGBA texel data.
endif::VK_EXT_texture_compression_astc_hdr[]
  * ename:VK_FORMAT_ASTC_8x5_UNORM_BLOCK specifies a four-component, ASTC
    compressed format where each 128-bit compressed texel block encodes an
    8{times}5 rectangle of unsigned normalized RGBA texel data.
  * ename:VK_FORMAT_ASTC_8x5_SRGB_BLOCK specifies a four-component, ASTC
    compressed format where each 128-bit compressed texel block encodes an
    8{times}5 rectangle of unsigned normalized RGBA texel data with sRGB
    nonlinear encoding applied to the RGB components.
ifdef::VK_EXT_texture_compression_astc_hdr[]
  * ename:VK_FORMAT_ASTC_8x5_SFLOAT_BLOCK_EXT specifies a four-component,
    ASTC compressed format where each 128-bit compressed texel block encodes
    a 8{times}5 rectangle of signed floating-point RGBA texel data.
endif::VK_EXT_texture_compression_astc_hdr[]
  * ename:VK_FORMAT_ASTC_8x6_UNORM_BLOCK specifies a four-component, ASTC
    compressed format where each 128-bit compressed texel block encodes an
    8{times}6 rectangle of unsigned normalized RGBA texel data.
  * ename:VK_FORMAT_ASTC_8x6_SRGB_BLOCK specifies a four-component, ASTC
    compressed format where each 128-bit compressed texel block encodes an
    8{times}6 rectangle of unsigned normalized RGBA texel data with sRGB
    nonlinear encoding applied to the RGB components.
ifdef::VK_EXT_texture_compression_astc_hdr[]
  * ename:VK_FORMAT_ASTC_8x6_SFLOAT_BLOCK_EXT specifies a four-component,
    ASTC compressed format where each 128-bit compressed texel block encodes
    a 8{times}6 rectangle of signed floating-point RGBA texel data.
endif::VK_EXT_texture_compression_astc_hdr[]
  * ename:VK_FORMAT_ASTC_8x8_UNORM_BLOCK specifies a four-component, ASTC
    compressed format where each 128-bit compressed texel block encodes an
    8{times}8 rectangle of unsigned normalized RGBA texel data.
  * ename:VK_FORMAT_ASTC_8x8_SRGB_BLOCK specifies a four-component, ASTC
    compressed format where each 128-bit compressed texel block encodes an
    8{times}8 rectangle of unsigned normalized RGBA texel data with sRGB
    nonlinear encoding applied to the RGB components.
ifdef::VK_EXT_texture_compression_astc_hdr[]
  * ename:VK_FORMAT_ASTC_8x8_SFLOAT_BLOCK_EXT specifies a four-component,
    ASTC compressed format where each 128-bit compressed texel block encodes
    a 8{times}8 rectangle of signed floating-point RGBA texel data.
endif::VK_EXT_texture_compression_astc_hdr[]
  * ename:VK_FORMAT_ASTC_10x5_UNORM_BLOCK specifies a four-component, ASTC
    compressed format where each 128-bit compressed texel block encodes a
    10{times}5 rectangle of unsigned normalized RGBA texel data.
  * ename:VK_FORMAT_ASTC_10x5_SRGB_BLOCK specifies a four-component, ASTC
    compressed format where each 128-bit compressed texel block encodes a
    10{times}5 rectangle of unsigned normalized RGBA texel data with sRGB
    nonlinear encoding applied to the RGB components.
ifdef::VK_EXT_texture_compression_astc_hdr[]
  * ename:VK_FORMAT_ASTC_10x5_SFLOAT_BLOCK_EXT specifies a four-component,
    ASTC compressed format where each 128-bit compressed texel block encodes
    a 10{times}5 rectangle of signed floating-point RGBA texel data.
endif::VK_EXT_texture_compression_astc_hdr[]
  * ename:VK_FORMAT_ASTC_10x6_UNORM_BLOCK specifies a four-component, ASTC
    compressed format where each 128-bit compressed texel block encodes a
    10{times}6 rectangle of unsigned normalized RGBA texel data.
  * ename:VK_FORMAT_ASTC_10x6_SRGB_BLOCK specifies a four-component, ASTC
    compressed format where each 128-bit compressed texel block encodes a
    10{times}6 rectangle of unsigned normalized RGBA texel data with sRGB
    nonlinear encoding applied to the RGB components.
ifdef::VK_EXT_texture_compression_astc_hdr[]
  * ename:VK_FORMAT_ASTC_10x6_SFLOAT_BLOCK_EXT specifies a four-component,
    ASTC compressed format where each 128-bit compressed texel block encodes
    a 10{times}6 rectangle of signed floating-point RGBA texel data.
endif::VK_EXT_texture_compression_astc_hdr[]
  * ename:VK_FORMAT_ASTC_10x8_UNORM_BLOCK specifies a four-component, ASTC
    compressed format where each 128-bit compressed texel block encodes a
    10{times}8 rectangle of unsigned normalized RGBA texel data.
  * ename:VK_FORMAT_ASTC_10x8_SRGB_BLOCK specifies a four-component, ASTC
    compressed format where each 128-bit compressed texel block encodes a
    10{times}8 rectangle of unsigned normalized RGBA texel data with sRGB
    nonlinear encoding applied to the RGB components.
ifdef::VK_EXT_texture_compression_astc_hdr[]
  * ename:VK_FORMAT_ASTC_10x8_SFLOAT_BLOCK_EXT specifies a four-component,
    ASTC compressed format where each 128-bit compressed texel block encodes
    a 10{times}8 rectangle of signed floating-point RGBA texel data.
endif::VK_EXT_texture_compression_astc_hdr[]
  * ename:VK_FORMAT_ASTC_10x10_UNORM_BLOCK specifies a four-component, ASTC
    compressed format where each 128-bit compressed texel block encodes a
    10{times}10 rectangle of unsigned normalized RGBA texel data.
  * ename:VK_FORMAT_ASTC_10x10_SRGB_BLOCK specifies a four-component, ASTC
    compressed format where each 128-bit compressed texel block encodes a
    10{times}10 rectangle of unsigned normalized RGBA texel data with sRGB
    nonlinear encoding applied to the RGB components.
ifdef::VK_EXT_texture_compression_astc_hdr[]
  * ename:VK_FORMAT_ASTC_10x10_SFLOAT_BLOCK_EXT specifies a four-component,
    ASTC compressed format where each 128-bit compressed texel block encodes
    a 10{times}10 rectangle of signed floating-point RGBA texel data.
endif::VK_EXT_texture_compression_astc_hdr[]
  * ename:VK_FORMAT_ASTC_12x10_UNORM_BLOCK specifies a four-component, ASTC
    compressed format where each 128-bit compressed texel block encodes a
    12{times}10 rectangle of unsigned normalized RGBA texel data.
  * ename:VK_FORMAT_ASTC_12x10_SRGB_BLOCK specifies a four-component, ASTC
    compressed format where each 128-bit compressed texel block encodes a
    12{times}10 rectangle of unsigned normalized RGBA texel data with sRGB
    nonlinear encoding applied to the RGB components.
ifdef::VK_EXT_texture_compression_astc_hdr[]
  * ename:VK_FORMAT_ASTC_12x10_SFLOAT_BLOCK_EXT specifies a four-component,
    ASTC compressed format where each 128-bit compressed texel block encodes
    a 12{times}10 rectangle of signed floating-point RGBA texel data.
endif::VK_EXT_texture_compression_astc_hdr[]
  * ename:VK_FORMAT_ASTC_12x12_UNORM_BLOCK specifies a four-component, ASTC
    compressed format where each 128-bit compressed texel block encodes a
    12{times}12 rectangle of unsigned normalized RGBA texel data.
  * ename:VK_FORMAT_ASTC_12x12_SRGB_BLOCK specifies a four-component, ASTC
    compressed format where each 128-bit compressed texel block encodes a
    12{times}12 rectangle of unsigned normalized RGBA texel data with sRGB
    nonlinear encoding applied to the RGB components.
ifdef::VK_EXT_texture_compression_astc_hdr[]
  * ename:VK_FORMAT_ASTC_12x12_SFLOAT_BLOCK_EXT specifies a four-component,
    ASTC compressed format where each 128-bit compressed texel block encodes
    a 12{times}12 rectangle of signed floating-point RGBA texel data.
endif::VK_EXT_texture_compression_astc_hdr[]
ifdef::VK_VERSION_1_1,VK_KHR_sampler_ycbcr_conversion[]
  * ename:VK_FORMAT_G8B8G8R8_422_UNORM specifies a four-component, 32-bit
    format containing a pair of G components, an R component, and a B
    component, collectively encoding a 2{times}1 rectangle of unsigned
    normalized RGB texel data.
    One G value is present at each _i_ coordinate, with the B and R values
    shared across both G values and thus recorded at half the horizontal
    resolution of the image.
    This format has an 8-bit G component for the even _i_ coordinate in byte
    0, an 8-bit B component in byte 1, an 8-bit G component for the odd _i_
    coordinate in byte 2, and an 8-bit R component in byte 3.
    This format only supports images with a width that is a multiple of two.
    For the purposes of the constraints on copy extents, this format is
    treated as a compressed format with a 2{times}1 compressed texel block.
  * ename:VK_FORMAT_B8G8R8G8_422_UNORM specifies a four-component, 32-bit
    format containing a pair of G components, an R component, and a B
    component, collectively encoding a 2{times}1 rectangle of unsigned
    normalized RGB texel data.
    One G value is present at each _i_ coordinate, with the B and R values
    shared across both G values and thus recorded at half the horizontal
    resolution of the image.
    This format has an 8-bit B component in byte 0, an 8-bit G component for
    the even _i_ coordinate in byte 1, an 8-bit R component in byte 2, and
    an 8-bit G component for the odd _i_ coordinate in byte 3.
    This format only supports images with a width that is a multiple of two.
    For the purposes of the constraints on copy extents, this format is
    treated as a compressed format with a 2{times}1 compressed texel block.
  * ename:VK_FORMAT_G8_B8_R8_3PLANE_420_UNORM specifies an unsigned
    normalized _multi-planar format_ that has an 8-bit G component in plane
    0, an 8-bit B component in plane 1, and an 8-bit R component in plane 2.
    The horizontal and vertical dimensions of the R and B planes are halved
    relative to the image dimensions, and each R and B component is shared
    with the G components for which latexmath:[\left\lfloor i_G \times 0.5
    \right\rfloor = i_B = i_R] and latexmath:[\left\lfloor j_G \times 0.5
    \right\rfloor = j_B = j_R].
    The location of each plane when this image is in linear layout can be
    determined via flink:vkGetImageSubresourceLayout, using
    ename:VK_IMAGE_ASPECT_PLANE_0_BIT for the G plane,
    ename:VK_IMAGE_ASPECT_PLANE_1_BIT for the B plane, and
    ename:VK_IMAGE_ASPECT_PLANE_2_BIT for the R plane.
    This format only supports images with a width and height that is a
    multiple of two.
  * ename:VK_FORMAT_G8_B8R8_2PLANE_420_UNORM specifies an unsigned
    normalized _multi-planar format_ that has an 8-bit G component in plane
    0, and a two-component, 16-bit BR plane 1 consisting of an 8-bit B
    component in byte 0 and an 8-bit R component in byte 1.
    The horizontal and vertical dimensions of the BR plane are halved
    relative to the image dimensions, and each R and B value is shared with
    the G components for which latexmath:[\left\lfloor i_G \times 0.5
    \right\rfloor = i_B = i_R] and latexmath:[\left\lfloor j_G \times 0.5
    \right\rfloor = j_B = j_R].
    The location of each plane when this image is in linear layout can be
    determined via flink:vkGetImageSubresourceLayout, using
    ename:VK_IMAGE_ASPECT_PLANE_0_BIT for the G plane, and
    ename:VK_IMAGE_ASPECT_PLANE_1_BIT for the BR plane.
    This format only supports images with a width and height that is a
    multiple of two.
  * ename:VK_FORMAT_G8_B8_R8_3PLANE_422_UNORM specifies an unsigned
    normalized _multi-planar format_ that has an 8-bit G component in plane
    0, an 8-bit B component in plane 1, and an 8-bit R component in plane 2.
    The horizontal dimension of the R and B plane is halved relative to the
    image dimensions, and each R and B value is shared with the G components
    for which latexmath:[\left\lfloor i_G \times 0.5 \right\rfloor = i_B =
    i_R].
    The location of each plane when this image is in linear layout can be
    determined via flink:vkGetImageSubresourceLayout, using
    ename:VK_IMAGE_ASPECT_PLANE_0_BIT for the G plane,
    ename:VK_IMAGE_ASPECT_PLANE_1_BIT for the B plane, and
    ename:VK_IMAGE_ASPECT_PLANE_2_BIT for the R plane.
    This format only supports images with a width that is a multiple of two.
  * ename:VK_FORMAT_G8_B8R8_2PLANE_422_UNORM specifies an unsigned
    normalized _multi-planar format_ that has an 8-bit G component in plane
    0, and a two-component, 16-bit BR plane 1 consisting of an 8-bit B
    component in byte 0 and an 8-bit R component in byte 1.
    The horizontal dimension of the BR plane is halved relative to the image
    dimensions, and each R and B value is shared with the G components for
    which latexmath:[\left\lfloor i_G \times 0.5 \right\rfloor = i_B = i_R].
    The location of each plane when this image is in linear layout can be
    determined via flink:vkGetImageSubresourceLayout, using
    ename:VK_IMAGE_ASPECT_PLANE_0_BIT for the G plane, and
    ename:VK_IMAGE_ASPECT_PLANE_1_BIT for the BR plane.
    This format only supports images with a width that is a multiple of two.
  * ename:VK_FORMAT_G8_B8_R8_3PLANE_444_UNORM specifies an unsigned
    normalized _multi-planar format_ that has an 8-bit G component in plane
    0, an 8-bit B component in plane 1, and an 8-bit R component in plane 2.
    Each plane has the same dimensions and each R, G and B component
    contributes to a single texel.
    The location of each plane when this image is in linear layout can be
    determined via flink:vkGetImageSubresourceLayout, using
    ename:VK_IMAGE_ASPECT_PLANE_0_BIT for the G plane,
    ename:VK_IMAGE_ASPECT_PLANE_1_BIT for the B plane, and
    ename:VK_IMAGE_ASPECT_PLANE_2_BIT for the R plane.
  * ename:VK_FORMAT_R10X6_UNORM_PACK16 specifies a one-component, 16-bit
    unsigned normalized format that has a single 10-bit R component in the
    top 10 bits of a 16-bit word, with the bottom 6 bits unused.
  * ename:VK_FORMAT_R10X6G10X6_UNORM_2PACK16 specifies a two-component,
    32-bit unsigned normalized format that has a 10-bit R component in the
    top 10 bits of the word in bytes 0..1, and a 10-bit G component in the
    top 10 bits of the word in bytes 2..3, with the bottom 6 bits of each
    word unused.
  * ename:VK_FORMAT_R10X6G10X6B10X6A10X6_UNORM_4PACK16 specifies a
    four-component, 64-bit unsigned normalized format that has a 10-bit R
    component in the top 10 bits of the word in bytes 0..1, a 10-bit G
    component in the top 10 bits of the word in bytes 2..3, a 10-bit B
    component in the top 10 bits of the word in bytes 4..5, and a 10-bit A
    component in the top 10 bits of the word in bytes 6..7, with the bottom
    6 bits of each word unused.
  * ename:VK_FORMAT_G10X6B10X6G10X6R10X6_422_UNORM_4PACK16 specifies a
    four-component, 64-bit format containing a pair of G components, an R
    component, and a B component, collectively encoding a 2{times}1
    rectangle of unsigned normalized RGB texel data.
    One G value is present at each _i_ coordinate, with the B and R values
    shared across both G values and thus recorded at half the horizontal
    resolution of the image.
    This format has a 10-bit G component for the even _i_ coordinate in the
    top 10 bits of the word in bytes 0..1, a 10-bit B component in the top
    10 bits of the word in bytes 2..3, a 10-bit G component for the odd _i_
    coordinate in the top 10 bits of the word in bytes 4..5, and a 10-bit R
    component in the top 10 bits of the word in bytes 6..7, with the bottom
    6 bits of each word unused.
    This format only supports images with a width that is a multiple of two.
    For the purposes of the constraints on copy extents, this format is
    treated as a compressed format with a 2{times}1 compressed texel block.
  * ename:VK_FORMAT_B10X6G10X6R10X6G10X6_422_UNORM_4PACK16 specifies a
    four-component, 64-bit format containing a pair of G components, an R
    component, and a B component, collectively encoding a 2{times}1
    rectangle of unsigned normalized RGB texel data.
    One G value is present at each _i_ coordinate, with the B and R values
    shared across both G values and thus recorded at half the horizontal
    resolution of the image.
    This format has a 10-bit B component in the top 10 bits of the word in
    bytes 0..1, a 10-bit G component for the even _i_ coordinate in the top
    10 bits of the word in bytes 2..3, a 10-bit R component in the top 10
    bits of the word in bytes 4..5, and a 10-bit G component for the odd _i_
    coordinate in the top 10 bits of the word in bytes 6..7, with the bottom
    6 bits of each word unused.
    This format only supports images with a width that is a multiple of two.
    For the purposes of the constraints on copy extents, this format is
    treated as a compressed format with a 2{times}1 compressed texel block.
  * ename:VK_FORMAT_G10X6_B10X6_R10X6_3PLANE_420_UNORM_3PACK16 specifies an
    unsigned normalized _multi-planar format_ that has a 10-bit G component
    in the top 10 bits of each 16-bit word of plane 0, a 10-bit B component
    in the top 10 bits of each 16-bit word of plane 1, and a 10-bit R
    component in the top 10 bits of each 16-bit word of plane 2, with the
    bottom 6 bits of each word unused.
    The horizontal and vertical dimensions of the R and B planes are halved
    relative to the image dimensions, and each R and B component is shared
    with the G components for which latexmath:[\left\lfloor i_G \times 0.5
    \right\rfloor = i_B = i_R] and latexmath:[\left\lfloor j_G \times 0.5
    \right\rfloor = j_B = j_R].
    The location of each plane when this image is in linear layout can be
    determined via flink:vkGetImageSubresourceLayout, using
    ename:VK_IMAGE_ASPECT_PLANE_0_BIT for the G plane,
    ename:VK_IMAGE_ASPECT_PLANE_1_BIT for the B plane, and
    ename:VK_IMAGE_ASPECT_PLANE_2_BIT for the R plane.
    This format only supports images with a width and height that is a
    multiple of two.
  * ename:VK_FORMAT_G10X6_B10X6R10X6_2PLANE_420_UNORM_3PACK16 specifies an
    unsigned normalized _multi-planar format_ that has a 10-bit G component
    in the top 10 bits of each 16-bit word of plane 0, and a two-component,
    32-bit BR plane 1 consisting of a 10-bit B component in the top 10 bits
    of the word in bytes 0..1, and a 10-bit R component in the top 10 bits
    of the word in bytes 2..3, with the bottom 6 bits of each word unused.
    The horizontal and vertical dimensions of the BR plane are halved
    relative to the image dimensions, and each R and B value is shared with
    the G components for which latexmath:[\left\lfloor i_G \times 0.5
    \right\rfloor = i_B = i_R] and latexmath:[\left\lfloor j_G \times 0.5
    \right\rfloor = j_B = j_R].
    The location of each plane when this image is in linear layout can be
    determined via flink:vkGetImageSubresourceLayout, using
    ename:VK_IMAGE_ASPECT_PLANE_0_BIT for the G plane, and
    ename:VK_IMAGE_ASPECT_PLANE_1_BIT for the BR plane.
    This format only supports images with a width and height that is a
    multiple of two.
  * ename:VK_FORMAT_G10X6_B10X6_R10X6_3PLANE_422_UNORM_3PACK16 specifies an
    unsigned normalized _multi-planar format_ that has a 10-bit G component
    in the top 10 bits of each 16-bit word of plane 0, a 10-bit B component
    in the top 10 bits of each 16-bit word of plane 1, and a 10-bit R
    component in the top 10 bits of each 16-bit word of plane 2, with the
    bottom 6 bits of each word unused.
    The horizontal dimension of the R and B plane is halved relative to the
    image dimensions, and each R and B value is shared with the G components
    for which latexmath:[\left\lfloor i_G \times 0.5 \right\rfloor = i_B =
    i_R].
    The location of each plane when this image is in linear layout can be
    determined via flink:vkGetImageSubresourceLayout, using
    ename:VK_IMAGE_ASPECT_PLANE_0_BIT for the G plane,
    ename:VK_IMAGE_ASPECT_PLANE_1_BIT for the B plane, and
    ename:VK_IMAGE_ASPECT_PLANE_2_BIT for the R plane.
    This format only supports images with a width that is a multiple of two.
  * ename:VK_FORMAT_G10X6_B10X6R10X6_2PLANE_422_UNORM_3PACK16 specifies an
    unsigned normalized _multi-planar format_ that has a 10-bit G component
    in the top 10 bits of each 16-bit word of plane 0, and a two-component,
    32-bit BR plane 1 consisting of a 10-bit B component in the top 10 bits
    of the word in bytes 0..1, and a 10-bit R component in the top 10 bits
    of the word in bytes 2..3, with the bottom 6 bits of each word unused.
    The horizontal dimension of the BR plane is halved relative to the image
    dimensions, and each R and B value is shared with the G components for
    which latexmath:[\left\lfloor i_G \times 0.5 \right\rfloor = i_B = i_R].
    The location of each plane when this image is in linear layout can be
    determined via flink:vkGetImageSubresourceLayout, using
    ename:VK_IMAGE_ASPECT_PLANE_0_BIT for the G plane, and
    ename:VK_IMAGE_ASPECT_PLANE_1_BIT for the BR plane.
    This format only supports images with a width that is a multiple of two.
  * ename:VK_FORMAT_G10X6_B10X6_R10X6_3PLANE_444_UNORM_3PACK16 specifies an
    unsigned normalized _multi-planar format_ that has a 10-bit G component
    in the top 10 bits of each 16-bit word of plane 0, a 10-bit B component
    in the top 10 bits of each 16-bit word of plane 1, and a 10-bit R
    component in the top 10 bits of each 16-bit word of plane 2, with the
    bottom 6 bits of each word unused.
    Each plane has the same dimensions and each R, G and B component
    contributes to a single texel.
    The location of each plane when this image is in linear layout can be
    determined via flink:vkGetImageSubresourceLayout, using
    ename:VK_IMAGE_ASPECT_PLANE_0_BIT for the G plane,
    ename:VK_IMAGE_ASPECT_PLANE_1_BIT for the B plane, and
    ename:VK_IMAGE_ASPECT_PLANE_2_BIT for the R plane.
  * ename:VK_FORMAT_R12X4_UNORM_PACK16 specifies a one-component, 16-bit
    unsigned normalized format that has a single 12-bit R component in the
    top 12 bits of a 16-bit word, with the bottom 4 bits unused.
  * ename:VK_FORMAT_R12X4G12X4_UNORM_2PACK16 specifies a two-component,
    32-bit unsigned normalized format that has a 12-bit R component in the
    top 12 bits of the word in bytes 0..1, and a 12-bit G component in the
    top 12 bits of the word in bytes 2..3, with the bottom 4 bits of each
    word unused.
  * ename:VK_FORMAT_R12X4G12X4B12X4A12X4_UNORM_4PACK16 specifies a
    four-component, 64-bit unsigned normalized format that has a 12-bit R
    component in the top 12 bits of the word in bytes 0..1, a 12-bit G
    component in the top 12 bits of the word in bytes 2..3, a 12-bit B
    component in the top 12 bits of the word in bytes 4..5, and a 12-bit A
    component in the top 12 bits of the word in bytes 6..7, with the bottom
    4 bits of each word unused.
  * ename:VK_FORMAT_G12X4B12X4G12X4R12X4_422_UNORM_4PACK16 specifies a
    four-component, 64-bit format containing a pair of G components, an R
    component, and a B component, collectively encoding a 2{times}1
    rectangle of unsigned normalized RGB texel data.
    One G value is present at each _i_ coordinate, with the B and R values
    shared across both G values and thus recorded at half the horizontal
    resolution of the image.
    This format has a 12-bit G component for the even _i_ coordinate in the
    top 12 bits of the word in bytes 0..1, a 12-bit B component in the top
    12 bits of the word in bytes 2..3, a 12-bit G component for the odd _i_
    coordinate in the top 12 bits of the word in bytes 4..5, and a 12-bit R
    component in the top 12 bits of the word in bytes 6..7, with the bottom
    4 bits of each word unused.
    This format only supports images with a width that is a multiple of two.
    For the purposes of the constraints on copy extents, this format is
    treated as a compressed format with a 2{times}1 compressed texel block.
  * ename:VK_FORMAT_B12X4G12X4R12X4G12X4_422_UNORM_4PACK16 specifies a
    four-component, 64-bit format containing a pair of G components, an R
    component, and a B component, collectively encoding a 2{times}1
    rectangle of unsigned normalized RGB texel data.
    One G value is present at each _i_ coordinate, with the B and R values
    shared across both G values and thus recorded at half the horizontal
    resolution of the image.
    This format has a 12-bit B component in the top 12 bits of the word in
    bytes 0..1, a 12-bit G component for the even _i_ coordinate in the top
    12 bits of the word in bytes 2..3, a 12-bit R component in the top 12
    bits of the word in bytes 4..5, and a 12-bit G component for the odd _i_
    coordinate in the top 12 bits of the word in bytes 6..7, with the bottom
    4 bits of each word unused.
    This format only supports images with a width that is a multiple of two.
    For the purposes of the constraints on copy extents, this format is
    treated as a compressed format with a 2{times}1 compressed texel block.
  * ename:VK_FORMAT_G12X4_B12X4_R12X4_3PLANE_420_UNORM_3PACK16 specifies an
    unsigned normalized _multi-planar format_ that has a 12-bit G component
    in the top 12 bits of each 16-bit word of plane 0, a 12-bit B component
    in the top 12 bits of each 16-bit word of plane 1, and a 12-bit R
    component in the top 12 bits of each 16-bit word of plane 2, with the
    bottom 4 bits of each word unused.
    The horizontal and vertical dimensions of the R and B planes are halved
    relative to the image dimensions, and each R and B component is shared
    with the G components for which latexmath:[\left\lfloor i_G \times 0.5
    \right\rfloor = i_B = i_R] and latexmath:[\left\lfloor j_G \times 0.5
    \right\rfloor = j_B = j_R].
    The location of each plane when this image is in linear layout can be
    determined via flink:vkGetImageSubresourceLayout, using
    ename:VK_IMAGE_ASPECT_PLANE_0_BIT for the G plane,
    ename:VK_IMAGE_ASPECT_PLANE_1_BIT for the B plane, and
    ename:VK_IMAGE_ASPECT_PLANE_2_BIT for the R plane.
    This format only supports images with a width and height that is a
    multiple of two.
  * ename:VK_FORMAT_G12X4_B12X4R12X4_2PLANE_420_UNORM_3PACK16 specifies an
    unsigned normalized _multi-planar format_ that has a 12-bit G component
    in the top 12 bits of each 16-bit word of plane 0, and a two-component,
    32-bit BR plane 1 consisting of a 12-bit B component in the top 12 bits
    of the word in bytes 0..1, and a 12-bit R component in the top 12 bits
    of the word in bytes 2..3, with the bottom 4 bits of each word unused.
    The horizontal and vertical dimensions of the BR plane are halved
    relative to the image dimensions, and each R and B value is shared with
    the G components for which latexmath:[\left\lfloor i_G \times 0.5
    \right\rfloor = i_B = i_R] and latexmath:[\left\lfloor j_G \times 0.5
    \right\rfloor = j_B = j_R].
    The location of each plane when this image is in linear layout can be
    determined via flink:vkGetImageSubresourceLayout, using
    ename:VK_IMAGE_ASPECT_PLANE_0_BIT for the G plane, and
    ename:VK_IMAGE_ASPECT_PLANE_1_BIT for the BR plane.
    This format only supports images with a width and height that is a
    multiple of two.
  * ename:VK_FORMAT_G12X4_B12X4_R12X4_3PLANE_422_UNORM_3PACK16 specifies an
    unsigned normalized _multi-planar format_ that has a 12-bit G component
    in the top 12 bits of each 16-bit word of plane 0, a 12-bit B component
    in the top 12 bits of each 16-bit word of plane 1, and a 12-bit R
    component in the top 12 bits of each 16-bit word of plane 2, with the
    bottom 4 bits of each word unused.
    The horizontal dimension of the R and B plane is halved relative to the
    image dimensions, and each R and B value is shared with the G components
    for which latexmath:[\left\lfloor i_G \times 0.5 \right\rfloor = i_B =
    i_R].
    The location of each plane when this image is in linear layout can be
    determined via flink:vkGetImageSubresourceLayout, using
    ename:VK_IMAGE_ASPECT_PLANE_0_BIT for the G plane,
    ename:VK_IMAGE_ASPECT_PLANE_1_BIT for the B plane, and
    ename:VK_IMAGE_ASPECT_PLANE_2_BIT for the R plane.
    This format only supports images with a width that is a multiple of two.
  * ename:VK_FORMAT_G12X4_B12X4R12X4_2PLANE_422_UNORM_3PACK16 specifies an
    unsigned normalized _multi-planar format_ that has a 12-bit G component
    in the top 12 bits of each 16-bit word of plane 0, and a two-component,
    32-bit BR plane 1 consisting of a 12-bit B component in the top 12 bits
    of the word in bytes 0..1, and a 12-bit R component in the top 12 bits
    of the word in bytes 2..3, with the bottom 4 bits of each word unused.
    The horizontal dimension of the BR plane is halved relative to the image
    dimensions, and each R and B value is shared with the G components for
    which latexmath:[\left\lfloor i_G \times 0.5 \right\rfloor = i_B = i_R].
    The location of each plane when this image is in linear layout can be
    determined via flink:vkGetImageSubresourceLayout, using
    ename:VK_IMAGE_ASPECT_PLANE_0_BIT for the G plane, and
    ename:VK_IMAGE_ASPECT_PLANE_1_BIT for the BR plane.
    This format only supports images with a width that is a multiple of two.
  * ename:VK_FORMAT_G12X4_B12X4_R12X4_3PLANE_444_UNORM_3PACK16 specifies an
    unsigned normalized _multi-planar format_ that has a 12-bit G component
    in the top 12 bits of each 16-bit word of plane 0, a 12-bit B component
    in the top 12 bits of each 16-bit word of plane 1, and a 12-bit R
    component in the top 12 bits of each 16-bit word of plane 2, with the
    bottom 4 bits of each word unused.
    Each plane has the same dimensions and each R, G and B component
    contributes to a single texel.
    The location of each plane when this image is in linear layout can be
    determined via flink:vkGetImageSubresourceLayout, using
    ename:VK_IMAGE_ASPECT_PLANE_0_BIT for the G plane,
    ename:VK_IMAGE_ASPECT_PLANE_1_BIT for the B plane, and
    ename:VK_IMAGE_ASPECT_PLANE_2_BIT for the R plane.
  * ename:VK_FORMAT_G16B16G16R16_422_UNORM specifies a four-component,
    64-bit format containing a pair of G components, an R component, and a B
    component, collectively encoding a 2{times}1 rectangle of unsigned
    normalized RGB texel data.
    One G value is present at each _i_ coordinate, with the B and R values
    shared across both G values and thus recorded at half the horizontal
    resolution of the image.
    This format has a 16-bit G component for the even _i_ coordinate in the
    word in bytes 0..1, a 16-bit B component in the word in bytes 2..3, a
    16-bit G component for the odd _i_ coordinate in the word in bytes 4..5,
    and a 16-bit R component in the word in bytes 6..7.
    This format only supports images with a width that is a multiple of two.
    For the purposes of the constraints on copy extents, this format is
    treated as a compressed format with a 2{times}1 compressed texel block.
  * ename:VK_FORMAT_B16G16R16G16_422_UNORM specifies a four-component,
    64-bit format containing a pair of G components, an R component, and a B
    component, collectively encoding a 2{times}1 rectangle of unsigned
    normalized RGB texel data.
    One G value is present at each _i_ coordinate, with the B and R values
    shared across both G values and thus recorded at half the horizontal
    resolution of the image.
    This format has a 16-bit B component in the word in bytes 0..1, a 16-bit
    G component for the even _i_ coordinate in the word in bytes 2..3, a
    16-bit R component in the word in bytes 4..5, and a 16-bit G component
    for the odd _i_ coordinate in the word in bytes 6..7.
    This format only supports images with a width that is a multiple of two.
    For the purposes of the constraints on copy extents, this format is
    treated as a compressed format with a 2{times}1 compressed texel block.
  * ename:VK_FORMAT_G16_B16_R16_3PLANE_420_UNORM specifies an unsigned
    normalized _multi-planar format_ that has a 16-bit G component in each
    16-bit word of plane 0, a 16-bit B component in each 16-bit word of
    plane 1, and a 16-bit R component in each 16-bit word of plane 2.
    The horizontal and vertical dimensions of the R and B planes are halved
    relative to the image dimensions, and each R and B component is shared
    with the G components for which latexmath:[\left\lfloor i_G \times 0.5
    \right\rfloor = i_B = i_R] and latexmath:[\left\lfloor j_G \times 0.5
    \right\rfloor = j_B = j_R].
    The location of each plane when this image is in linear layout can be
    determined via flink:vkGetImageSubresourceLayout, using
    ename:VK_IMAGE_ASPECT_PLANE_0_BIT for the G plane,
    ename:VK_IMAGE_ASPECT_PLANE_1_BIT for the B plane, and
    ename:VK_IMAGE_ASPECT_PLANE_2_BIT for the R plane.
    This format only supports images with a width and height that is a
    multiple of two.
  * ename:VK_FORMAT_G16_B16R16_2PLANE_420_UNORM specifies an unsigned
    normalized _multi-planar format_ that has a 16-bit G component in each
    16-bit word of plane 0, and a two-component, 32-bit BR plane 1
    consisting of a 16-bit B component in the word in bytes 0..1, and a
    16-bit R component in the word in bytes 2..3.
    The horizontal and vertical dimensions of the BR plane are halved
    relative to the image dimensions, and each R and B value is shared with
    the G components for which latexmath:[\left\lfloor i_G \times 0.5
    \right\rfloor = i_B = i_R] and latexmath:[\left\lfloor j_G \times 0.5
    \right\rfloor = j_B = j_R].
    The location of each plane when this image is in linear layout can be
    determined via flink:vkGetImageSubresourceLayout, using
    ename:VK_IMAGE_ASPECT_PLANE_0_BIT for the G plane, and
    ename:VK_IMAGE_ASPECT_PLANE_1_BIT for the BR plane.
    This format only supports images with a width and height that is a
    multiple of two.
  * ename:VK_FORMAT_G16_B16_R16_3PLANE_422_UNORM specifies an unsigned
    normalized _multi-planar format_ that has a 16-bit G component in each
    16-bit word of plane 0, a 16-bit B component in each 16-bit word of
    plane 1, and a 16-bit R component in each 16-bit word of plane 2.
    The horizontal dimension of the R and B plane is halved relative to the
    image dimensions, and each R and B value is shared with the G components
    for which latexmath:[\left\lfloor i_G \times 0.5 \right\rfloor = i_B =
    i_R].
    The location of each plane when this image is in linear layout can be
    determined via flink:vkGetImageSubresourceLayout, using
    ename:VK_IMAGE_ASPECT_PLANE_0_BIT for the G plane,
    ename:VK_IMAGE_ASPECT_PLANE_1_BIT for the B plane, and
    ename:VK_IMAGE_ASPECT_PLANE_2_BIT for the R plane.
    This format only supports images with a width that is a multiple of two.
  * ename:VK_FORMAT_G16_B16R16_2PLANE_422_UNORM specifies an unsigned
    normalized _multi-planar format_ that has a 16-bit G component in each
    16-bit word of plane 0, and a two-component, 32-bit BR plane 1
    consisting of a 16-bit B component in the word in bytes 0..1, and a
    16-bit R component in the word in bytes 2..3.
    The horizontal dimension of the BR plane is halved relative to the image
    dimensions, and each R and B value is shared with the G components for
    which latexmath:[\left\lfloor i_G \times 0.5 \right\rfloor = i_B = i_R].
    The location of each plane when this image is in linear layout can be
    determined via flink:vkGetImageSubresourceLayout, using
    ename:VK_IMAGE_ASPECT_PLANE_0_BIT for the G plane, and
    ename:VK_IMAGE_ASPECT_PLANE_1_BIT for the BR plane.
    This format only supports images with a width that is a multiple of two.
  * ename:VK_FORMAT_G16_B16_R16_3PLANE_444_UNORM specifies an unsigned
    normalized _multi-planar format_ that has a 16-bit G component in each
    16-bit word of plane 0, a 16-bit B component in each 16-bit word of
    plane 1, and a 16-bit R component in each 16-bit word of plane 2.
    Each plane has the same dimensions and each R, G and B component
    contributes to a single texel.
    The location of each plane when this image is in linear layout can be
    determined via flink:vkGetImageSubresourceLayout, using
    ename:VK_IMAGE_ASPECT_PLANE_0_BIT for the G plane,
    ename:VK_IMAGE_ASPECT_PLANE_1_BIT for the B plane, and
    ename:VK_IMAGE_ASPECT_PLANE_2_BIT for the R plane.
endif::VK_VERSION_1_1,VK_KHR_sampler_ycbcr_conversion[]
ifdef::VK_EXT_ycbcr_2plane_444_formats[]
  * ename:VK_FORMAT_G8_B8R8_2PLANE_444_UNORM_EXT specifies an unsigned
    normalized _multi-planar format_ that has an 8-bit G component in plane
    0, and a two-component, 16-bit BR plane 1 consisting of an 8-bit B
    component in byte 0 and an 8-bit R component in byte 1.
    Both planes have the same dimensions and each R, G and B component
    contributes to a single texel.
    The location of each plane when this image is in linear layout can be
    determined via flink:vkGetImageSubresourceLayout, using
    ename:VK_IMAGE_ASPECT_PLANE_0_BIT for the G plane, and
    ename:VK_IMAGE_ASPECT_PLANE_1_BIT for the BR plane.
  * ename:VK_FORMAT_G10X6_B10X6R10X6_2PLANE_444_UNORM_3PACK16_EXT specifies
    an unsigned normalized _multi-planar format_ that has a 10-bit G
    component in the top 10 bits of each 16-bit word of plane 0, and a
    two-component, 32-bit BR plane 1 consisting of a 10-bit B component in
    the top 10 bits of the word in bytes 0..1, and a 10-bit R component in
    the top 10 bits of the word in bytes 2..3, the bottom 6 bits of each
    word unused.
    Both planes have the same dimensions and each R, G and B component
    contributes to a single texel.
    The location of each plane when this image is in linear layout can be
    determined via flink:vkGetImageSubresourceLayout, using
    ename:VK_IMAGE_ASPECT_PLANE_0_BIT for the G plane, and
    ename:VK_IMAGE_ASPECT_PLANE_1_BIT for the BR plane.
  * ename:VK_FORMAT_G12X4_B12X4R12X4_2PLANE_444_UNORM_3PACK16_EXT specifies
    an unsigned normalized _multi-planar format_ that has a 12-bit G
    component in the top 12 bits of each 16-bit word of plane 0, and a
    two-component, 32-bit BR plane 1 consisting of a 12-bit B component in
    the top 12 bits of the word in bytes 0..1, and a 12-bit R component in
    the top 12 bits of the word in bytes 2..3, the bottom 4 bits of each
    word unused.
    Both planes have the same dimensions and each R, G and B component
    contributes to a single texel.
    The location of each plane when this image is in linear layout can be
    determined via flink:vkGetImageSubresourceLayout, using
    ename:VK_IMAGE_ASPECT_PLANE_0_BIT for the G plane, and
    ename:VK_IMAGE_ASPECT_PLANE_1_BIT for the BR plane.
  * ename:VK_FORMAT_G16_B16R16_2PLANE_444_UNORM_EXT specifies an unsigned
    normalized _multi-planar format_ that has a 16-bit G component in each
    16-bit word of plane 0, and a two-component, 32-bit BR plane 1
    consisting of a 16-bit B component in the word in bytes 0..1, and a
    16-bit R component in the word in bytes 2..3.
    Both planes have the same dimensions and each R, G and B component
    contributes to a single texel.
    The location of each plane when this image is in linear layout can be
    determined via flink:vkGetImageSubresourceLayout, using
    ename:VK_IMAGE_ASPECT_PLANE_0_BIT for the G plane, and
    ename:VK_IMAGE_ASPECT_PLANE_1_BIT for the BR plane.
endif::VK_EXT_ycbcr_2plane_444_formats[]
ifdef::VK_IMG_format_pvrtc[]
  * ename:VK_FORMAT_PVRTC1_2BPP_UNORM_BLOCK_IMG specifies a four-component,
    PVRTC compressed format where each 64-bit compressed texel block encodes
    an 8{times}4 rectangle of unsigned normalized RGBA texel data.
  * ename:VK_FORMAT_PVRTC1_4BPP_UNORM_BLOCK_IMG specifies a four-component,
    PVRTC compressed format where each 64-bit compressed texel block encodes
    a 4{times}4 rectangle of unsigned normalized RGBA texel data.
  * ename:VK_FORMAT_PVRTC2_2BPP_UNORM_BLOCK_IMG specifies a four-component,
    PVRTC compressed format where each 64-bit compressed texel block encodes
    an 8{times}4 rectangle of unsigned normalized RGBA texel data.
  * ename:VK_FORMAT_PVRTC2_4BPP_UNORM_BLOCK_IMG specifies a four-component,
    PVRTC compressed format where each 64-bit compressed texel block encodes
    a 4{times}4 rectangle of unsigned normalized RGBA texel data.
  * ename:VK_FORMAT_PVRTC1_2BPP_SRGB_BLOCK_IMG specifies a four-component,
    PVRTC compressed format where each 64-bit compressed texel block encodes
    an 8{times}4 rectangle of unsigned normalized RGBA texel data with sRGB
    nonlinear encoding applied to the RGB components.
  * ename:VK_FORMAT_PVRTC1_4BPP_SRGB_BLOCK_IMG specifies a four-component,
    PVRTC compressed format where each 64-bit compressed texel block encodes
    a 4{times}4 rectangle of unsigned normalized RGBA texel data with sRGB
    nonlinear encoding applied to the RGB components.
  * ename:VK_FORMAT_PVRTC2_2BPP_SRGB_BLOCK_IMG specifies a four-component,
    PVRTC compressed format where each 64-bit compressed texel block encodes
    an 8{times}4 rectangle of unsigned normalized RGBA texel data with sRGB
    nonlinear encoding applied to the RGB components.
  * ename:VK_FORMAT_PVRTC2_4BPP_SRGB_BLOCK_IMG specifies a four-component,
    PVRTC compressed format where each 64-bit compressed texel block encodes
    a 4{times}4 rectangle of unsigned normalized RGBA texel data with sRGB
    nonlinear encoding applied to the RGB components.
endif::VK_IMG_format_pvrtc[]

--


ifdef::VK_VERSION_1_1,VK_KHR_sampler_ycbcr_conversion[]

[[formats-compatible-planes]]
=== Compatible formats of planes of multi-planar formats

Individual planes of multi-planar formats are _compatible_ with single-plane
formats if they occupy the same number of bits per texel block.
In the following table, individual planes of a _multi-planar_ format are
compatible with the format listed against the relevant plane index for that
multi-planar format, and any format compatible with the listed single-plane
format according to <<formats-compatibility-classes, Format Compatibility
Classes>>.

.Plane Format Compatibility Table
[width="95%",cols="1,6,3,3",options="header"]
|====
^| Plane ^| Compatible format for plane ^| Width relative to the width _w_ of the plane with the largest dimensions ^| Height relative to the height _h_ of the plane with the largest dimensions
4+| *ename:VK_FORMAT_G8_B8_R8_3PLANE_420_UNORM*
^| 0     ^| ename:VK_FORMAT_R8_UNORM ^| w ^| h
^| 1     ^| ename:VK_FORMAT_R8_UNORM ^| w/2 ^| h/2
^| 2     ^| ename:VK_FORMAT_R8_UNORM ^| w/2 ^| h/2
4+| *ename:VK_FORMAT_G8_B8R8_2PLANE_420_UNORM*
^| 0     ^| ename:VK_FORMAT_R8_UNORM ^| w ^| h
^| 1     ^| ename:VK_FORMAT_R8G8_UNORM ^| w/2 ^| h/2
4+| *ename:VK_FORMAT_G8_B8_R8_3PLANE_422_UNORM*
^| 0     ^| ename:VK_FORMAT_R8_UNORM ^| w ^| h
^| 1     ^| ename:VK_FORMAT_R8_UNORM ^| w/2 ^| h
^| 2     ^| ename:VK_FORMAT_R8_UNORM ^| w/2 ^| h
4+| *ename:VK_FORMAT_G8_B8R8_2PLANE_422_UNORM*
^| 0     ^| ename:VK_FORMAT_R8_UNORM ^| w ^| h
^| 1     ^| ename:VK_FORMAT_R8G8_UNORM ^| w/2 ^| h
4+| *ename:VK_FORMAT_G8_B8_R8_3PLANE_444_UNORM*
^| 0     ^| ename:VK_FORMAT_R8_UNORM ^| w ^| h
^| 1     ^| ename:VK_FORMAT_R8_UNORM ^| w ^| h
^| 2     ^| ename:VK_FORMAT_R8_UNORM ^| w ^| h
4+| *ename:VK_FORMAT_G10X6_B10X6_R10X6_3PLANE_420_UNORM_3PACK16*
^| 0     ^| ename:VK_FORMAT_R10X6_UNORM_PACK16 ^| w ^| h
^| 1     ^| ename:VK_FORMAT_R10X6_UNORM_PACK16 ^| w/2 ^| h/2
^| 2     ^| ename:VK_FORMAT_R10X6_UNORM_PACK16 ^| w/2 ^| h/2
4+| *ename:VK_FORMAT_G10X6_B10X6R10X6_2PLANE_420_UNORM_3PACK16*
^| 0     ^| ename:VK_FORMAT_R10X6_UNORM_PACK16 ^| w ^| h
^| 1     ^| ename:VK_FORMAT_R10X6G10X6_UNORM_2PACK16 ^| w/2 ^| h/2
4+| *ename:VK_FORMAT_G10X6_B10X6_R10X6_3PLANE_422_UNORM_3PACK16*
^| 0     ^| ename:VK_FORMAT_R10X6_UNORM_PACK16 ^| w ^| h
^| 1     ^| ename:VK_FORMAT_R10X6_UNORM_PACK16 ^| w/2 ^| h
^| 2     ^| ename:VK_FORMAT_R10X6_UNORM_PACK16 ^| w/2 ^| h
4+| *ename:VK_FORMAT_G10X6_B10X6R10X6_2PLANE_422_UNORM_3PACK16*
^| 0     ^| ename:VK_FORMAT_R10X6_UNORM_PACK16 ^| w ^| h
^| 1     ^| ename:VK_FORMAT_R10X6G10X6_UNORM_2PACK16 ^| w/2 ^| h
4+| *ename:VK_FORMAT_G10X6_B10X6_R10X6_3PLANE_444_UNORM_3PACK16*
^| 0     ^| ename:VK_FORMAT_R10X6_UNORM_PACK16 ^| w ^| h
^| 1     ^| ename:VK_FORMAT_R10X6_UNORM_PACK16 ^| w ^| h
^| 2     ^| ename:VK_FORMAT_R10X6_UNORM_PACK16 ^| w ^| h
4+| *ename:VK_FORMAT_G12X4_B12X4_R12X4_3PLANE_420_UNORM_3PACK16*
^| 0     ^| ename:VK_FORMAT_R12X4_UNORM_PACK16 ^| w ^| h
^| 1     ^| ename:VK_FORMAT_R12X4_UNORM_PACK16 ^| w/2 ^| h/2
^| 2     ^| ename:VK_FORMAT_R12X4_UNORM_PACK16 ^| w/2 ^| h/2
4+| *ename:VK_FORMAT_G12X4_B12X4R12X4_2PLANE_420_UNORM_3PACK16*
^| 0     ^| ename:VK_FORMAT_R12X4_UNORM_PACK16 ^| w ^| h
^| 1     ^| ename:VK_FORMAT_R12X4G12X4_UNORM_2PACK16 ^| w/2 ^| h/2
4+| *ename:VK_FORMAT_G12X4_B12X4_R12X4_3PLANE_422_UNORM_3PACK16*
^| 0     ^| ename:VK_FORMAT_R12X4_UNORM_PACK16 ^| w ^| h
^| 1     ^| ename:VK_FORMAT_R12X4_UNORM_PACK16 ^| w/2 ^| h
^| 2     ^| ename:VK_FORMAT_R12X4_UNORM_PACK16 ^| w/2 ^| h
4+| *ename:VK_FORMAT_G12X4_B12X4R12X4_2PLANE_422_UNORM_3PACK16*
^| 0     ^| ename:VK_FORMAT_R12X4_UNORM_PACK16 ^| w ^| h
^| 1     ^| ename:VK_FORMAT_R12X4G12X4_UNORM_2PACK16 ^| w/2 ^| h
4+| *ename:VK_FORMAT_G12X4_B12X4_R12X4_3PLANE_444_UNORM_3PACK16*
^| 0     ^| ename:VK_FORMAT_R12X4_UNORM_PACK16 ^| w ^| h
^| 1     ^| ename:VK_FORMAT_R12X4_UNORM_PACK16 ^| w ^| h
^| 2     ^| ename:VK_FORMAT_R12X4_UNORM_PACK16 ^| w ^| h
4+| *ename:VK_FORMAT_G16_B16_R16_3PLANE_420_UNORM*
^| 0     ^| ename:VK_FORMAT_R16_UNORM ^| w ^| h
^| 1     ^| ename:VK_FORMAT_R16_UNORM ^| w/2 ^| h/2
^| 2     ^| ename:VK_FORMAT_R16_UNORM ^| w/2 ^| h/2
4+| *ename:VK_FORMAT_G16_B16R16_2PLANE_420_UNORM*
^| 0     ^| ename:VK_FORMAT_R16_UNORM ^| w ^| h
^| 1     ^| ename:VK_FORMAT_R16G16_UNORM ^| w/2 ^| h/2
4+| *ename:VK_FORMAT_G16_B16_R16_3PLANE_422_UNORM*
^| 0     ^| ename:VK_FORMAT_R16_UNORM ^| w ^| h
^| 1     ^| ename:VK_FORMAT_R16_UNORM ^| w/2 ^| h
^| 2     ^| ename:VK_FORMAT_R16_UNORM ^| w/2 ^| h
4+| *ename:VK_FORMAT_G16_B16R16_2PLANE_422_UNORM*
^| 0     ^| ename:VK_FORMAT_R16_UNORM ^| w ^| h
^| 1     ^| ename:VK_FORMAT_R16G16_UNORM ^| w/2 ^| h
4+| *ename:VK_FORMAT_G16_B16_R16_3PLANE_444_UNORM*
^| 0     ^| ename:VK_FORMAT_R16_UNORM ^| w ^| h
^| 1     ^| ename:VK_FORMAT_R16_UNORM ^| w ^| h
^| 2     ^| ename:VK_FORMAT_R16_UNORM ^| w ^| h
ifdef::VK_EXT_ycbcr_2plane_444_formats[]
4+| *ename:VK_FORMAT_G8_B8R8_2PLANE_444_UNORM_EXT*
^| 0     ^| ename:VK_FORMAT_R8_UNORM   ^| w ^| h
^| 1     ^| ename:VK_FORMAT_R8G8_UNORM ^| w ^| h
4+| *ename:VK_FORMAT_G10X6_B10X6R10X6_2PLANE_444_UNORM_3PACK16_EXT*
^| 0     ^| ename:VK_FORMAT_R10X6_UNORM_PACK16       ^| w ^| h
^| 1     ^| ename:VK_FORMAT_R10X6G10X6_UNORM_2PACK16 ^| w ^| h
4+| *ename:VK_FORMAT_G12X4_B12X4R12X4_2PLANE_444_UNORM_3PACK16_EXT*
^| 0     ^| ename:VK_FORMAT_R12X4_UNORM_PACK16       ^| w ^| h
^| 1     ^| ename:VK_FORMAT_R12X4G12X4_UNORM_2PACK16 ^| w ^| h
4+| *ename:VK_FORMAT_G16_B16R16_2PLANE_444_UNORM_EXT*
^| 0     ^| ename:VK_FORMAT_R16_UNORM    ^| w ^| h
^| 1     ^| ename:VK_FORMAT_R16G16_UNORM ^| w ^| h
endif::VK_EXT_ycbcr_2plane_444_formats[]
|====

endif::VK_VERSION_1_1,VK_KHR_sampler_ycbcr_conversion[]


[[formats-packed]]
=== Packed Formats

For the purposes of address alignment when accessing buffer memory
containing vertex attribute or texel data, the following formats are
considered _packed_ - whole texels or attributes are stored in bitfields of
a single 8-, 16-, or 32-bit fundamental data type.

  * <<formats-packed-8-bit,Packed into 8-bit data types>>:
  ** ename:VK_FORMAT_R4G4_UNORM_PACK8
  * <<formats-packed-16-bit,Packed into 16-bit data types>>:
  ** ename:VK_FORMAT_R4G4B4A4_UNORM_PACK16
  ** ename:VK_FORMAT_B4G4R4A4_UNORM_PACK16
ifdef::VK_EXT_4444_formats[]
  ** ename:VK_FORMAT_A4R4G4B4_UNORM_PACK16_EXT
  ** ename:VK_FORMAT_A4B4G4R4_UNORM_PACK16_EXT
endif::VK_EXT_4444_formats[]
  ** ename:VK_FORMAT_R5G6B5_UNORM_PACK16
  ** ename:VK_FORMAT_B5G6R5_UNORM_PACK16
  ** ename:VK_FORMAT_R5G5B5A1_UNORM_PACK16
  ** ename:VK_FORMAT_B5G5R5A1_UNORM_PACK16
  ** ename:VK_FORMAT_A1R5G5B5_UNORM_PACK16
  * <<formats-packed-32-bit,Packed into 32-bit data types>>:
  ** ename:VK_FORMAT_A8B8G8R8_UNORM_PACK32
  ** ename:VK_FORMAT_A8B8G8R8_SNORM_PACK32
  ** ename:VK_FORMAT_A8B8G8R8_USCALED_PACK32
  ** ename:VK_FORMAT_A8B8G8R8_SSCALED_PACK32
  ** ename:VK_FORMAT_A8B8G8R8_UINT_PACK32
  ** ename:VK_FORMAT_A8B8G8R8_SINT_PACK32
  ** ename:VK_FORMAT_A8B8G8R8_SRGB_PACK32
  ** ename:VK_FORMAT_A2R10G10B10_UNORM_PACK32
  ** ename:VK_FORMAT_A2R10G10B10_SNORM_PACK32
  ** ename:VK_FORMAT_A2R10G10B10_USCALED_PACK32
  ** ename:VK_FORMAT_A2R10G10B10_SSCALED_PACK32
  ** ename:VK_FORMAT_A2R10G10B10_UINT_PACK32
  ** ename:VK_FORMAT_A2R10G10B10_SINT_PACK32
  ** ename:VK_FORMAT_A2B10G10R10_UNORM_PACK32
  ** ename:VK_FORMAT_A2B10G10R10_SNORM_PACK32
  ** ename:VK_FORMAT_A2B10G10R10_USCALED_PACK32
  ** ename:VK_FORMAT_A2B10G10R10_SSCALED_PACK32
  ** ename:VK_FORMAT_A2B10G10R10_UINT_PACK32
  ** ename:VK_FORMAT_A2B10G10R10_SINT_PACK32
  ** ename:VK_FORMAT_B10G11R11_UFLOAT_PACK32
  ** ename:VK_FORMAT_E5B9G9R9_UFLOAT_PACK32
  ** ename:VK_FORMAT_X8_D24_UNORM_PACK32


=== Identification of Formats

A "`format`" is represented by a single enum value.
The name of a format is usually built up by using the following pattern:

....
    VK_FORMAT_{component-format|compression-scheme}_{numeric-format}
....

The component-format indicates either the size of the R, G, B, and A
components (if they are present) in the case of a color format, or the size
of the depth (D) and stencil (S) components (if they are present) in the
case of a depth/stencil format (see below).
An X indicates a component that is unused, but may: be present for padding.

<<<

[[formats-numericformat]]
.Interpretation of Numeric Format
[width="95%",cols="2,3,10",options="header"]
|====
| Numeric format | SPIR-V _Sampled Type_ | Description
| etext:UNORM    | OpTypeFloat           | The components are unsigned normalized values in the range [eq]#[0,1]#
| etext:SNORM    | OpTypeFloat           | The components are signed normalized values in the range [eq]#[-1,1]#
| etext:USCALED  | OpTypeFloat           | The components are unsigned integer values that get converted to floating-point in the range [0,2^n^-1]
| etext:SSCALED  | OpTypeFloat           | The components are signed integer values that get converted to floating-point in the range [-2^n-1^,2^n-1^-1]
| etext:UINT     | OpTypeInt             | The components are unsigned integer values in the range [0,2^n^-1]
| etext:SINT     | OpTypeInt             | The components are signed integer values in the range [-2^n-1^,2^n-1^-1]
| etext:UFLOAT   | OpTypeFloat           | The components are unsigned floating-point numbers (used by packed, shared exponent, and some compressed formats)
| etext:SFLOAT   | OpTypeFloat           | The components are signed floating-point numbers
| etext:SRGB     | OpTypeFloat           | The R, G, and B components are unsigned normalized values that represent values using sRGB nonlinear encoding, while the A component (if one exists) is a regular unsigned normalized value
3+| [eq]#n# is the number of bits in the component.
|====

The suffix etext:_PACKnn indicates that the format is packed into an
underlying type with nn bits.
ifdef::VK_VERSION_1_1,VK_KHR_sampler_ycbcr_conversion[]
The suffix etext:_mPACKnn is a short-hand that indicates that the format has
several components (which may or may not be stored in separate _planes_)
that are each packed into an underlying type with nn bits.
endif::VK_VERSION_1_1,VK_KHR_sampler_ycbcr_conversion[]

The suffix etext:_BLOCK indicates that the format is a block-compressed
format, with the representation of multiple pixels encoded interdependently
within a region.

[[formats-compressionscheme]]
.Interpretation of Compression Scheme
[width="95%",cols="2,10",options="header"]
|====
| Compression scheme | Description
| etext:BC           | Block Compression. See <<appendix-compressedtex-bc>>.
| etext:ETC2         | Ericsson Texture Compression. See <<appendix-compressedtex-etc2>>.
| etext:EAC          | ETC2 Alpha Compression. See <<appendix-compressedtex-etc2>>.
| etext:ASTC         | Adaptive Scalable Texture Compression (LDR Profile). See <<appendix-compressedtex-astc>>.
|====

ifdef::VK_VERSION_1_1,VK_KHR_sampler_ycbcr_conversion[]
For _multi-planar_ images, the components in separate _planes_ are separated
by underscores, and the number of planes is indicated by the addition of a
etext:_2PLANE or etext:_3PLANE suffix.
Similarly, the separate aspects of depth-stencil formats are separated by
underscores, although these are not considered separate planes.
Formats are suffixed by etext:_422 to indicate that planes other than the
first are reduced in size by a factor of two horizontally or that the R and
B values appear at half the horizontal frequency of the G values, etext:_420
to indicate that planes other than the first are reduced in size by a factor
of two both horizontally and vertically, and etext:_444 for consistency to
indicate that all three planes of a three-planar image are the same size.

[NOTE]
.Note
====
No common format has a single plane containing both R and B channels but
does not store these channels at reduced horizontal resolution.
====
endif::VK_VERSION_1_1,VK_KHR_sampler_ycbcr_conversion[]


[[texel-block-size]]
=== Representation and Texel Block Size

Color formats must: be represented in memory in exactly the form indicated
by the format's name.
This means that promoting one format to another with more bits per component
and/or additional components must: not occur for color formats.
Depth/stencil formats have more relaxed requirements as discussed
<<formats-depth-stencil,below>>.

Each format has a _texel block size_, the number of bytes used to store one
_texel block_ (a single addressable element of an uncompressed image, or a
single compressed block of a compressed image).
The texel block size for each format is shown in the
<<formats-compatibility, Compatible formats>> table.

The representation of non-packed formats is that the first component
specified in the name of the format is in the lowest memory addresses and
the last component specified is in the highest memory addresses.
See <<formats-non-packed,Byte mappings for non-packed/compressed color
formats>>.
The in-memory ordering of bytes within a component is determined by the host
endianness.

[[formats-non-packed]]
.Byte mappings for non-packed/compressed color formats
[options="header",cols="16*1,10",width="100%"]
|====
>|0 >|1 >|2 >|3 >|4 >|5 >|6 >|7 >|8 >|9 >|10 >|11 >|12 >|13 >|14 >|15 ^| {leftarrow} Byte
^|R 16+>s|etext:VK_FORMAT_R8_*
^|R ^|G 15+>s|etext:VK_FORMAT_R8G8_*
^|R ^|G ^|B 14+>s|etext:VK_FORMAT_R8G8B8_*
^|B ^|G ^|R 14+>s|etext:VK_FORMAT_B8G8R8_*
^|R ^|G ^|B ^|A 13+>s|etext:VK_FORMAT_R8G8B8A8_*
^|B ^|G ^|R ^|A 13+>s|etext:VK_FORMAT_B8G8R8A8_*
ifdef::VK_VERSION_1_1,VK_KHR_sampler_ycbcr_conversion[]
^|G~0~ ^|B ^|G~1~ ^|R 13+>s|ename:VK_FORMAT_G8B8G8R8_422_UNORM
^|B ^|G~0~ ^|R ^|G~1~ 13+>s|ename:VK_FORMAT_B8G8R8G8_422_UNORM
endif::VK_VERSION_1_1,VK_KHR_sampler_ycbcr_conversion[]
2+^|R 15+>s|etext:VK_FORMAT_R16_*
2+^|R 2+^|G 13+>s|etext:VK_FORMAT_R16G16_*
2+^|R 2+^|G 2+^|B 11+>s|etext:VK_FORMAT_R16G16B16_*
2+^|R 2+^|G 2+^|B 2+^|A 9+>s|etext:VK_FORMAT_R16G16B16A16_*
ifdef::VK_VERSION_1_1,VK_KHR_sampler_ycbcr_conversion[]
2+^|G~0~ 2+^|B 2+^|G~1~ 2+^|R 9+>s|etext:VK_FORMAT_G10X6B10X6G10X6R10X6_4PACK16_422_UNORM
etext:VK_FORMAT_G12X4B12X4G12X4R12X4_4PACK16_422_UNORM
etext:VK_FORMAT_G16B16G16R16_UNORM
2+^|B 2+^|G~0~ 2+^|R 2+^|G~1~ 9+>s|etext:VK_FORMAT_B10X6G10X6R10X6G10X6_4PACK16_422_UNORM
etext:VK_FORMAT_B12X4G12X4R12X4G12X4_4PACK16_422_UNORM
ename:VK_FORMAT_B16G16R16G16_422_UNORM
endif::VK_VERSION_1_1,VK_KHR_sampler_ycbcr_conversion[]
4+^|R 13+>s|etext:VK_FORMAT_R32_*
4+^|R 4+^|G 9+>s|etext:VK_FORMAT_R32G32_*
4+^|R 4+^|G 4+^|B 5+>s|etext:VK_FORMAT_R32G32B32_*
4+^|R 4+^|G 4+^|B 4+^|A >s|etext:VK_FORMAT_R32G32B32A32_*
8+^|R 9+>s|etext:VK_FORMAT_R64_*
8+^|R 8+^|G >s|etext:VK_FORMAT_R64G64_*
17+^s|etext:VK_FORMAT_R64G64B64_* as etext:VK_FORMAT_R64G64_* but with B in bytes 16-23
17+^s|etext:VK_FORMAT_R64G64B64A64_* as etext:VK_FORMAT_R64G64B64_* but with A in bytes 24-31
|====

Packed formats store multiple components within one underlying type.
The bit representation is that the first component specified in the name of
the format is in the most-significant bits and the last component specified
is in the least-significant bits of the underlying type.
The in-memory ordering of bytes comprising the underlying type is determined
by the host endianness.

[[formats-packed-8-bit]]
.Bit mappings for packed 8-bit formats
[options="header",cols="8*1",width="100%"]
|====
8+^h| Bit
>|~7~ >|~6~ >|~5~ >|~4~ >|~3~ >|~2~ >|~1~ >|~0~
8+^h| ename:VK_FORMAT_R4G4_UNORM_PACK8
4+^s|R 4+^s|G
^| ~3~ ^| ~2~ ^| ~1~ ^| ~0~
^| ~3~ ^| ~2~ ^| ~1~ ^| ~0~
|====

[[formats-packed-16-bit]]
.Bit mappings for packed 16-bit formats
[options="header",cols="16*1",width="100%"]
|====
16+^h| Bit
>|~15~ >|~14~ >|~13~ >|~12~ >|~11~ >|~10~ >|~9~ >|~8~ >|~7~ >|~6~ >|~5~ >|~4~ >|~3~ >|~2~ >|~1~ >|~0~
16+^h|ename:VK_FORMAT_R4G4B4A4_UNORM_PACK16
4+^s|R 4+^s|G 4+^s|B 4+^s|A
^| ~3~ ^| ~2~ ^| ~1~ ^| ~0~
^| ~3~ ^| ~2~ ^| ~1~ ^| ~0~
^| ~3~ ^| ~2~ ^| ~1~ ^| ~0~
^| ~3~ ^| ~2~ ^| ~1~ ^| ~0~
16+^h|ename:VK_FORMAT_B4G4R4A4_UNORM_PACK16
4+^s|B 4+^s|G 4+^s|R 4+^s|A
^| ~3~ ^| ~2~ ^| ~1~ ^| ~0~
^| ~3~ ^| ~2~ ^| ~1~ ^| ~0~
^| ~3~ ^| ~2~ ^| ~1~ ^| ~0~
^| ~3~ ^| ~2~ ^| ~1~ ^| ~0~
ifdef::VK_EXT_4444_formats[]
16+^h|ename:VK_FORMAT_A4R4G4B4_UNORM_PACK16_EXT
4+^s|A 4+^s|R 4+^s|G 4+^s|B
^| ~3~ ^| ~2~ ^| ~1~ ^| ~0~
^| ~3~ ^| ~2~ ^| ~1~ ^| ~0~
^| ~3~ ^| ~2~ ^| ~1~ ^| ~0~
^| ~3~ ^| ~2~ ^| ~1~ ^| ~0~
16+^h|ename:VK_FORMAT_A4B4G4R4_UNORM_PACK16_EXT
4+^s|A 4+^s|B 4+^s|G 4+^s|R
^| ~3~ ^| ~2~ ^| ~1~ ^| ~0~
^| ~3~ ^| ~2~ ^| ~1~ ^| ~0~
^| ~3~ ^| ~2~ ^| ~1~ ^| ~0~
^| ~3~ ^| ~2~ ^| ~1~ ^| ~0~
endif::VK_EXT_4444_formats[]
16+^h|ename:VK_FORMAT_R5G6B5_UNORM_PACK16
5+^s|R 6+^s|G 5+^s|B
^| ~4~ ^| ~3~ ^| ~2~ ^| ~1~ ^| ~0~
^| ~5~ ^| ~4~ ^| ~3~ ^| ~2~ ^| ~1~ ^| ~0~
^| ~4~ ^| ~3~ ^| ~2~ ^| ~1~ ^| ~0~
16+^h|ename:VK_FORMAT_B5G6R5_UNORM_PACK16
5+^s|B 6+^s|G 5+^s|R
^| ~4~ ^| ~3~ ^| ~2~ ^| ~1~ ^| ~0~
^| ~5~ ^| ~4~ ^| ~3~ ^| ~2~ ^| ~1~ ^| ~0~
^| ~4~ ^| ~3~ ^| ~2~ ^| ~1~ ^| ~0~
16+^h|ename:VK_FORMAT_R5G5B5A1_UNORM_PACK16
5+^s|R 5+^s|G 5+^s|B 1+^s|A
^| ~4~ ^| ~3~ ^| ~2~ ^| ~1~ ^| ~0~
^| ~4~ ^| ~3~ ^| ~2~ ^| ~1~ ^| ~0~
^| ~4~ ^| ~3~ ^| ~2~ ^| ~1~ ^| ~0~
^| ~0~
16+^h|ename:VK_FORMAT_B5G5R5A1_UNORM_PACK16
5+^s|B 5+^s|G 5+^s|R 1+^s|A
^| ~4~ ^| ~3~ ^| ~2~ ^| ~1~ ^| ~0~
^| ~4~ ^| ~3~ ^| ~2~ ^| ~1~ ^| ~0~
^| ~4~ ^| ~3~ ^| ~2~ ^| ~1~ ^| ~0~
^| ~0~
16+^h|ename:VK_FORMAT_A1R5G5B5_UNORM_PACK16
1+^s|A 5+^s|R 5+^s|G 5+^s|B
^| ~0~
^| ~4~ ^| ~3~ ^| ~2~ ^| ~1~ ^| ~0~
^| ~4~ ^| ~3~ ^| ~2~ ^| ~1~ ^| ~0~
^| ~4~ ^| ~3~ ^| ~2~ ^| ~1~ ^| ~0~
ifdef::VK_VERSION_1_1,VK_KHR_sampler_ycbcr_conversion[]
16+^h|ename:VK_FORMAT_R10X6_UNORM_PACK16
10+^s|R 6+^s|X
^| ~9~ ^| ~8~ ^| ~7~ ^| ~6~ ^| ~5~
^| ~4~ ^| ~3~ ^| ~2~ ^| ~1~ ^| ~0~
^| ~5~ ^| ~4~ ^| ~3~ ^| ~2~ ^| ~1~ ^| ~0~
16+^h|ename:VK_FORMAT_R12X4_UNORM_PACK16
12+^s|R 4+^s|X
^| ~11~ ^| ~10~
^| ~9~ ^| ~8~ ^| ~7~ ^| ~6~ ^| ~5~
^| ~4~ ^| ~3~ ^| ~2~ ^| ~1~ ^| ~0~
^| ~3~ ^| ~2~ ^| ~1~ ^| ~0~
endif::VK_VERSION_1_1,VK_KHR_sampler_ycbcr_conversion[]
|====

[[formats-packed-32-bit]]
.Bit mappings for packed 32-bit formats
[cols="32*1",options="header"]
|====
32+^h|Bit
>|~31~ >|~30~ >|~29~ >|~28~ >|~27~ >|~26~ >|~25~ >|~24~ >|~23~ >|~22~ >|~21~ >|~20~ >|~19~ >|~18~ >|~17~ >|~16~
>|~15~ >|~14~ >|~13~ >|~12~ >|~11~ >|~10~ >|~9~ >|~8~ >|~7~ >|~6~ >|~5~ >|~4~ >|~3~ >|~2~ >|~1~ >|~0~
32+^h|etext:VK_FORMAT_A8B8G8R8_*_PACK32
8+^s|A 8+^s|B 8+^s|G 8+^s|R
^|~7~ ^|~6~ ^|~5~ ^|~4~
^|~3~ ^|~2~ ^|~1~ ^|~0~
^|~7~ ^|~6~ ^|~5~ ^|~4~
^|~3~ ^|~2~ ^|~1~ ^|~0~
^|~7~ ^|~6~ ^|~5~ ^|~4~
^|~3~ ^|~2~ ^|~1~ ^|~0~
^|~7~ ^|~6~ ^|~5~ ^|~4~
^|~3~ ^|~2~ ^|~1~ ^|~0~
32+^h|etext:VK_FORMAT_A2R10G10B10_*_PACK32
2+^s|A 10+^s|R 10+^s|G 10+^s|B
^|~1~ ^|~0~
^|~9~ ^|~8~ ^|~7~ ^|~6~ ^|~5~
^|~4~ ^|~3~ ^|~2~ ^|~1~ ^|~0~
^|~9~ ^|~8~ ^|~7~ ^|~6~ ^|~5~
^|~4~ ^|~3~ ^|~2~ ^|~1~ ^|~0~
^|~9~ ^|~8~ ^|~7~ ^|~6~ ^|~5~
^|~4~ ^|~3~ ^|~2~ ^|~1~ ^|~0~
32+^h|etext:VK_FORMAT_A2B10G10R10_*_PACK32
2+^s|A 10+^s|B 10+^s|G 10+^s|R
^|~1~ ^|~0~
^|~9~ ^|~8~ ^|~7~ ^|~6~ ^|~5~
^|~4~ ^|~3~ ^|~2~ ^|~1~ ^|~0~
^|~9~ ^|~8~ ^|~7~ ^|~6~ ^|~5~
^|~4~ ^|~3~ ^|~2~ ^|~1~ ^|~0~
^|~9~ ^|~8~ ^|~7~ ^|~6~ ^|~5~
^|~4~ ^|~3~ ^|~2~ ^|~1~ ^|~0~
32+^h|ename:VK_FORMAT_B10G11R11_UFLOAT_PACK32
10+^s|B 11+^s|G 11+^s|R
^|~9~ ^|~8~ ^|~7~ ^|~6~ ^|~5~
^|~4~ ^|~3~ ^|~2~ ^|~1~ ^|~0~
^|~10~ ^|~9~ ^|~8~ ^|~7~ ^|~6~ ^|~5~
^|~4~ ^|~3~ ^|~2~ ^|~1~ ^|~0~
^|~10~ ^|~9~ ^|~8~ ^|~7~ ^|~6~ ^|~5~
^|~4~ ^|~3~ ^|~2~ ^|~1~ ^|~0~
32+^h|ename:VK_FORMAT_E5B9G9R9_UFLOAT_PACK32
5+^s|E 9+^s|B 9+^s|G 9+^s|R
^|~4~ ^|~3~ ^|~2~ ^|~1~ ^|~0~
^|~8~ ^|~7~ ^|~6~ ^|~5~
^|~4~ ^|~3~ ^|~2~ ^|~1~ ^|~0~
^|~8~ ^|~7~ ^|~6~ ^|~5~
^|~4~ ^|~3~ ^|~2~ ^|~1~ ^|~0~
^|~8~ ^|~7~ ^|~6~ ^|~5~
^|~4~ ^|~3~ ^|~2~ ^|~1~ ^|~0~
32+^h|ename:VK_FORMAT_X8_D24_UNORM_PACK32
8+^s|X 24+^s|D
^|~7~ ^|~6~ ^|~5~ ^|~4~
^|~3~ ^|~2~ ^|~1~ ^|~0~
^|~23~ ^|~22~ ^|~21~ ^|~20~
^|~19~ ^|~18~ ^|~17~ ^|~16~
^|~15~ ^|~14~ ^|~13~ ^|~12~
^|~11~ ^|~10~ ^|~9~ ^|~8~
^|~7~ ^|~6~ ^|~5~ ^|~4~
^|~3~ ^|~2~ ^|~1~ ^|~0~
|====


[[formats-depth-stencil]]
=== Depth/Stencil Formats

Depth/stencil formats are considered opaque and need not be stored in the
exact number of bits per texel or component ordering indicated by the format
enum.
However, implementations must: not substitute a different depth or stencil
precision than that described in the format (e.g. D16 must: not be
implemented as D24 or D32).


[[formats-compatibility-classes]]
=== Format Compatibility Classes

Uncompressed color formats are _compatible_ with each other if they occupy
the same number of bits per texel block.
Compressed color formats are compatible with each other if the only
difference between them is the numerical type of the uncompressed pixels
(e.g. signed vs. unsigned, or SRGB vs. UNORM encoding).
Each depth/stencil format is only compatible with itself.
In the <<formats-compatibility,following>> table, all the formats in the
same row are compatible.


[[formats-compatibility]]
.Compatible Formats
[width="90%",cols="4,10",options="header"]
|====
| Class, Texel Block Size, # Texels/Block | Formats
| 8-bit +
  Block size 1 byte +
  1 texel/block
                  | ename:VK_FORMAT_R4G4_UNORM_PACK8, +
                    ename:VK_FORMAT_R8_UNORM, +
                    ename:VK_FORMAT_R8_SNORM, +
                    ename:VK_FORMAT_R8_USCALED, +
                    ename:VK_FORMAT_R8_SSCALED, +
                    ename:VK_FORMAT_R8_UINT, +
                    ename:VK_FORMAT_R8_SINT, +
                    ename:VK_FORMAT_R8_SRGB
| 16-bit +
  Block size 2 bytes +
  1 texel/block
                  | ename:VK_FORMAT_R4G4B4A4_UNORM_PACK16, +
                    ename:VK_FORMAT_B4G4R4A4_UNORM_PACK16, +
ifdef::VK_EXT_4444_formats[]
                    ename:VK_FORMAT_A4R4G4B4_UNORM_PACK16_EXT, +
                    ename:VK_FORMAT_A4B4G4R4_UNORM_PACK16_EXT, +
endif::VK_EXT_4444_formats[]
                    ename:VK_FORMAT_R5G6B5_UNORM_PACK16, +
                    ename:VK_FORMAT_B5G6R5_UNORM_PACK16, +
                    ename:VK_FORMAT_R5G5B5A1_UNORM_PACK16, +
                    ename:VK_FORMAT_B5G5R5A1_UNORM_PACK16, +
                    ename:VK_FORMAT_A1R5G5B5_UNORM_PACK16, +
                    ename:VK_FORMAT_R8G8_UNORM, +
                    ename:VK_FORMAT_R8G8_SNORM, +
                    ename:VK_FORMAT_R8G8_USCALED, +
                    ename:VK_FORMAT_R8G8_SSCALED, +
                    ename:VK_FORMAT_R8G8_UINT, +
                    ename:VK_FORMAT_R8G8_SINT, +
                    ename:VK_FORMAT_R8G8_SRGB, +
                    ename:VK_FORMAT_R16_UNORM, +
                    ename:VK_FORMAT_R16_SNORM, +
                    ename:VK_FORMAT_R16_USCALED, +
                    ename:VK_FORMAT_R16_SSCALED, +
                    ename:VK_FORMAT_R16_UINT, +
                    ename:VK_FORMAT_R16_SINT, +
ifndef::VK_VERSION_1_1,VK_KHR_sampler_ycbcr_conversion[]
                    ename:VK_FORMAT_R16_SFLOAT
endif::VK_VERSION_1_1,VK_KHR_sampler_ycbcr_conversion[]
ifdef::VK_VERSION_1_1,VK_KHR_sampler_ycbcr_conversion[]
                    ename:VK_FORMAT_R16_SFLOAT, +
                    ename:VK_FORMAT_R10X6_UNORM_PACK16, +
                    ename:VK_FORMAT_R12X4_UNORM_PACK16
endif::VK_VERSION_1_1,VK_KHR_sampler_ycbcr_conversion[]
| 24-bit +
  Block size 3 bytes +
  1 texel/block
                  | ename:VK_FORMAT_R8G8B8_UNORM, +
                    ename:VK_FORMAT_R8G8B8_SNORM, +
                    ename:VK_FORMAT_R8G8B8_USCALED, +
                    ename:VK_FORMAT_R8G8B8_SSCALED, +
                    ename:VK_FORMAT_R8G8B8_UINT, +
                    ename:VK_FORMAT_R8G8B8_SINT, +
                    ename:VK_FORMAT_R8G8B8_SRGB, +
                    ename:VK_FORMAT_B8G8R8_UNORM, +
                    ename:VK_FORMAT_B8G8R8_SNORM, +
                    ename:VK_FORMAT_B8G8R8_USCALED, +
                    ename:VK_FORMAT_B8G8R8_SSCALED, +
                    ename:VK_FORMAT_B8G8R8_UINT, +
                    ename:VK_FORMAT_B8G8R8_SINT, +
                    ename:VK_FORMAT_B8G8R8_SRGB
| 32-bit +
  Block size 4 bytes +
  1 texel/block
                  | ename:VK_FORMAT_R8G8B8A8_UNORM, +
                    ename:VK_FORMAT_R8G8B8A8_SNORM, +
                    ename:VK_FORMAT_R8G8B8A8_USCALED, +
                    ename:VK_FORMAT_R8G8B8A8_SSCALED, +
                    ename:VK_FORMAT_R8G8B8A8_UINT, +
                    ename:VK_FORMAT_R8G8B8A8_SINT, +
                    ename:VK_FORMAT_R8G8B8A8_SRGB, +
                    ename:VK_FORMAT_B8G8R8A8_UNORM, +
                    ename:VK_FORMAT_B8G8R8A8_SNORM, +
                    ename:VK_FORMAT_B8G8R8A8_USCALED, +
                    ename:VK_FORMAT_B8G8R8A8_SSCALED, +
                    ename:VK_FORMAT_B8G8R8A8_UINT, +
                    ename:VK_FORMAT_B8G8R8A8_SINT, +
                    ename:VK_FORMAT_B8G8R8A8_SRGB, +
                    ename:VK_FORMAT_A8B8G8R8_UNORM_PACK32, +
                    ename:VK_FORMAT_A8B8G8R8_SNORM_PACK32, +
                    ename:VK_FORMAT_A8B8G8R8_USCALED_PACK32, +
                    ename:VK_FORMAT_A8B8G8R8_SSCALED_PACK32, +
                    ename:VK_FORMAT_A8B8G8R8_UINT_PACK32, +
                    ename:VK_FORMAT_A8B8G8R8_SINT_PACK32, +
                    ename:VK_FORMAT_A8B8G8R8_SRGB_PACK32, +
                    ename:VK_FORMAT_A2R10G10B10_UNORM_PACK32, +
                    ename:VK_FORMAT_A2R10G10B10_SNORM_PACK32, +
                    ename:VK_FORMAT_A2R10G10B10_USCALED_PACK32, +
                    ename:VK_FORMAT_A2R10G10B10_SSCALED_PACK32, +
                    ename:VK_FORMAT_A2R10G10B10_UINT_PACK32, +
                    ename:VK_FORMAT_A2R10G10B10_SINT_PACK32, +
                    ename:VK_FORMAT_A2B10G10R10_UNORM_PACK32, +
                    ename:VK_FORMAT_A2B10G10R10_SNORM_PACK32, +
                    ename:VK_FORMAT_A2B10G10R10_USCALED_PACK32, +
                    ename:VK_FORMAT_A2B10G10R10_SSCALED_PACK32, +
                    ename:VK_FORMAT_A2B10G10R10_UINT_PACK32, +
                    ename:VK_FORMAT_A2B10G10R10_SINT_PACK32, +
                    ename:VK_FORMAT_R16G16_UNORM, +
                    ename:VK_FORMAT_R16G16_SNORM, +
                    ename:VK_FORMAT_R16G16_USCALED, +
                    ename:VK_FORMAT_R16G16_SSCALED, +
                    ename:VK_FORMAT_R16G16_UINT, +
                    ename:VK_FORMAT_R16G16_SINT, +
                    ename:VK_FORMAT_R16G16_SFLOAT, +
                    ename:VK_FORMAT_R32_UINT, +
                    ename:VK_FORMAT_R32_SINT, +
                    ename:VK_FORMAT_R32_SFLOAT, +
                    ename:VK_FORMAT_B10G11R11_UFLOAT_PACK32, +
ifndef::VK_VERSION_1_1,VK_KHR_sampler_ycbcr_conversion[]
                    ename:VK_FORMAT_E5B9G9R9_UFLOAT_PACK32
endif::VK_VERSION_1_1,VK_KHR_sampler_ycbcr_conversion[]
ifdef::VK_VERSION_1_1,VK_KHR_sampler_ycbcr_conversion[]
                    ename:VK_FORMAT_E5B9G9R9_UFLOAT_PACK32, +
                    ename:VK_FORMAT_R10X6G10X6_UNORM_2PACK16, +
                    ename:VK_FORMAT_R12X4G12X4_UNORM_2PACK16
| 32-bit G8B8G8R8 +
  Block size 4 bytes +
  1 texel/block
                  | ename:VK_FORMAT_G8B8G8R8_422_UNORM
| 32-bit B8G8R8G8 +
  Block size 4 bytes +
  1 texel/block
                  | ename:VK_FORMAT_B8G8R8G8_422_UNORM
endif::VK_VERSION_1_1,VK_KHR_sampler_ycbcr_conversion[]
| 48-bit +
  Block size 6 bytes +
  1 texel/block
                  | ename:VK_FORMAT_R16G16B16_UNORM, +
                    ename:VK_FORMAT_R16G16B16_SNORM, +
                    ename:VK_FORMAT_R16G16B16_USCALED, +
                    ename:VK_FORMAT_R16G16B16_SSCALED, +
                    ename:VK_FORMAT_R16G16B16_UINT, +
                    ename:VK_FORMAT_R16G16B16_SINT, +
                    ename:VK_FORMAT_R16G16B16_SFLOAT
| 64-bit +
  Block size 8 bytes +
  1 texel/block
                  | ename:VK_FORMAT_R16G16B16A16_UNORM, +
                    ename:VK_FORMAT_R16G16B16A16_SNORM, +
                    ename:VK_FORMAT_R16G16B16A16_USCALED, +
                    ename:VK_FORMAT_R16G16B16A16_SSCALED, +
                    ename:VK_FORMAT_R16G16B16A16_UINT, +
                    ename:VK_FORMAT_R16G16B16A16_SINT, +
                    ename:VK_FORMAT_R16G16B16A16_SFLOAT, +
                    ename:VK_FORMAT_R32G32_UINT, +
                    ename:VK_FORMAT_R32G32_SINT, +
                    ename:VK_FORMAT_R32G32_SFLOAT, +
                    ename:VK_FORMAT_R64_UINT, +
                    ename:VK_FORMAT_R64_SINT, +
                    ename:VK_FORMAT_R64_SFLOAT
ifdef::VK_VERSION_1_1,VK_KHR_sampler_ycbcr_conversion[]
| 64-bit R10G10B10A10 +
  Block size 8 bytes +
  1 texel/block
                  | ename:VK_FORMAT_R10X6G10X6B10X6A10X6_UNORM_4PACK16
| 64-bit G10B10G10R10 +
  Block size 8 bytes +
  1 texel/block
                  | ename:VK_FORMAT_G10X6B10X6G10X6R10X6_422_UNORM_4PACK16
| 64-bit B10G10R10G10 +
  Block size 8 bytes +
  1 texel/block
                  | ename:VK_FORMAT_B10X6G10X6R10X6G10X6_422_UNORM_4PACK16
| 64-bit R12G12B12A12 +
  Block size 8 bytes +
  1 texel/block
                  | ename:VK_FORMAT_R12X4G12X4B12X4A12X4_UNORM_4PACK16
| 64-bit G12B12G12R12 +
  Block size 8 bytes +
  1 texel/block
                  | ename:VK_FORMAT_G12X4B12X4G12X4R12X4_422_UNORM_4PACK16
| 64-bit B12G12R12G12 +
  Block size 8 bytes +
  1 texel/block
                  | ename:VK_FORMAT_B12X4G12X4R12X4G12X4_422_UNORM_4PACK16
| 64-bit G16B16G16R16 +
  Block size 8 bytes +
  1 texel/block
                  | ename:VK_FORMAT_G16B16G16R16_422_UNORM
| 64-bit B16G16R16G16 +
  Block size 8 bytes +
  1 texel/block
                  | ename:VK_FORMAT_B16G16R16G16_422_UNORM
endif::VK_VERSION_1_1,VK_KHR_sampler_ycbcr_conversion[]
| 96-bit +
  Block size 12 bytes +
  1 texel/block
                  | ename:VK_FORMAT_R32G32B32_UINT, +
                    ename:VK_FORMAT_R32G32B32_SINT, +
                    ename:VK_FORMAT_R32G32B32_SFLOAT
| 128-bit +
  Block size 16 bytes +
  1 texel/block
                  | ename:VK_FORMAT_R32G32B32A32_UINT, +
                    ename:VK_FORMAT_R32G32B32A32_SINT, +
                    ename:VK_FORMAT_R32G32B32A32_SFLOAT, +
                    ename:VK_FORMAT_R64G64_UINT, +
                    ename:VK_FORMAT_R64G64_SINT, +
                    ename:VK_FORMAT_R64G64_SFLOAT
| 192-bit +
  Block size 24 bytes +
  1 texel/block
                  | ename:VK_FORMAT_R64G64B64_UINT, +
                    ename:VK_FORMAT_R64G64B64_SINT, +
                    ename:VK_FORMAT_R64G64B64_SFLOAT
| 256-bit +
  Block size 32 bytes +
  1 texel/block
                  | ename:VK_FORMAT_R64G64B64A64_UINT, +
                    ename:VK_FORMAT_R64G64B64A64_SINT, +
                    ename:VK_FORMAT_R64G64B64A64_SFLOAT
| BC1_RGB (64 bit) +
  Block size 8 bytes +
  16 texels/block
                  | ename:VK_FORMAT_BC1_RGB_UNORM_BLOCK, +
                    ename:VK_FORMAT_BC1_RGB_SRGB_BLOCK
| BC1_RGBA (64 bit) +
  Block size 8 bytes +
  16 texels/block
                  | ename:VK_FORMAT_BC1_RGBA_UNORM_BLOCK, +
                    ename:VK_FORMAT_BC1_RGBA_SRGB_BLOCK
| BC2 (128 bit) +
  Block size 16 bytes +
  16 texels/block
                  | ename:VK_FORMAT_BC2_UNORM_BLOCK, +
                    ename:VK_FORMAT_BC2_SRGB_BLOCK
| BC3 (128 bit) +
  Block size 16 bytes +
  16 texels/block
                  | ename:VK_FORMAT_BC3_UNORM_BLOCK, +
                    ename:VK_FORMAT_BC3_SRGB_BLOCK
| BC4 (64 bit) +
  Block size 8 bytes +
  16 texels/block
                  | ename:VK_FORMAT_BC4_UNORM_BLOCK, +
                    ename:VK_FORMAT_BC4_SNORM_BLOCK
| BC5 (128 bit) +
  Block size 16 bytes +
  16 texels/block
                  | ename:VK_FORMAT_BC5_UNORM_BLOCK, +
                    ename:VK_FORMAT_BC5_SNORM_BLOCK
| BC6H (128 bit) +
  Block size 16 bytes +
  16 texels/block
                  | ename:VK_FORMAT_BC6H_UFLOAT_BLOCK, +
                    ename:VK_FORMAT_BC6H_SFLOAT_BLOCK
| BC7 (128 bit) +
  Block size 16 bytes +
  16 texels/block
                  | ename:VK_FORMAT_BC7_UNORM_BLOCK, +
                    ename:VK_FORMAT_BC7_SRGB_BLOCK
| ETC2_RGB (64 bit) +
  Block size 8 bytes +
  16 texels/block
                  | ename:VK_FORMAT_ETC2_R8G8B8_UNORM_BLOCK, +
                    ename:VK_FORMAT_ETC2_R8G8B8_SRGB_BLOCK
| ETC2_RGBA (64 bit) +
  Block size 8 bytes +
  16 texels/block
                  | ename:VK_FORMAT_ETC2_R8G8B8A1_UNORM_BLOCK, +
                    ename:VK_FORMAT_ETC2_R8G8B8A1_SRGB_BLOCK
| ETC2_EAC_RGBA (64 bit) +
  Block size 8 bytes +
  16 texels/block
                  | ename:VK_FORMAT_ETC2_R8G8B8A8_UNORM_BLOCK, +
                    ename:VK_FORMAT_ETC2_R8G8B8A8_SRGB_BLOCK
| EAC_R (64 bit) +
  Block size 8 bytes +
  16 texels/block
                  | ename:VK_FORMAT_EAC_R11_UNORM_BLOCK, +
                    ename:VK_FORMAT_EAC_R11_SNORM_BLOCK
| EAC_RG (128 bit) +
  Block size 16 bytes +
  16 texels/block
                  | ename:VK_FORMAT_EAC_R11G11_UNORM_BLOCK, +
                    ename:VK_FORMAT_EAC_R11G11_SNORM_BLOCK
| ASTC_4x4 (128 bit) +
  Block size 16 bytes +
  16 texels/block
                  | ename:VK_FORMAT_ASTC_4x4_UNORM_BLOCK, +
ifdef::VK_EXT_texture_compression_astc_hdr[]
                    ename:VK_FORMAT_ASTC_4x4_SFLOAT_BLOCK_EXT, +
endif::VK_EXT_texture_compression_astc_hdr[]
                    ename:VK_FORMAT_ASTC_4x4_SRGB_BLOCK
| ASTC_5x4 (128 bit) +
  Block size 16 bytes +
  20 texels/block
                  | ename:VK_FORMAT_ASTC_5x4_UNORM_BLOCK, +
ifdef::VK_EXT_texture_compression_astc_hdr[]
                    ename:VK_FORMAT_ASTC_5x4_SFLOAT_BLOCK_EXT, +
endif::VK_EXT_texture_compression_astc_hdr[]
                    ename:VK_FORMAT_ASTC_5x4_SRGB_BLOCK
| ASTC_5x5 (128 bit) +
  Block size 16 bytes +
  25 texels/block
                  | ename:VK_FORMAT_ASTC_5x5_UNORM_BLOCK, +
ifdef::VK_EXT_texture_compression_astc_hdr[]
                    ename:VK_FORMAT_ASTC_5x5_SFLOAT_BLOCK_EXT, +
endif::VK_EXT_texture_compression_astc_hdr[]
                    ename:VK_FORMAT_ASTC_5x5_SRGB_BLOCK
| ASTC_6x5 (128 bit) +
  Block size 16 bytes +
  30 texels/block
                  | ename:VK_FORMAT_ASTC_6x5_UNORM_BLOCK, +
ifdef::VK_EXT_texture_compression_astc_hdr[]
                    ename:VK_FORMAT_ASTC_6x5_SFLOAT_BLOCK_EXT, +
endif::VK_EXT_texture_compression_astc_hdr[]
                    ename:VK_FORMAT_ASTC_6x5_SRGB_BLOCK
| ASTC_6x6 (128 bit) +
  Block size 16 bytes +
  36 texels/block
                  | ename:VK_FORMAT_ASTC_6x6_UNORM_BLOCK, +
ifdef::VK_EXT_texture_compression_astc_hdr[]
                    ename:VK_FORMAT_ASTC_6x6_SFLOAT_BLOCK_EXT, +
endif::VK_EXT_texture_compression_astc_hdr[]
                    ename:VK_FORMAT_ASTC_6x6_SRGB_BLOCK
| ASTC_8x5 (128 bit) +
  Block size 16 bytes +
  40 texels/block
                  | ename:VK_FORMAT_ASTC_8x5_UNORM_BLOCK, +
ifdef::VK_EXT_texture_compression_astc_hdr[]
                    ename:VK_FORMAT_ASTC_8x5_SFLOAT_BLOCK_EXT, +
endif::VK_EXT_texture_compression_astc_hdr[]
                    ename:VK_FORMAT_ASTC_8x5_SRGB_BLOCK
| ASTC_8x6 (128 bit) +
  Block size 16 bytes +
  48 texels/block
                  | ename:VK_FORMAT_ASTC_8x6_UNORM_BLOCK, +
ifdef::VK_EXT_texture_compression_astc_hdr[]
                    ename:VK_FORMAT_ASTC_8x6_SFLOAT_BLOCK_EXT, +
endif::VK_EXT_texture_compression_astc_hdr[]
                    ename:VK_FORMAT_ASTC_8x6_SRGB_BLOCK
| ASTC_8x8 (128 bit) +
  Block size 16 bytes +
  64 texels/block
                  | ename:VK_FORMAT_ASTC_8x8_UNORM_BLOCK, +
ifdef::VK_EXT_texture_compression_astc_hdr[]
                    ename:VK_FORMAT_ASTC_8x8_SFLOAT_BLOCK_EXT, +
endif::VK_EXT_texture_compression_astc_hdr[]
                    ename:VK_FORMAT_ASTC_8x8_SRGB_BLOCK
| ASTC_10x5 (128 bit) +
  Block size 16 bytes +
  50 texels/block
                  | ename:VK_FORMAT_ASTC_10x5_UNORM_BLOCK, +
ifdef::VK_EXT_texture_compression_astc_hdr[]
                    ename:VK_FORMAT_ASTC_10x5_SFLOAT_BLOCK_EXT, +
endif::VK_EXT_texture_compression_astc_hdr[]
                    ename:VK_FORMAT_ASTC_10x5_SRGB_BLOCK
| ASTC_10x6 (128 bit) +
  Block size 16 bytes +
  60 texels/block
                  | ename:VK_FORMAT_ASTC_10x6_UNORM_BLOCK, +
ifdef::VK_EXT_texture_compression_astc_hdr[]
                    ename:VK_FORMAT_ASTC_10x6_SFLOAT_BLOCK_EXT, +
endif::VK_EXT_texture_compression_astc_hdr[]
                    ename:VK_FORMAT_ASTC_10x6_SRGB_BLOCK
| ASTC_10x8 (128 bit) +
  Block size 16 bytes +
  80 texels/block
                  | ename:VK_FORMAT_ASTC_10x8_UNORM_BLOCK, +
ifdef::VK_EXT_texture_compression_astc_hdr[]
                    ename:VK_FORMAT_ASTC_10x8_SFLOAT_BLOCK_EXT, +
endif::VK_EXT_texture_compression_astc_hdr[]
                    ename:VK_FORMAT_ASTC_10x8_SRGB_BLOCK
| ASTC_10x10 (128 bit) +
  Block size 16 bytes +
  100 texels/block
                  | ename:VK_FORMAT_ASTC_10x10_UNORM_BLOCK, +
ifdef::VK_EXT_texture_compression_astc_hdr[]
                    ename:VK_FORMAT_ASTC_10x10_SFLOAT_BLOCK_EXT, +
endif::VK_EXT_texture_compression_astc_hdr[]
                    ename:VK_FORMAT_ASTC_10x10_SRGB_BLOCK
| ASTC_12x10 (128 bit) +
  Block size 16 bytes +
  120 texels/block
                  | ename:VK_FORMAT_ASTC_12x10_UNORM_BLOCK, +
ifdef::VK_EXT_texture_compression_astc_hdr[]
                    ename:VK_FORMAT_ASTC_12x10_SFLOAT_BLOCK_EXT, +
endif::VK_EXT_texture_compression_astc_hdr[]
                    ename:VK_FORMAT_ASTC_12x10_SRGB_BLOCK
| ASTC_12x12 (128 bit) +
  Block size 16 bytes +
  144 texels/block
                  | ename:VK_FORMAT_ASTC_12x12_UNORM_BLOCK, +
ifdef::VK_EXT_texture_compression_astc_hdr[]
                    ename:VK_FORMAT_ASTC_12x12_SFLOAT_BLOCK_EXT, +
endif::VK_EXT_texture_compression_astc_hdr[]
                    ename:VK_FORMAT_ASTC_12x12_SRGB_BLOCK
| D16 (16 bit) +
  Block size 2 bytes +
  1 texel/block
                  | ename:VK_FORMAT_D16_UNORM
| D24 (32 bit) +
  Block size 4 bytes +
  1 texel/block
                  | ename:VK_FORMAT_X8_D24_UNORM_PACK32
| D32 (32 bit) +
  Block size 4 bytes +
  1 texel/block
                  | ename:VK_FORMAT_D32_SFLOAT
| S8 (8 bit) +
  Block size 1 byte +
  1 texel/block
                  | ename:VK_FORMAT_S8_UINT
| D16S8 (24 bit) +
  Block size 3 bytes +
  1 texel/block
                  | ename:VK_FORMAT_D16_UNORM_S8_UINT
| D24S8 (32 bit) +
  Block size 4 bytes +
  1 texel/block
                  | ename:VK_FORMAT_D24_UNORM_S8_UINT
| D32S8 (40 bit) +
  Block size 5 bytes +
  1 texel/block
                  | ename:VK_FORMAT_D32_SFLOAT_S8_UINT
ifdef::VK_VERSION_1_1,VK_KHR_sampler_ycbcr_conversion[]
| 8-bit 3-plane 420 +
  Block size (1,1,1) bytes +
  1 texel/block
                  | ename:VK_FORMAT_G8_B8_R8_3PLANE_420_UNORM
| 8-bit 2-plane 420 +
  Block size (1,2) bytes +
  1 texel/block
                  | ename:VK_FORMAT_G8_B8R8_2PLANE_420_UNORM
| 8-bit 3-plane 422 +
  Block size (1,1,1) bytes +
  1 texel/block
                  | ename:VK_FORMAT_G8_B8_R8_3PLANE_422_UNORM
| 8-bit 2-plane 422 +
  Block size (1,2) bytes +
  1 texel/block
                  | ename:VK_FORMAT_G8_B8R8_2PLANE_422_UNORM
| 8-bit 3-plane 444 +
  Block size (1,1,1) bytes +
  1 texel/block
                  | ename:VK_FORMAT_G8_B8_R8_3PLANE_444_UNORM
| 10-bit 3-plane 420 +
  Block size (2,2,2) bytes +
  1 texel/block
                  | ename:VK_FORMAT_G10X6_B10X6_R10X6_3PLANE_420_UNORM_3PACK16
| 10-bit 2-plane 420 +
  Block size (2,4) bytes +
  1 texel/block
                  | ename:VK_FORMAT_G10X6_B10X6R10X6_2PLANE_420_UNORM_3PACK16
| 10-bit 3-plane 422 +
  Block size (2,2,2) bytes +
  1 texel/block
                  | ename:VK_FORMAT_G10X6_B10X6_R10X6_3PLANE_422_UNORM_3PACK16
| 10-bit 2-plane 422 +
  Block size (2,2) bytes +
  1 texel/block
                  | ename:VK_FORMAT_G10X6_B10X6R10X6_2PLANE_422_UNORM_3PACK16
| 10-bit 3-plane 444 +
  Block size (2,2,2) bytes +
  1 texel/block
                  | ename:VK_FORMAT_G10X6_B10X6_R10X6_3PLANE_444_UNORM_3PACK16
| 12-bit 3-plane 420 +
  Block size (2,2,2) bytes +
  1 texel/block
                  | ename:VK_FORMAT_G12X4_B12X4_R12X4_3PLANE_420_UNORM_3PACK16
| 12-bit 2-plane 420 +
  Block size (2,4) bytes +
  1 texel/block
                  | ename:VK_FORMAT_G12X4_B12X4R12X4_2PLANE_420_UNORM_3PACK16
| 12-bit 3-plane 422 +
  Block size (2,2,2) bytes +
  1 texel/block
                  | ename:VK_FORMAT_G12X4_B12X4_R12X4_3PLANE_422_UNORM_3PACK16
| 12-bit 2-plane 422 +
  Block size (2,4) bytes +
  1 texel/block
                  | ename:VK_FORMAT_G12X4_B12X4R12X4_2PLANE_422_UNORM_3PACK16
| 12-bit 3-plane 444 +
  Block size (2,2,2) bytes +
  1 texel/block
                  | ename:VK_FORMAT_G12X4_B12X4_R12X4_3PLANE_444_UNORM_3PACK16
| 16-bit 3-plane 420 +
  Block size (2,2,2) bytes +
  1 texel/block
                  | ename:VK_FORMAT_G16_B16_R16_3PLANE_420_UNORM
| 16-bit 2-plane 420 +
  Block size (2,4) bytes +
  1 texel/block
                  | ename:VK_FORMAT_G16_B16R16_2PLANE_420_UNORM
| 16-bit 3-plane 422 +
  Block size (2,2,2) bytes +
  1 texel/block
                  | ename:VK_FORMAT_G16_B16_R16_3PLANE_422_UNORM
| 16-bit 2-plane 422 +
  Block size (2,4) bytes +
  1 texel/block
                  | ename:VK_FORMAT_G16_B16R16_2PLANE_422_UNORM
| 16-bit 3-plane 444 +
  Block size (2,2,2) bytes +
  1 texel/block
                  | ename:VK_FORMAT_G16_B16_R16_3PLANE_444_UNORM
ifdef::VK_EXT_ycbcr_2plane_444_formats[]
| 8-bit 2-plane 444 +
  Block size (1,2) bytes +
  1 texel/block
                  | ename:VK_FORMAT_G8_B8R8_2PLANE_444_UNORM_EXT
| 10-bit 2-plane 444 +
  Block size (2,4) bytes +
  1 texel/block
                  | ename:VK_FORMAT_G10X6_B10X6R10X6_2PLANE_444_UNORM_3PACK16_EXT
| 12-bit 2-plane 444 +
  Block size (2,4) bytes +
  1 texel/block
                  | ename:VK_FORMAT_G12X4_B12X4R12X4_2PLANE_444_UNORM_3PACK16_EXT
| 16-bit 2-plane 444 +
  Block size (2,4) bytes +
  1 texel/block
                  | ename:VK_FORMAT_G16_B16R16_2PLANE_444_UNORM_EXT
endif::VK_EXT_ycbcr_2plane_444_formats[]

endif::VK_VERSION_1_1,VK_KHR_sampler_ycbcr_conversion[]
|====


[[formats-properties]]
== Format Properties

[open,refpage='vkGetPhysicalDeviceFormatProperties',desc='Lists physical device\'s format capabilities',type='protos']
--
To query supported format features which are properties of the physical
device, call:

include::{generated}/api/protos/vkGetPhysicalDeviceFormatProperties.txt[]

  * pname:physicalDevice is the physical device from which to query the
    format properties.
  * pname:format is the format whose properties are queried.
  * pname:pFormatProperties is a pointer to a slink:VkFormatProperties
    structure in which physical device properties for pname:format are
    returned.

include::{generated}/validity/protos/vkGetPhysicalDeviceFormatProperties.txt[]
--

[open,refpage='VkFormatProperties',desc='Structure specifying image format properties',type='structs']
--
The sname:VkFormatProperties structure is defined as:

include::{generated}/api/structs/VkFormatProperties.txt[]

  * pname:linearTilingFeatures is a bitmask of elink:VkFormatFeatureFlagBits
    specifying features supported by images created with a pname:tiling
    parameter of ename:VK_IMAGE_TILING_LINEAR.
  * pname:optimalTilingFeatures is a bitmask of
    elink:VkFormatFeatureFlagBits specifying features supported by images
    created with a pname:tiling parameter of ename:VK_IMAGE_TILING_OPTIMAL.
  * pname:bufferFeatures is a bitmask of elink:VkFormatFeatureFlagBits
    specifying features supported by buffers.

[NOTE]
.Note
====
ifndef::VK_VERSION_1_1,VK_KHR_maintenance1[]
If no format feature flags are supported, then the only possible use would
be image transfers - which alone are not useful.
As such, if no format feature flags are supported, the format itself is not
supported, and images of that format cannot be created.
endif::VK_VERSION_1_1,VK_KHR_maintenance1[]
ifdef::VK_VERSION_1_1,VK_KHR_maintenance1[]
If no format feature flags are supported, the format itself is not
supported, and images of that format cannot be created.
endif::VK_VERSION_1_1,VK_KHR_maintenance1[]
====

If pname:format is a block-compressed format, then pname:bufferFeatures
must: not support any features for the format.

ifdef::VK_VERSION_1_1,VK_KHR_sampler_ycbcr_conversion[]
If pname:format is not a multi-plane format then pname:linearTilingFeatures
and pname:optimalTilingFeatures must: not contain
ename:VK_FORMAT_FEATURE_DISJOINT_BIT.
endif::VK_VERSION_1_1,VK_KHR_sampler_ycbcr_conversion[]

include::{generated}/validity/structs/VkFormatProperties.txt[]
--

[open,refpage='VkFormatFeatureFlagBits',desc='Bitmask specifying features supported by a buffer',type='enums']
--
Bits which can: be set in the slink:VkFormatProperties features
pname:linearTilingFeatures, pname:optimalTilingFeatures,
ifdef::VK_EXT_image_drm_format_modifier[]
slink:VkDrmFormatModifierPropertiesEXT::pname:drmFormatModifierTilingFeatures,
endif::VK_EXT_image_drm_format_modifier[]
and pname:bufferFeatures are:

include::{generated}/api/enums/VkFormatFeatureFlagBits.txt[]

The following bits may: be set in
ifndef::VK_EXT_image_drm_format_modifier[]
pname:linearTilingFeatures and pname:optimalTilingFeatures,
endif::VK_EXT_image_drm_format_modifier[]
ifdef::VK_EXT_image_drm_format_modifier[]
pname:linearTilingFeatures, pname:optimalTilingFeatures, and
slink:VkDrmFormatModifierPropertiesEXT::pname:drmFormatModifierTilingFeatures,
endif::VK_EXT_image_drm_format_modifier[]
specifying that the features are supported by <<VkImage,images>> or
<<VkImageView,image views>>
ifdef::VK_VERSION_1_1,VK_KHR_sampler_ycbcr_conversion[]
or <<VkSamplerYcbcrConversion,sampler {YCbCr} conversion objects>>
endif::VK_VERSION_1_1,VK_KHR_sampler_ycbcr_conversion[]
created with the queried
flink:vkGetPhysicalDeviceFormatProperties::pname:format:

  * ename:VK_FORMAT_FEATURE_SAMPLED_IMAGE_BIT specifies that an image view
    can: be <<descriptorsets-sampledimage, sampled from>>.
  * ename:VK_FORMAT_FEATURE_STORAGE_IMAGE_BIT specifies that an image view
    can: be used as a <<descriptorsets-storageimage, storage image>>.
  * ename:VK_FORMAT_FEATURE_STORAGE_IMAGE_ATOMIC_BIT specifies that an image
    view can: be used as storage image that supports atomic operations.
  * ename:VK_FORMAT_FEATURE_COLOR_ATTACHMENT_BIT specifies that an image
    view can: be used as a framebuffer color attachment and as an input
    attachment.
  * ename:VK_FORMAT_FEATURE_COLOR_ATTACHMENT_BLEND_BIT specifies that an
    image view can: be used as a framebuffer color attachment that supports
    blending and as an input attachment.
  * ename:VK_FORMAT_FEATURE_DEPTH_STENCIL_ATTACHMENT_BIT specifies that an
    image view can: be used as a framebuffer depth/stencil attachment and as
    an input attachment.
  * ename:VK_FORMAT_FEATURE_BLIT_SRC_BIT specifies that an image can: be
    used as pname:srcImage for the
ifndef::VK_KHR_copy_commands2[]
    fname:vkCmdBlitImage command.
endif::VK_KHR_copy_commands2[]
ifdef::VK_KHR_copy_commands2[]
    fname:vkCmdBlitImage2KHR and fname:vkCmdBlitImage commands.
endif::VK_KHR_copy_commands2[]
  * ename:VK_FORMAT_FEATURE_BLIT_DST_BIT specifies that an image can: be
    used as pname:dstImage for the
ifndef::VK_KHR_copy_commands2[]
    fname:vkCmdBlitImage command.
endif::VK_KHR_copy_commands2[]
ifdef::VK_KHR_copy_commands2[]
    fname:vkCmdBlitImage2KHR and fname:vkCmdBlitImage commands.
endif::VK_KHR_copy_commands2[]
  * ename:VK_FORMAT_FEATURE_SAMPLED_IMAGE_FILTER_LINEAR_BIT specifies that
    if ename:VK_FORMAT_FEATURE_SAMPLED_IMAGE_BIT is also set, an image view
    can: be used with a sampler that has either of pname:magFilter or
    pname:minFilter set to ename:VK_FILTER_LINEAR, or pname:mipmapMode set
    to ename:VK_SAMPLER_MIPMAP_MODE_LINEAR.
    If ename:VK_FORMAT_FEATURE_BLIT_SRC_BIT is also set, an image can be
    used as the pname:srcImage to
ifndef::VK_KHR_copy_commands2[]
    fname:vkCmdBlitImage
endif::VK_KHR_copy_commands2[]
ifdef::VK_KHR_copy_commands2[]
    fname:vkCmdBlitImage2KHR and fname:vkCmdBlitImage
endif::VK_KHR_copy_commands2[]
    with a pname:filter of ename:VK_FILTER_LINEAR.
    This bit must: only be exposed for formats that also support the
    ename:VK_FORMAT_FEATURE_SAMPLED_IMAGE_BIT or
    ename:VK_FORMAT_FEATURE_BLIT_SRC_BIT.
+
If the format being queried is a depth/stencil format, this bit only
specifies that the depth aspect (not the stencil aspect) of an image of this
format supports linear filtering, and that linear filtering of the depth
aspect is supported whether depth compare is enabled in the sampler or not.
If this bit is not present, linear filtering with depth compare disabled is
unsupported and linear filtering with depth compare enabled is supported,
but may: compute the filtered value in an implementation-dependent manner
which differs from the normal rules of linear filtering.
The resulting value must: be in the range [eq]#[0,1]# and should: be
proportional to, or a weighted average of, the number of comparison passes
or failures.

ifdef::VK_VERSION_1_1,VK_KHR_maintenance1[]
  * ename:VK_FORMAT_FEATURE_TRANSFER_SRC_BIT specifies that an image can: be
    used as a source image for <<copies, copy commands>>.
  * ename:VK_FORMAT_FEATURE_TRANSFER_DST_BIT specifies that an image can: be
    used as a destination image for <<copies, copy commands>> and <<clears,
    clear commands>>.
endif::VK_VERSION_1_1,VK_KHR_maintenance1[]
ifdef::VK_VERSION_1_2,VK_EXT_sampler_filter_minmax[]
  * ename:VK_FORMAT_FEATURE_SAMPLED_IMAGE_FILTER_MINMAX_BIT specifies
    sname:VkImage can: be used as a sampled image with a min or max
    elink:VkSamplerReductionMode.
    This bit must: only be exposed for formats that also support the
    ename:VK_FORMAT_FEATURE_SAMPLED_IMAGE_BIT.
endif::VK_VERSION_1_2,VK_EXT_sampler_filter_minmax[]
ifdef::VK_IMG_filter_cubic,VK_EXT_filter_cubic[]
  * ename:VK_FORMAT_FEATURE_SAMPLED_IMAGE_FILTER_CUBIC_BIT_EXT specifies
    that sname:VkImage can: be used with a sampler that has either of
    pname:magFilter or pname:minFilter set to ename:VK_FILTER_CUBIC_EXT, or
    be the source image for a blit with pname:filter set to
    ename:VK_FILTER_CUBIC_EXT.
    This bit must: only be exposed for formats that also support the
    ename:VK_FORMAT_FEATURE_SAMPLED_IMAGE_BIT.
    If the format being queried is a depth/stencil format, this only
    specifies that the depth aspect is cubic filterable.
endif::VK_IMG_filter_cubic,VK_EXT_filter_cubic[]
ifdef::VK_VERSION_1_1,VK_KHR_sampler_ycbcr_conversion[]
  * ename:VK_FORMAT_FEATURE_MIDPOINT_CHROMA_SAMPLES_BIT specifies that an
    application can: define a <<samplers-YCbCr-conversion,sampler {YCbCr}
    conversion>> using this format as a source, and that an image of this
    format can: be used with a slink:VkSamplerYcbcrConversionCreateInfo
    pname:xChromaOffset and/or pname:yChromaOffset of
    ename:VK_CHROMA_LOCATION_MIDPOINT.
    Otherwise both pname:xChromaOffset and pname:yChromaOffset must: be
    ename:VK_CHROMA_LOCATION_COSITED_EVEN.
    If a format does not incorporate chroma downsampling (it is not a
    "`422`" or "`420`" format) but the implementation supports sampler
    {YCbCr} conversion for this format, the implementation must: set
    ename:VK_FORMAT_FEATURE_MIDPOINT_CHROMA_SAMPLES_BIT.
  * ename:VK_FORMAT_FEATURE_COSITED_CHROMA_SAMPLES_BIT specifies that an
    application can: define a <<samplers-YCbCr-conversion,sampler {YCbCr}
    conversion>> using this format as a source, and that an image of this
    format can: be used with a slink:VkSamplerYcbcrConversionCreateInfo
    pname:xChromaOffset and/or pname:yChromaOffset of
    ename:VK_CHROMA_LOCATION_COSITED_EVEN.
    Otherwise both pname:xChromaOffset and pname:yChromaOffset must: be
    ename:VK_CHROMA_LOCATION_MIDPOINT.
    If neither ename:VK_FORMAT_FEATURE_COSITED_CHROMA_SAMPLES_BIT nor
    ename:VK_FORMAT_FEATURE_MIDPOINT_CHROMA_SAMPLES_BIT is set, the
    application must: not define a <<samplers-YCbCr-conversion,sampler
    {YCbCr} conversion>> using this format as a source.
  * ename:VK_FORMAT_FEATURE_SAMPLED_IMAGE_YCBCR_CONVERSION_LINEAR_FILTER_BIT
    specifies that an application can: define a
    <<samplers-YCbCr-conversion,sampler {YCbCr} conversion>> using this
    format as a source with pname:chromaFilter set to
    ename:VK_FILTER_LINEAR.
  * ename:VK_FORMAT_FEATURE_SAMPLED_IMAGE_YCBCR_CONVERSION_SEPARATE_RECONSTRUCTION_FILTER_BIT
    specifies that the format can have different chroma, min, and mag
    filters.
  * ename:VK_FORMAT_FEATURE_SAMPLED_IMAGE_YCBCR_CONVERSION_CHROMA_RECONSTRUCTION_EXPLICIT_BIT
    specifies that reconstruction is explicit, as described in
    <<textures-chroma-reconstruction>>.
    If this bit is not present, reconstruction is implicit by default.
  * ename:VK_FORMAT_FEATURE_SAMPLED_IMAGE_YCBCR_CONVERSION_CHROMA_RECONSTRUCTION_EXPLICIT_FORCEABLE_BIT
    specifies that reconstruction can: be forcibly made explicit by setting
    slink:VkSamplerYcbcrConversionCreateInfo::pname:forceExplicitReconstruction
    to ename:VK_TRUE.
    If the format being queried supports
    ename:VK_FORMAT_FEATURE_SAMPLED_IMAGE_YCBCR_CONVERSION_CHROMA_RECONSTRUCTION_EXPLICIT_BIT
    it must: also support
    ename:VK_FORMAT_FEATURE_SAMPLED_IMAGE_YCBCR_CONVERSION_CHROMA_RECONSTRUCTION_EXPLICIT_FORCEABLE_BIT.
  * ename:VK_FORMAT_FEATURE_DISJOINT_BIT specifies that a multi-planar image
    can: have the ename:VK_IMAGE_CREATE_DISJOINT_BIT set during image
    creation.
    An implementation must: not set ename:VK_FORMAT_FEATURE_DISJOINT_BIT for
    _single-plane formats_.
endif::VK_VERSION_1_1,VK_KHR_sampler_ycbcr_conversion[]
ifdef::VK_EXT_fragment_density_map[]
  * ename:VK_FORMAT_FEATURE_FRAGMENT_DENSITY_MAP_BIT_EXT specifies that an
    image view can: be used as a
    <<renderpass-fragmentdensitymapattachment,fragment density map
    attachment>>.
endif::VK_EXT_fragment_density_map[]
ifdef::VK_KHR_fragment_shading_rate[]
  * ename:VK_FORMAT_FEATURE_FRAGMENT_SHADING_RATE_ATTACHMENT_BIT_KHR
    specifies that an image view can: be used as a
    <<primsrast-fragment-shading-rate-attachment, fragment shading rate
    attachment>>.
    An implementation must: not set this feature for formats with numeric
    type other than etext:*UINT, or set it as a buffer feature.
endif::VK_KHR_fragment_shading_rate[]
ifdef::VK_KHR_video_decode_queue[]
  * ename:VK_FORMAT_FEATURE_VIDEO_DECODE_OUTPUT_BIT_KHR specifies that an
    image view with this format can: be used as an output for
    <<video-decode-operations,video decode operations>>
  * ename:VK_FORMAT_FEATURE_VIDEO_DECODE_DPB_BIT_KHR specifies that an image
    view with this format can: be used as a DPB for
    <<video-decode-operations,video decode operations>>
endif::VK_KHR_video_decode_queue[]
ifdef::VK_KHR_video_encode_queue[]
  * ename:VK_FORMAT_FEATURE_VIDEO_ENCODE_INPUT_BIT_KHR specifies that an
    image view with this format can: be used as an input to
    <<video-encode-operations,video encode operations>>
  * ename:VK_FORMAT_FEATURE_VIDEO_ENCODE_DPB_BIT_KHR specifies that an image
    view with this format can: be used as a DPB for
    <<video-encode-operations,video encode operations>>
endif::VK_KHR_video_encode_queue[]

The following bits may: be set in pname:bufferFeatures, specifying that the
features are supported by <<VkBuffer,buffers>> or <<VkBufferView,buffer
views>> created with the queried
flink:vkGetPhysicalDeviceFormatProperties::pname:format:

  * ename:VK_FORMAT_FEATURE_UNIFORM_TEXEL_BUFFER_BIT specifies that the
    format can: be used to create a buffer view that can: be bound to a
    ename:VK_DESCRIPTOR_TYPE_UNIFORM_TEXEL_BUFFER descriptor.
  * ename:VK_FORMAT_FEATURE_STORAGE_TEXEL_BUFFER_BIT specifies that the
    format can: be used to create a buffer view that can: be bound to a
    ename:VK_DESCRIPTOR_TYPE_STORAGE_TEXEL_BUFFER descriptor.
  * ename:VK_FORMAT_FEATURE_STORAGE_TEXEL_BUFFER_ATOMIC_BIT specifies that
    atomic operations are supported on
    ename:VK_DESCRIPTOR_TYPE_STORAGE_TEXEL_BUFFER with this format.
  * ename:VK_FORMAT_FEATURE_VERTEX_BUFFER_BIT specifies that the format can:
    be used as a vertex attribute format
    (sname:VkVertexInputAttributeDescription::pname:format).
ifdef::VK_KHR_acceleration_structure[]
  * ename:VK_FORMAT_FEATURE_ACCELERATION_STRUCTURE_VERTEX_BUFFER_BIT_KHR
    specifies that the format can: be used as the vertex format when
    creating an <<acceleration-structure,acceleration structure>>
    (sname:VkAccelerationStructureGeometryTrianglesDataKHR::pname:vertexFormat).
    This format can: also be used as the vertex format in host memory when
    doing <<host-acceleration-structure, host acceleration structure>>
    builds.
endif::VK_KHR_acceleration_structure[]

--

[open,refpage='VkFormatFeatureFlags',desc='Bitmask of VkFormatFeatureFlagBits',type='flags']
--
include::{generated}/api/flags/VkFormatFeatureFlags.txt[]

tname:VkFormatFeatureFlags is a bitmask type for setting a mask of zero or
more elink:VkFormatFeatureFlagBits.
--

ifdef::VK_VERSION_1_1,VK_KHR_get_physical_device_properties2[]

[open,refpage='vkGetPhysicalDeviceFormatProperties2',desc='Lists physical device\'s format capabilities',type='protos']
--
To query supported format features which are properties of the physical
device, call:

ifdef::VK_VERSION_1_1[]
include::{generated}/api/protos/vkGetPhysicalDeviceFormatProperties2.txt[]
endif::VK_VERSION_1_1[]

ifdef::VK_VERSION_1_1+VK_KHR_get_physical_device_properties2[or the equivalent command]

ifdef::VK_KHR_get_physical_device_properties2[]
include::{generated}/api/protos/vkGetPhysicalDeviceFormatProperties2KHR.txt[]
endif::VK_KHR_get_physical_device_properties2[]

  * pname:physicalDevice is the physical device from which to query the
    format properties.
  * pname:format is the format whose properties are queried.
  * pname:pFormatProperties is a pointer to a slink:VkFormatProperties2
    structure in which physical device properties for pname:format are
    returned.

fname:vkGetPhysicalDeviceFormatProperties2 behaves similarly to
flink:vkGetPhysicalDeviceFormatProperties, with the ability to return
extended information in a pname:pNext chain of output structures.

include::{generated}/validity/protos/vkGetPhysicalDeviceFormatProperties2.txt[]
--

[open,refpage='VkFormatProperties2',desc='Structure specifying image format properties',type='structs']
--
The sname:VkFormatProperties2 structure is defined as:

include::{generated}/api/structs/VkFormatProperties2.txt[]

ifdef::VK_KHR_get_physical_device_properties2[]
or the equivalent

include::{generated}/api/structs/VkFormatProperties2KHR.txt[]
endif::VK_KHR_get_physical_device_properties2[]

  * pname:sType is the type of this structure.
  * pname:pNext is `NULL` or a pointer to a structure extending this
    structure.
  * pname:formatProperties is a slink:VkFormatProperties structure
    describing features supported by the requested format.

include::{generated}/validity/structs/VkFormatProperties2.txt[]
--

ifdef::VK_EXT_image_drm_format_modifier[]
[open,refpage='VkDrmFormatModifierPropertiesListEXT',desc='Structure specifying the list of DRM format modifiers supported for a format',type='structs']
--
To obtain the list of <<glossary-drm-format-modifier,Linux DRM format
modifiers>> compatible with a elink:VkFormat, add a
slink:VkDrmFormatModifierPropertiesListEXT structure to the pname:pNext
chain of slink:VkFormatProperties2.

The slink:VkDrmFormatModifierPropertiesListEXT structure is defined as:

include::{generated}/api/structs/VkDrmFormatModifierPropertiesListEXT.txt[]

  * pname:sType is the type of this structure.
  * pname:pNext is `NULL` or a pointer to a structure extending this
    structure.
  * pname:drmFormatModifierCount is an inout parameter related to the number
    of modifiers compatible with the pname:format, as described below.
  * pname:pDrmFormatModifierProperties is either `NULL` or a pointer to an
    array of slink:VkDrmFormatModifierPropertiesEXT structures.

If pname:pDrmFormatModifierProperties is `NULL`, then the function returns
in pname:drmFormatModifierCount the number of modifiers compatible with the
queried pname:format.
Otherwise, the application must: set pname:drmFormatModifierCount to the
length of the array pname:pDrmFormatModifierProperties; the function will
write at most pname:drmFormatModifierCount elements to the array, and will
return in pname:drmFormatModifierCount the number of elements written.

Among the elements in array pname:pDrmFormatModifierProperties, each
returned pname:drmFormatModifier must: be unique.

include::{generated}/validity/structs/VkDrmFormatModifierPropertiesListEXT.txt[]
--

[open,refpage='VkDrmFormatModifierPropertiesEXT',desc='Structure specifying properties of a format when combined with a DRM format modifier',type='structs']
--
The slink:VkDrmFormatModifierPropertiesEXT structure describes properties of
a elink:VkFormat when that format is combined with a
<<glossary-drm-format-modifier,Linux DRM format modifier>>.
These properties, like those of slink:VkFormatProperties2, are independent
of any particular image.

The slink:VkDrmFormatModifierPropertiesEXT structure is defined as:

include::{generated}/api/structs/VkDrmFormatModifierPropertiesEXT.txt[]

  * pname:drmFormatModifier is a _Linux DRM format modifier_.
  * pname:drmFormatModifierPlaneCount is the number of _memory planes_ in
    any image created with pname:format and pname:drmFormatModifier.
    An image's _memory planecount_ is distinct from its _format planecount_,
    as explained below.
  * pname:drmFormatModifierTilingFeatures is a bitmask of
    elink:VkFormatFeatureFlagBits that are supported by any image created
    with pname:format and pname:drmFormatModifier.

The returned pname:drmFormatModifierTilingFeatures must: contain at least
one bit.

The implementation must: not return etext:DRM_FORMAT_MOD_INVALID in
pname:drmFormatModifier.

An image's _memory planecount_ (as returned by
pname:drmFormatModifierPlaneCount) is distinct from its _format planecount_
(in the sense of <<formats-requiring-sampler-ycbcr-conversion,multi-planar>>
{YCbCr} formats).
In tlink:VkImageAspectFlags, each
etext:VK_IMAGE_ASPECT_MEMORY_PLANE___i___BIT_EXT represents a _memory plane_
and each etext:VK_IMAGE_ASPECT_PLANE___i___BIT a _format plane_.

An image's set of _format planes_ is an ordered partition of the image's
*content* into separable groups of format channels.
The ordered partition is encoded in the name of each elink:VkFormat.
For example, ename:VK_FORMAT_G8_B8R8_2PLANE_420_UNORM contains two _format
planes_; the first plane contains the green channel and the second plane
contains the blue channel and red channel.
If the format name does not contain `PLANE`, then the format contains a
single plane; for example, ename:VK_FORMAT_R8G8B8A8_UNORM.
Some commands, such as flink:vkCmdCopyBufferToImage, do not operate on all
format channels in the image, but instead operate only on the _format
planes_ explicitly chosen by the application and operate on each _format
plane_ independently.

An image's set of _memory planes_ is an ordered partition of the image's
*memory* rather than the image's *content*.
Each _memory plane_ is a contiguous range of memory.
The union of an image's _memory planes_ is not necessarily contiguous.

If an image is <<glossary-linear-resource,linear>>, then the partition is
the same for _memory planes_ and for _format planes_.
Therefore, if the returned pname:drmFormatModifier is
code:DRM_FORMAT_MOD_LINEAR, then pname:drmFormatModifierPlaneCount must:
equal the _format planecount_, and pname:drmFormatModifierTilingFeatures
must: be identical to the
slink:VkFormatProperties2::pname:linearTilingFeatures returned in the same
pname:pNext chain.

If an image is <<glossary-linear-resource,non-linear>>, then the partition
of the image's *memory* into _memory planes_ is implementation-specific and
may: be unrelated to the partition of the image's *content* into _format
planes_.
For example, consider an image whose pname:format is
ename:VK_FORMAT_G8_B8_R8_3PLANE_420_UNORM, pname:tiling is
ename:VK_IMAGE_TILING_DRM_FORMAT_MODIFIER_EXT, whose pname:drmFormatModifier
is not code:DRM_FORMAT_MOD_LINEAR, and pname:flags lacks
ename:VK_IMAGE_CREATE_DISJOINT_BIT.
The image has 3 _format planes_, and commands such
flink:vkCmdCopyBufferToImage act on each _format plane_ independently as if
the data of each _format plane_ were separable from the data of the other
planes.
In a straightforward implementation, the implementation may: store the
image's content in 3 adjacent _memory planes_ where each _memory plane_
corresponds exactly to a _format plane_.
However, the implementation may: also store the image's content in a single
_memory plane_ where all format channels are combined using an
implementation-private block-compressed format; or the implementation may:
store the image's content in a collection of 7 adjacent _memory planes_
using an implementation-private sharding technique.
Because the image is non-linear and non-disjoint, the implementation has
much freedom when choosing the image's placement in memory.

The _memory planecount_ applies to function parameters and structures only
when the API specifies an explicit requirement on
pname:drmFormatModifierPlaneCount.
In all other cases, the _memory planecount_ is ignored.

include::{generated}/validity/structs/VkDrmFormatModifierPropertiesEXT.txt[]
--
endif::VK_EXT_image_drm_format_modifier[]
endif::VK_VERSION_1_1,VK_KHR_get_physical_device_properties2[]

[[potential-format-features]]
=== Potential Format Features

Some <<fundamentals-validusage,valid usage conditions>> depend on the format
features supported by an slink:VkImage whose elink:VkImageTiling is unknown.
In such cases the exact elink:VkFormatFeatureFlagBits supported by the
slink:VkImage cannot be determined, so the valid usage conditions are
expressed in terms of the _potential format features_ of the slink:VkImage
format.

The _potential format features_ of a elink:VkFormat are defined as follows:

  * The union of elink:VkFormatFeatureFlagBits supported when the
    elink:VkImageTiling is ename:VK_IMAGE_TILING_OPTIMAL
ifdef::VK_EXT_image_drm_format_modifier[]
    , ename:VK_IMAGE_TILING_DRM_FORMAT_MODIFIER_EXT,
endif::VK_EXT_image_drm_format_modifier[]
    or ename:VK_IMAGE_TILING_LINEAR
ifdef::VK_ANDROID_external_memory_android_hardware_buffer[]
    if elink:VkFormat is not ename:VK_FORMAT_UNDEFINED
  * slink:VkAndroidHardwareBufferFormatPropertiesANDROID::pname:formatFeatures
    of a valid external format if elink:VkFormat is
    ename:VK_FORMAT_UNDEFINED
endif::VK_ANDROID_external_memory_android_hardware_buffer[]

[[features-required-format-support]]
== Required Format Support

Implementations must: support at least the following set of features on the
listed formats.
For images, these features must: be supported for every elink:VkImageType
(including arrayed and cube variants) unless otherwise noted.
These features are supported on existing formats without needing to
advertise an extension or needing to explicitly enable them.
Support for additional functionality beyond the requirements listed here is
queried using the flink:vkGetPhysicalDeviceFormatProperties command.

[NOTE]
.Note
====
Unless otherwise excluded below, the required formats are supported for all
tlink:VkImageCreateFlags values as long as those flag values are otherwise
allowed.
====

The following tables show which feature bits must: be supported for each
format.
ifdef::VK_VERSION_1_1,VK_KHR_maintenance1[]
Formats that are required to support
ename:VK_FORMAT_FEATURE_SAMPLED_IMAGE_BIT must: also support
ename:VK_FORMAT_FEATURE_TRANSFER_SRC_BIT and
ename:VK_FORMAT_FEATURE_TRANSFER_DST_BIT.
endif::VK_VERSION_1_1,VK_KHR_maintenance1[]

.Key for format feature tables
[width="70%",cols="1,10"]
|====
^|{sym1} | This feature must: be supported on the named format
^|{sym2} | This feature must: be supported on at least some
of the named formats, with more information in the table
where the symbol appears
^|{sym3} | This feature must: be supported with some caveats or
preconditions, with more information in the table where the symbol appears
|====

.Feature bits in pname:optimalTilingFeatures
[width="70%"]
|====
ifdef::VK_VERSION_1_1,VK_KHR_maintenance1[]
|ename:VK_FORMAT_FEATURE_TRANSFER_SRC_BIT
|ename:VK_FORMAT_FEATURE_TRANSFER_DST_BIT
endif::VK_VERSION_1_1,VK_KHR_maintenance1[]
|ename:VK_FORMAT_FEATURE_SAMPLED_IMAGE_BIT
|ename:VK_FORMAT_FEATURE_BLIT_SRC_BIT
|ename:VK_FORMAT_FEATURE_SAMPLED_IMAGE_FILTER_LINEAR_BIT
|ename:VK_FORMAT_FEATURE_STORAGE_IMAGE_BIT
|ename:VK_FORMAT_FEATURE_STORAGE_IMAGE_ATOMIC_BIT
|ename:VK_FORMAT_FEATURE_COLOR_ATTACHMENT_BIT
|ename:VK_FORMAT_FEATURE_BLIT_DST_BIT
|ename:VK_FORMAT_FEATURE_COLOR_ATTACHMENT_BLEND_BIT
|ename:VK_FORMAT_FEATURE_DEPTH_STENCIL_ATTACHMENT_BIT
ifdef::VK_VERSION_1_2,VK_EXT_sampler_filter_minmax[]
|ename:VK_FORMAT_FEATURE_SAMPLED_IMAGE_FILTER_MINMAX_BIT
endif::VK_VERSION_1_2,VK_EXT_sampler_filter_minmax[]
|====

.Feature bits in pname:bufferFeatures
[width="70%"]
|====
|ename:VK_FORMAT_FEATURE_VERTEX_BUFFER_BIT
|ename:VK_FORMAT_FEATURE_UNIFORM_TEXEL_BUFFER_BIT
|ename:VK_FORMAT_FEATURE_STORAGE_TEXEL_BUFFER_BIT
|ename:VK_FORMAT_FEATURE_STORAGE_TEXEL_BUFFER_ATOMIC_BIT
|====

<<<

[[formats-mandatory-features-subbyte]]
.Mandatory format support: sub-byte channels
[width="100%",cols="12,^1,^1,^1,^1,^1,^1,^1,^1,^1,^1,^1,^1,^1",options="unbreakable"]
|====
13+>| ename:VK_FORMAT_FEATURE_STORAGE_TEXEL_BUFFER_ATOMIC_BIT .14+^.^| {downarrow}
12+>| ename:VK_FORMAT_FEATURE_STORAGE_TEXEL_BUFFER_BIT        .13+^.^| {downarrow}
11+>| ename:VK_FORMAT_FEATURE_UNIFORM_TEXEL_BUFFER_BIT        .12+^.^| {downarrow}
10+>| ename:VK_FORMAT_FEATURE_VERTEX_BUFFER_BIT               .11+^.^| {downarrow}
9+>| ename:VK_FORMAT_FEATURE_DEPTH_STENCIL_ATTACHMENT_BIT     .10+^.^| {downarrow}
8+>| ename:VK_FORMAT_FEATURE_COLOR_ATTACHMENT_BLEND_BIT        .9+^.^| {downarrow}
7+>| ename:VK_FORMAT_FEATURE_BLIT_DST_BIT                      .8+^.^| {downarrow}
6+>| ename:VK_FORMAT_FEATURE_COLOR_ATTACHMENT_BIT              .7+^.^| {downarrow}
5+>| ename:VK_FORMAT_FEATURE_STORAGE_IMAGE_ATOMIC_BIT          .6+^.^| {downarrow}
4+>| ename:VK_FORMAT_FEATURE_STORAGE_IMAGE_BIT                 .5+^.^| {downarrow}
3+>| ename:VK_FORMAT_FEATURE_SAMPLED_IMAGE_FILTER_LINEAR_BIT   .4+^.^| {downarrow}
2+>| ename:VK_FORMAT_FEATURE_BLIT_SRC_BIT                      .3+^.^| {downarrow}
1+>| ename:VK_FORMAT_FEATURE_SAMPLED_IMAGE_BIT                 .2+^.^| {downarrow}
s| Format
| ename:VK_FORMAT_UNDEFINED                  |   |   |   |   |   |   |   |   |   |   |   |   |
| ename:VK_FORMAT_R4G4_UNORM_PACK8           |   |   |   |   |   |   |   |   |   |   |   |   |
| ename:VK_FORMAT_R4G4B4A4_UNORM_PACK16      |   |   |   |   |   |   |   |   |   |   |   |   |
| ename:VK_FORMAT_B4G4R4A4_UNORM_PACK16      | {sym1} | {sym1} | {sym1} |   |   |   |   |   |   |   |   |   |
| ename:VK_FORMAT_R5G6B5_UNORM_PACK16        | {sym1} | {sym1} | {sym1} |   |   | {sym1} | {sym1} | {sym1} |   |   |   |   |
| ename:VK_FORMAT_B5G6R5_UNORM_PACK16        |   |   |   |   |   |   |   |   |   |   |   |   |
| ename:VK_FORMAT_R5G5B5A1_UNORM_PACK16      |   |   |   |   |   |   |   |   |   |   |   |   |
| ename:VK_FORMAT_B5G5R5A1_UNORM_PACK16      |   |   |   |   |   |   |   |   |   |   |   |   |
| ename:VK_FORMAT_A1R5G5B5_UNORM_PACK16      | {sym1} | {sym1} | {sym1} |   |   | {sym1} | {sym1} | {sym1} |   |   |   |   |
ifdef::VK_EXT_4444_formats[]
| ename:VK_FORMAT_A4R4G4B4_UNORM_PACK16_EXT      | {sym2} | {sym2} | {sym2} |   |   |   |   |   |   |   |   |   |
| ename:VK_FORMAT_A4B4G4R4_UNORM_PACK16_EXT      | {sym3} | {sym3} | {sym3} |   |   |   |   |   |   |   |   |   |
14+| Format features marked {sym2} must: be supported for
pname:optimalTilingFeatures if the sname:VkPhysicalDevice supports the
slink:VkPhysicalDevice4444FormatsFeaturesEXT::pname:formatA4R4G4B4 feature.
14+| Format features marked {sym3} must: be supported for
pname:optimalTilingFeatures if the sname:VkPhysicalDevice supports the
slink:VkPhysicalDevice4444FormatsFeaturesEXT::pname:formatA4B4G4R4 feature.
endif::VK_EXT_4444_formats[]
|====

<<<

[[formats-mandatory-features-2byte]]
.Mandatory format support: 1-3 byte-sized channels
[width="100%",cols="12,^1,^1,^1,^1,^1,^1,^1,^1,^1,^1,^1,^1,^1",options="unbreakable"]
|====
13+>| ename:VK_FORMAT_FEATURE_STORAGE_TEXEL_BUFFER_ATOMIC_BIT .14+^.^| {downarrow}
12+>| ename:VK_FORMAT_FEATURE_STORAGE_TEXEL_BUFFER_BIT        .13+^.^| {downarrow}
11+>| ename:VK_FORMAT_FEATURE_UNIFORM_TEXEL_BUFFER_BIT        .12+^.^| {downarrow}
10+>| ename:VK_FORMAT_FEATURE_VERTEX_BUFFER_BIT               .11+^.^| {downarrow}
9+>| ename:VK_FORMAT_FEATURE_DEPTH_STENCIL_ATTACHMENT_BIT     .10+^.^| {downarrow}
8+>| ename:VK_FORMAT_FEATURE_COLOR_ATTACHMENT_BLEND_BIT        .9+^.^| {downarrow}
7+>| ename:VK_FORMAT_FEATURE_BLIT_DST_BIT                      .8+^.^| {downarrow}
6+>| ename:VK_FORMAT_FEATURE_COLOR_ATTACHMENT_BIT              .7+^.^| {downarrow}
5+>| ename:VK_FORMAT_FEATURE_STORAGE_IMAGE_ATOMIC_BIT          .6+^.^| {downarrow}
4+>| ename:VK_FORMAT_FEATURE_STORAGE_IMAGE_BIT                 .5+^.^| {downarrow}
3+>| ename:VK_FORMAT_FEATURE_SAMPLED_IMAGE_FILTER_LINEAR_BIT   .4+^.^| {downarrow}
2+>| ename:VK_FORMAT_FEATURE_BLIT_SRC_BIT                      .3+^.^| {downarrow}
1+>| ename:VK_FORMAT_FEATURE_SAMPLED_IMAGE_BIT                 .2+^.^| {downarrow}
s| Format
| ename:VK_FORMAT_R8_UNORM                   | {sym1} | {sym1} | {sym1} | {sym3} |   | {sym1} | {sym1} | {sym1} |   | {sym1} | {sym1} |   |
| ename:VK_FORMAT_R8_SNORM                   | {sym1} | {sym1} | {sym1} | {sym3} |   |        |        |        |   | {sym1} | {sym1} |   |
| ename:VK_FORMAT_R8_USCALED                 |        |        |        |        |   |        |        |        |   |        |        |   |
| ename:VK_FORMAT_R8_SSCALED                 |        |        |        |        |   |        |        |        |   |        |        |   |
| ename:VK_FORMAT_R8_UINT                    | {sym1} | {sym1} |        | {sym3} |   | {sym1} | {sym1} |        |   | {sym1} | {sym1} |   |
| ename:VK_FORMAT_R8_SINT                    | {sym1} | {sym1} |        | {sym3} |   | {sym1} | {sym1} |        |   | {sym1} | {sym1} |   |
| ename:VK_FORMAT_R8_SRGB                    |        |        |        |        |   |        |        |        |   |        |        |   |
| ename:VK_FORMAT_R8G8_UNORM                 | {sym1} | {sym1} | {sym1} | {sym3} |   | {sym1} | {sym1} | {sym1} |   | {sym1} | {sym1} |   |
| ename:VK_FORMAT_R8G8_SNORM                 | {sym1} | {sym1} | {sym1} | {sym3} |   |        |        |        |   | {sym1} | {sym1} |   |
| ename:VK_FORMAT_R8G8_USCALED               |        |        |        |        |   |        |        |        |   |        |        |   |
| ename:VK_FORMAT_R8G8_SSCALED               |        |        |        |        |   |        |        |        |   |        |        |   |
| ename:VK_FORMAT_R8G8_UINT                  | {sym1} | {sym1} |        | {sym3} |   | {sym1} | {sym1} |        |   | {sym1} | {sym1} |   |
| ename:VK_FORMAT_R8G8_SINT                  | {sym1} | {sym1} |        | {sym3} |   | {sym1} | {sym1} |        |   | {sym1} | {sym1} |   |
| ename:VK_FORMAT_R8G8_SRGB                  |        |        |        |        |   |        |        |        |   |        |        |   |
| ename:VK_FORMAT_R8G8B8_UNORM               |        |        |        |        |   |        |        |        |   |        |        |   |
| ename:VK_FORMAT_R8G8B8_SNORM               |        |        |        |        |   |        |        |        |   |        |        |   |
| ename:VK_FORMAT_R8G8B8_USCALED             |        |        |        |        |   |        |        |        |   |        |        |   |
| ename:VK_FORMAT_R8G8B8_SSCALED             |        |        |        |        |   |        |        |        |   |        |        |   |
| ename:VK_FORMAT_R8G8B8_UINT                |        |        |        |        |   |        |        |        |   |        |        |   |
| ename:VK_FORMAT_R8G8B8_SINT                |        |        |        |        |   |        |        |        |   |        |        |   |
| ename:VK_FORMAT_R8G8B8_SRGB                |        |        |        |        |   |        |        |        |   |        |        |   |
| ename:VK_FORMAT_B8G8R8_UNORM               |        |        |        |        |   |        |        |        |   |        |        |   |
| ename:VK_FORMAT_B8G8R8_SNORM               |        |        |        |        |   |        |        |        |   |        |        |   |
| ename:VK_FORMAT_B8G8R8_USCALED             |        |        |        |        |   |        |        |        |   |        |        |   |
| ename:VK_FORMAT_B8G8R8_SSCALED             |        |        |        |        |   |        |        |        |   |        |        |   |
| ename:VK_FORMAT_B8G8R8_UINT                |        |        |        |        |   |        |        |        |   |        |        |   |
| ename:VK_FORMAT_B8G8R8_SINT                |        |        |        |        |   |        |        |        |   |        |        |   |
| ename:VK_FORMAT_B8G8R8_SRGB                |        |        |        |        |   |        |        |        |   |        |        |   |
14+| Format features marked with {sym3} must: be supported for
pname:optimalTilingFeatures if the sname:VkPhysicalDevice supports the
<<features-shaderStorageImageExtendedFormats,
pname:shaderStorageImageExtendedFormats>> feature.
|====

<<<

[[formats-mandatory-features-4byte]]
.Mandatory format support: 4 byte-sized channels
[width="100%",cols="12,^1,^1,^1,^1,^1,^1,^1,^1,^1,^1,^1,^1,^1",options="unbreakable"]
|====
13+>| ename:VK_FORMAT_FEATURE_STORAGE_TEXEL_BUFFER_ATOMIC_BIT .14+^.^| {downarrow}
12+>| ename:VK_FORMAT_FEATURE_STORAGE_TEXEL_BUFFER_BIT        .13+^.^| {downarrow}
11+>| ename:VK_FORMAT_FEATURE_UNIFORM_TEXEL_BUFFER_BIT        .12+^.^| {downarrow}
10+>| ename:VK_FORMAT_FEATURE_VERTEX_BUFFER_BIT               .11+^.^| {downarrow}
9+>| ename:VK_FORMAT_FEATURE_DEPTH_STENCIL_ATTACHMENT_BIT     .10+^.^| {downarrow}
8+>| ename:VK_FORMAT_FEATURE_COLOR_ATTACHMENT_BLEND_BIT        .9+^.^| {downarrow}
7+>| ename:VK_FORMAT_FEATURE_BLIT_DST_BIT                      .8+^.^| {downarrow}
6+>| ename:VK_FORMAT_FEATURE_COLOR_ATTACHMENT_BIT              .7+^.^| {downarrow}
5+>| ename:VK_FORMAT_FEATURE_STORAGE_IMAGE_ATOMIC_BIT          .6+^.^| {downarrow}
4+>| ename:VK_FORMAT_FEATURE_STORAGE_IMAGE_BIT                 .5+^.^| {downarrow}
3+>| ename:VK_FORMAT_FEATURE_SAMPLED_IMAGE_FILTER_LINEAR_BIT   .4+^.^| {downarrow}
2+>| ename:VK_FORMAT_FEATURE_BLIT_SRC_BIT                      .3+^.^| {downarrow}
1+>| ename:VK_FORMAT_FEATURE_SAMPLED_IMAGE_BIT                 .2+^.^| {downarrow}
s| Format
| ename:VK_FORMAT_R8G8B8A8_UNORM             | {sym1} | {sym1} | {sym1} | {sym1} |   | {sym1} | {sym1} | {sym1} |   | {sym1} | {sym1} | {sym1} |
| ename:VK_FORMAT_R8G8B8A8_SNORM             | {sym1} | {sym1} | {sym1} | {sym1} |   |   |   |   |   | {sym1} | {sym1} | {sym1} |
| ename:VK_FORMAT_R8G8B8A8_USCALED           |   |   |   |   |   |   |   |   |   |   |   |   |
| ename:VK_FORMAT_R8G8B8A8_SSCALED           |   |   |   |   |   |   |   |   |   |   |   |   |
| ename:VK_FORMAT_R8G8B8A8_UINT              | {sym1} | {sym1} |   | {sym1} |   | {sym1} | {sym1} |   |   | {sym1} | {sym1} | {sym1} |
| ename:VK_FORMAT_R8G8B8A8_SINT              | {sym1} | {sym1} |   | {sym1} |   | {sym1} | {sym1} |   |   | {sym1} | {sym1} | {sym1} |
| ename:VK_FORMAT_R8G8B8A8_SRGB              | {sym1} | {sym1} | {sym1} |   |   | {sym1} | {sym1} | {sym1} |   |   |   |   |
| ename:VK_FORMAT_B8G8R8A8_UNORM             | {sym1} | {sym1} | {sym1} |   |   | {sym1} | {sym1} | {sym1} |   | {sym1} | {sym1} |   |
| ename:VK_FORMAT_B8G8R8A8_SNORM             |   |   |   |   |   |   |   |   |   |   |   |   |
| ename:VK_FORMAT_B8G8R8A8_USCALED           |   |   |   |   |   |   |   |   |   |   |   |   |
| ename:VK_FORMAT_B8G8R8A8_SSCALED           |   |   |   |   |   |   |   |   |   |   |   |   |
| ename:VK_FORMAT_B8G8R8A8_UINT              |   |   |   |   |   |   |   |   |   |   |   |   |
| ename:VK_FORMAT_B8G8R8A8_SINT              |   |   |   |   |   |   |   |   |   |   |   |   |
| ename:VK_FORMAT_B8G8R8A8_SRGB              | {sym1} | {sym1} | {sym1} |   |   | {sym1} | {sym1} | {sym1} |   |   |   |   |
| ename:VK_FORMAT_A8B8G8R8_UNORM_PACK32      | {sym1} | {sym1} | {sym1} |   |   | {sym1} | {sym1} | {sym1} |   | {sym1} | {sym1} | {sym1} |
| ename:VK_FORMAT_A8B8G8R8_SNORM_PACK32      | {sym1} | {sym1} | {sym1} |   |   |   |   |   |   | {sym1} | {sym1} | {sym1} |
| ename:VK_FORMAT_A8B8G8R8_USCALED_PACK32    |   |   |   |   |   |   |   |   |   |   |   |   |
| ename:VK_FORMAT_A8B8G8R8_SSCALED_PACK32    |   |   |   |   |   |   |   |   |   |   |   |   |
| ename:VK_FORMAT_A8B8G8R8_UINT_PACK32       | {sym1} | {sym1} |   |   |   | {sym1} | {sym1} |   |   | {sym1} | {sym1} | {sym1} |
| ename:VK_FORMAT_A8B8G8R8_SINT_PACK32       | {sym1} | {sym1} |   |   |   | {sym1} | {sym1} |   |   | {sym1} | {sym1} | {sym1} |
| ename:VK_FORMAT_A8B8G8R8_SRGB_PACK32       | {sym1} | {sym1} | {sym1} |   |   | {sym1} | {sym1} | {sym1} |   |   |   |   |
|====

<<<

[[formats-mandatory-features-10bit]]
.Mandatory format support: 10- and 12-bit channels
[width="100%",cols="12,^1,^1,^1,^1,^1,^1,^1,^1,^1,^1,^1,^1,^1",options="unbreakable"]
|====
13+>| ename:VK_FORMAT_FEATURE_STORAGE_TEXEL_BUFFER_ATOMIC_BIT .14+^.^| {downarrow}
12+>| ename:VK_FORMAT_FEATURE_STORAGE_TEXEL_BUFFER_BIT        .13+^.^| {downarrow}
11+>| ename:VK_FORMAT_FEATURE_UNIFORM_TEXEL_BUFFER_BIT        .12+^.^| {downarrow}
10+>| ename:VK_FORMAT_FEATURE_VERTEX_BUFFER_BIT               .11+^.^| {downarrow}
9+>| ename:VK_FORMAT_FEATURE_DEPTH_STENCIL_ATTACHMENT_BIT     .10+^.^| {downarrow}
8+>| ename:VK_FORMAT_FEATURE_COLOR_ATTACHMENT_BLEND_BIT        .9+^.^| {downarrow}
7+>| ename:VK_FORMAT_FEATURE_BLIT_DST_BIT                      .8+^.^| {downarrow}
6+>| ename:VK_FORMAT_FEATURE_COLOR_ATTACHMENT_BIT              .7+^.^| {downarrow}
5+>| ename:VK_FORMAT_FEATURE_STORAGE_IMAGE_ATOMIC_BIT          .6+^.^| {downarrow}
4+>| ename:VK_FORMAT_FEATURE_STORAGE_IMAGE_BIT                 .5+^.^| {downarrow}
3+>| ename:VK_FORMAT_FEATURE_SAMPLED_IMAGE_FILTER_LINEAR_BIT   .4+^.^| {downarrow}
2+>| ename:VK_FORMAT_FEATURE_BLIT_SRC_BIT                      .3+^.^| {downarrow}
1+>| ename:VK_FORMAT_FEATURE_SAMPLED_IMAGE_BIT                 .2+^.^| {downarrow}
s| Format
| ename:VK_FORMAT_A2R10G10B10_UNORM_PACK32   |        |        |        |        |   |        |        |        |   |        |        |   |
| ename:VK_FORMAT_A2R10G10B10_SNORM_PACK32   |        |        |        |        |   |        |        |        |   |        |        |   |
| ename:VK_FORMAT_A2R10G10B10_USCALED_PACK32 |        |        |        |        |   |        |        |        |   |        |        |   |
| ename:VK_FORMAT_A2R10G10B10_SSCALED_PACK32 |        |        |        |        |   |        |        |        |   |        |        |   |
| ename:VK_FORMAT_A2R10G10B10_UINT_PACK32    |        |        |        |        |   |        |        |        |   |        |        |   |
| ename:VK_FORMAT_A2R10G10B10_SINT_PACK32    |        |        |        |        |   |        |        |        |   |        |        |   |
| ename:VK_FORMAT_A2B10G10R10_UNORM_PACK32   | {sym1} | {sym1} | {sym1} | {sym3} |   | {sym1} | {sym1} | {sym1} |   | {sym1} | {sym1} |   |
| ename:VK_FORMAT_A2B10G10R10_SNORM_PACK32   |        |        |        |        |   |        |        |        |   |        |        |   |
| ename:VK_FORMAT_A2B10G10R10_USCALED_PACK32 |        |        |        |        |   |        |        |        |   |        |        |   |
| ename:VK_FORMAT_A2B10G10R10_SSCALED_PACK32 |        |        |        |        |   |        |        |        |   |        |        |   |
| ename:VK_FORMAT_A2B10G10R10_UINT_PACK32    | {sym1} | {sym1} |        | {sym3} |   | {sym1} | {sym1} |        |   |        | {sym1} |   |
| ename:VK_FORMAT_A2B10G10R10_SINT_PACK32    |        |        |        |        |   |        |        |        |   |        |        |   |
ifdef::VK_VERSION_1_1,VK_KHR_sampler_ycbcr_conversion[]
| ename:VK_FORMAT_R10X6_UNORM_PACK16         |        |        |        |        |   |        |        |        |   |        |        |   |
| ename:VK_FORMAT_R10X6G10X6_UNORM_2PACK16   |        |        |        |        |   |        |        |        |   |        |        |   |
| ename:VK_FORMAT_R12X4_UNORM_PACK16         |        |        |        |        |   |        |        |        |   |        |        |   |
| ename:VK_FORMAT_R12X4G12X4_UNORM_2PACK16   |        |        |        |        |   |        |        |        |   |        |        |   |
endif::VK_VERSION_1_1,VK_KHR_sampler_ycbcr_conversion[]
14+| Format features marked with {sym3} must: be supported for
pname:optimalTilingFeatures if the sname:VkPhysicalDevice supports the
<<features-shaderStorageImageExtendedFormats,
pname:shaderStorageImageExtendedFormats>> feature.
|====

<<<

[[formats-mandatory-features-16bit]]
.Mandatory format support: 16-bit channels
[width="100%",cols="12,^1,^1,^1,^1,^1,^1,^1,^1,^1,^1,^1,^1,^1",options="unbreakable"]
|====
13+>| ename:VK_FORMAT_FEATURE_STORAGE_TEXEL_BUFFER_ATOMIC_BIT .14+^.^| {downarrow}
12+>| ename:VK_FORMAT_FEATURE_STORAGE_TEXEL_BUFFER_BIT        .13+^.^| {downarrow}
11+>| ename:VK_FORMAT_FEATURE_UNIFORM_TEXEL_BUFFER_BIT        .12+^.^| {downarrow}
10+>| ename:VK_FORMAT_FEATURE_VERTEX_BUFFER_BIT               .11+^.^| {downarrow}
9+>| ename:VK_FORMAT_FEATURE_DEPTH_STENCIL_ATTACHMENT_BIT     .10+^.^| {downarrow}
8+>| ename:VK_FORMAT_FEATURE_COLOR_ATTACHMENT_BLEND_BIT        .9+^.^| {downarrow}
7+>| ename:VK_FORMAT_FEATURE_BLIT_DST_BIT                      .8+^.^| {downarrow}
6+>| ename:VK_FORMAT_FEATURE_COLOR_ATTACHMENT_BIT              .7+^.^| {downarrow}
5+>| ename:VK_FORMAT_FEATURE_STORAGE_IMAGE_ATOMIC_BIT          .6+^.^| {downarrow}
4+>| ename:VK_FORMAT_FEATURE_STORAGE_IMAGE_BIT                 .5+^.^| {downarrow}
3+>| ename:VK_FORMAT_FEATURE_SAMPLED_IMAGE_FILTER_LINEAR_BIT   .4+^.^| {downarrow}
2+>| ename:VK_FORMAT_FEATURE_BLIT_SRC_BIT                      .3+^.^| {downarrow}
1+>| ename:VK_FORMAT_FEATURE_SAMPLED_IMAGE_BIT                 .2+^.^| {downarrow}
s| Format
| ename:VK_FORMAT_R16_UNORM                  |        |        |        | {sym3} |   |        |        |        |   | {sym1} |        |        |
| ename:VK_FORMAT_R16_SNORM                  |        |        |        | {sym3} |   |        |        |        |   | {sym1} |        |        |
| ename:VK_FORMAT_R16_USCALED                |        |        |        |        |   |        |        |        |   |        |        |        |
| ename:VK_FORMAT_R16_SSCALED                |        |        |        |        |   |        |        |        |   |        |        |        |
| ename:VK_FORMAT_R16_UINT                   | {sym1} | {sym1} |        | {sym3} |   | {sym1} | {sym1} |        |   | {sym1} | {sym1} |        |
| ename:VK_FORMAT_R16_SINT                   | {sym1} | {sym1} |        | {sym3} |   | {sym1} | {sym1} |        |   | {sym1} | {sym1} |        |
| ename:VK_FORMAT_R16_SFLOAT                 | {sym1} | {sym1} | {sym1} | {sym3} |   | {sym1} | {sym1} | {sym1} |   | {sym1} | {sym1} |        |
| ename:VK_FORMAT_R16G16_UNORM               |        |        |        | {sym3} |   |        |        |        |   | {sym1} |        |        |
| ename:VK_FORMAT_R16G16_SNORM               |        |        |        | {sym3} |   |        |        |        |   | {sym1} |        |        |
| ename:VK_FORMAT_R16G16_USCALED             |        |        |        |        |   |        |        |        |   |        |        |        |
| ename:VK_FORMAT_R16G16_SSCALED             |        |        |        |        |   |        |        |        |   |        |        |        |
| ename:VK_FORMAT_R16G16_UINT                | {sym1} | {sym1} |        | {sym3} |   | {sym1} | {sym1} |        |   | {sym1} | {sym1} |        |
| ename:VK_FORMAT_R16G16_SINT                | {sym1} | {sym1} |        | {sym3} |   | {sym1} | {sym1} |        |   | {sym1} | {sym1} |        |
| ename:VK_FORMAT_R16G16_SFLOAT              | {sym1} | {sym1} | {sym1} | {sym3} |   | {sym1} | {sym1} | {sym1} |   | {sym1} | {sym1} |        |
| ename:VK_FORMAT_R16G16B16_UNORM            |        |        |        |        |   |        |        |        |   |        |        |        |
| ename:VK_FORMAT_R16G16B16_SNORM            |        |        |        |        |   |        |        |        |   |        |        |        |
| ename:VK_FORMAT_R16G16B16_USCALED          |        |        |        |        |   |        |        |        |   |        |        |        |
| ename:VK_FORMAT_R16G16B16_SSCALED          |        |        |        |        |   |        |        |        |   |        |        |        |
| ename:VK_FORMAT_R16G16B16_UINT             |        |        |        |        |   |        |        |        |   |        |        |        |
| ename:VK_FORMAT_R16G16B16_SINT             |        |        |        |        |   |        |        |        |   |        |        |        |
| ename:VK_FORMAT_R16G16B16_SFLOAT           |        |        |        |        |   |        |        |        |   |        |        |        |
| ename:VK_FORMAT_R16G16B16A16_UNORM         |        |        |        | {sym3} |   |        |        |        |   | {sym1} |        |        |
| ename:VK_FORMAT_R16G16B16A16_SNORM         |        |        |        | {sym3} |   |        |        |        |   | {sym1} |        |        |
| ename:VK_FORMAT_R16G16B16A16_USCALED       |        |        |        |        |   |        |        |        |   |        |        |        |
| ename:VK_FORMAT_R16G16B16A16_SSCALED       |        |        |        |        |   |        |        |        |   |        |        |        |
| ename:VK_FORMAT_R16G16B16A16_UINT          | {sym1} | {sym1} |        | {sym1} |   | {sym1} | {sym1} |        |   | {sym1} | {sym1} | {sym1} |
| ename:VK_FORMAT_R16G16B16A16_SINT          | {sym1} | {sym1} |        | {sym1} |   | {sym1} | {sym1} |        |   | {sym1} | {sym1} | {sym1} |
| ename:VK_FORMAT_R16G16B16A16_SFLOAT        | {sym1} | {sym1} | {sym1} | {sym1} |   | {sym1} | {sym1} | {sym1} |   | {sym1} | {sym1} | {sym1} |
14+| Format features marked with {sym3} must: be supported for
pname:optimalTilingFeatures if the sname:VkPhysicalDevice supports the
<<features-shaderStorageImageExtendedFormats,
pname:shaderStorageImageExtendedFormats>> feature.
|====

<<<

[[formats-mandatory-features-32bit]]
.Mandatory format support: 32-bit channels
[width="100%",cols="12,^1,^1,^1,^1,^1,^1,^1,^1,^1,^1,^1,^1,^1",options="unbreakable"]
|====
13+>| ename:VK_FORMAT_FEATURE_STORAGE_TEXEL_BUFFER_ATOMIC_BIT .14+^.^| {downarrow}
12+>| ename:VK_FORMAT_FEATURE_STORAGE_TEXEL_BUFFER_BIT        .13+^.^| {downarrow}
11+>| ename:VK_FORMAT_FEATURE_UNIFORM_TEXEL_BUFFER_BIT        .12+^.^| {downarrow}
10+>| ename:VK_FORMAT_FEATURE_VERTEX_BUFFER_BIT               .11+^.^| {downarrow}
9+>| ename:VK_FORMAT_FEATURE_DEPTH_STENCIL_ATTACHMENT_BIT     .10+^.^| {downarrow}
8+>| ename:VK_FORMAT_FEATURE_COLOR_ATTACHMENT_BLEND_BIT        .9+^.^| {downarrow}
7+>| ename:VK_FORMAT_FEATURE_BLIT_DST_BIT                      .8+^.^| {downarrow}
6+>| ename:VK_FORMAT_FEATURE_COLOR_ATTACHMENT_BIT              .7+^.^| {downarrow}
5+>| ename:VK_FORMAT_FEATURE_STORAGE_IMAGE_ATOMIC_BIT          .6+^.^| {downarrow}
4+>| ename:VK_FORMAT_FEATURE_STORAGE_IMAGE_BIT                 .5+^.^| {downarrow}
3+>| ename:VK_FORMAT_FEATURE_SAMPLED_IMAGE_FILTER_LINEAR_BIT   .4+^.^| {downarrow}
2+>| ename:VK_FORMAT_FEATURE_BLIT_SRC_BIT                      .3+^.^| {downarrow}
1+>| ename:VK_FORMAT_FEATURE_SAMPLED_IMAGE_BIT                 .2+^.^| {downarrow}
s| Format
| ename:VK_FORMAT_R32_UINT                   | {sym1} | {sym1} |   | {sym1} | {sym1} | {sym1} | {sym1} |   |   | {sym1} | {sym1} | {sym1} | {sym1}
| ename:VK_FORMAT_R32_SINT                   | {sym1} | {sym1} |   | {sym1} | {sym1} | {sym1} | {sym1} |   |   | {sym1} | {sym1} | {sym1} | {sym1}
| ename:VK_FORMAT_R32_SFLOAT                 | {sym1} | {sym1} |   | {sym1} |   | {sym1} | {sym1} |   |   | {sym1} | {sym1} | {sym1} |
| ename:VK_FORMAT_R32G32_UINT                | {sym1} | {sym1} |   | {sym1} |   | {sym1} | {sym1} |   |   | {sym1} | {sym1} | {sym1} |
| ename:VK_FORMAT_R32G32_SINT                | {sym1} | {sym1} |   | {sym1} |   | {sym1} | {sym1} |   |   | {sym1} | {sym1} | {sym1} |
| ename:VK_FORMAT_R32G32_SFLOAT              | {sym1} | {sym1} |   | {sym1} |   | {sym1} | {sym1} |   |   | {sym1} | {sym1} | {sym1} |
| ename:VK_FORMAT_R32G32B32_UINT             |   |   |   |   |   |   |   |   |   | {sym1} |   |   |
| ename:VK_FORMAT_R32G32B32_SINT             |   |   |   |   |   |   |   |   |   | {sym1} |   |   |
| ename:VK_FORMAT_R32G32B32_SFLOAT           |   |   |   |   |   |   |   |   |   | {sym1} |   |   |
| ename:VK_FORMAT_R32G32B32A32_UINT          | {sym1} | {sym1} |   | {sym1} |   | {sym1} | {sym1} |   |   | {sym1} | {sym1} | {sym1} |
| ename:VK_FORMAT_R32G32B32A32_SINT          | {sym1} | {sym1} |   | {sym1} |   | {sym1} | {sym1} |   |   | {sym1} | {sym1} | {sym1} |
| ename:VK_FORMAT_R32G32B32A32_SFLOAT        | {sym1} | {sym1} |   | {sym1} |   | {sym1} | {sym1} |   |   | {sym1} | {sym1} | {sym1} |
ifdef::VK_EXT_shader_atomic_float[]
14+|
If the <<features-shaderImageFloat32Atomics, pname:shaderImageFloat32Atomics>>
or the <<features-shaderImageFloat32AtomicAdd, pname:shaderImageFloat32AtomicAdd>>
ifdef::VK_EXT_shader_atomic_float2[]
or the <<features-shaderImageFloat32AtomicMinMax, pname:shaderImageFloat32AtomicMinMax>>
endif::VK_EXT_shader_atomic_float2[]
feature is supported, ename:VK_FORMAT_FEATURE_STORAGE_IMAGE_BIT and
ename:VK_FORMAT_FEATURE_STORAGE_IMAGE_ATOMIC_BIT must: be advertised in
pname:optimalTilingFeatures for ename:VK_FORMAT_R32_SFLOAT.
endif::VK_EXT_shader_atomic_float[]
|====

<<<

[[formats-mandatory-features-64bit]]
.Mandatory format support: 64-bit/uneven channels
[width="100%",cols="12,^1,^1,^1,^1,^1,^1,^1,^1,^1,^1,^1,^1,^1",options="unbreakable"]
|====
13+>| ename:VK_FORMAT_FEATURE_STORAGE_TEXEL_BUFFER_ATOMIC_BIT .14+^.^| {downarrow}
12+>| ename:VK_FORMAT_FEATURE_STORAGE_TEXEL_BUFFER_BIT        .13+^.^| {downarrow}
11+>| ename:VK_FORMAT_FEATURE_UNIFORM_TEXEL_BUFFER_BIT        .12+^.^| {downarrow}
10+>| ename:VK_FORMAT_FEATURE_VERTEX_BUFFER_BIT               .11+^.^| {downarrow}
9+>| ename:VK_FORMAT_FEATURE_DEPTH_STENCIL_ATTACHMENT_BIT     .10+^.^| {downarrow}
8+>| ename:VK_FORMAT_FEATURE_COLOR_ATTACHMENT_BLEND_BIT        .9+^.^| {downarrow}
7+>| ename:VK_FORMAT_FEATURE_BLIT_DST_BIT                      .8+^.^| {downarrow}
6+>| ename:VK_FORMAT_FEATURE_COLOR_ATTACHMENT_BIT              .7+^.^| {downarrow}
5+>| ename:VK_FORMAT_FEATURE_STORAGE_IMAGE_ATOMIC_BIT          .6+^.^| {downarrow}
4+>| ename:VK_FORMAT_FEATURE_STORAGE_IMAGE_BIT                 .5+^.^| {downarrow}
3+>| ename:VK_FORMAT_FEATURE_SAMPLED_IMAGE_FILTER_LINEAR_BIT   .4+^.^| {downarrow}
2+>| ename:VK_FORMAT_FEATURE_BLIT_SRC_BIT                      .3+^.^| {downarrow}
1+>| ename:VK_FORMAT_FEATURE_SAMPLED_IMAGE_BIT                 .2+^.^| {downarrow}
s| Format
| ename:VK_FORMAT_R64_UINT                   |        |        |
|
ifdef::VK_EXT_shader_image_atomic_int64[{sym2}]
|
ifdef::VK_EXT_shader_image_atomic_int64[{sym2}]
                                                                                     |   |   |   |   |   |        |   |
| ename:VK_FORMAT_R64_SINT                   |        |        |
|
ifdef::VK_EXT_shader_image_atomic_int64[{sym2}]
|
ifdef::VK_EXT_shader_image_atomic_int64[{sym2}]
                                                                                     |   |   |   |   |   |        |   |
| ename:VK_FORMAT_R64_SFLOAT                 |        |        |        |        |   |   |   |   |   |   |        |   |
| ename:VK_FORMAT_R64G64_UINT                |        |        |        |        |   |   |   |   |   |   |        |   |
| ename:VK_FORMAT_R64G64_SINT                |        |        |        |        |   |   |   |   |   |   |        |   |
| ename:VK_FORMAT_R64G64_SFLOAT              |        |        |        |        |   |   |   |   |   |   |        |   |
| ename:VK_FORMAT_R64G64B64_UINT             |        |        |        |        |   |   |   |   |   |   |        |   |
| ename:VK_FORMAT_R64G64B64_SINT             |        |        |        |        |   |   |   |   |   |   |        |   |
| ename:VK_FORMAT_R64G64B64_SFLOAT           |        |        |        |        |   |   |   |   |   |   |        |   |
| ename:VK_FORMAT_R64G64B64A64_UINT          |        |        |        |        |   |   |   |   |   |   |        |   |
| ename:VK_FORMAT_R64G64B64A64_SINT          |        |        |        |        |   |   |   |   |   |   |        |   |
| ename:VK_FORMAT_R64G64B64A64_SFLOAT        |        |        |        |        |   |   |   |   |   |   |        |   |
| ename:VK_FORMAT_B10G11R11_UFLOAT_PACK32    | {sym1} | {sym1} | {sym1} | {sym3} |   |   |   |   |   |   | {sym1} |   |
| ename:VK_FORMAT_E5B9G9R9_UFLOAT_PACK32     | {sym1} | {sym1} | {sym1} |        |   |   |   |   |   |   |        |   |
14+| Format features marked with {sym3} must: be supported for
pname:optimalTilingFeatures if the sname:VkPhysicalDevice supports the
<<features-shaderStorageImageExtendedFormats,
pname:shaderStorageImageExtendedFormats>> feature.
ifdef::VK_EXT_shader_image_atomic_int64[]
14+|
If the <<features-shaderImageInt64Atomics, pname:shaderImageInt64Atomics>>
feature is supported, ename:VK_FORMAT_FEATURE_STORAGE_IMAGE_BIT and
ename:VK_FORMAT_FEATURE_STORAGE_IMAGE_ATOMIC_BIT must: be advertised in
pname:optimalTilingFeatures for both ename:VK_FORMAT_R64_UINT and
ename:VK_FORMAT_R64_SINT.
endif::VK_EXT_shader_image_atomic_int64[]
|====

<<<

[[formats-mandatory-features-depth-stencil]]
.Mandatory format support: depth/stencil with `VkImageType` ename:VK_IMAGE_TYPE_2D
[width="100%",cols="12,^1,^1,^1,^1,^1,^1,^1,^1,^1,^1,^1,^1,^1",options="unbreakable"]
|====
13+>| ename:VK_FORMAT_FEATURE_STORAGE_TEXEL_BUFFER_ATOMIC_BIT .14+^.^| {downarrow}
12+>| ename:VK_FORMAT_FEATURE_STORAGE_TEXEL_BUFFER_BIT        .13+^.^| {downarrow}
11+>| ename:VK_FORMAT_FEATURE_UNIFORM_TEXEL_BUFFER_BIT        .12+^.^| {downarrow}
10+>| ename:VK_FORMAT_FEATURE_VERTEX_BUFFER_BIT               .11+^.^| {downarrow}
9+>| ename:VK_FORMAT_FEATURE_DEPTH_STENCIL_ATTACHMENT_BIT     .10+^.^| {downarrow}
8+>| ename:VK_FORMAT_FEATURE_COLOR_ATTACHMENT_BLEND_BIT        .9+^.^| {downarrow}
7+>| ename:VK_FORMAT_FEATURE_BLIT_DST_BIT                      .8+^.^| {downarrow}
6+>| ename:VK_FORMAT_FEATURE_COLOR_ATTACHMENT_BIT              .7+^.^| {downarrow}
5+>| ename:VK_FORMAT_FEATURE_STORAGE_IMAGE_ATOMIC_BIT          .6+^.^| {downarrow}
4+>| ename:VK_FORMAT_FEATURE_STORAGE_IMAGE_BIT                 .5+^.^| {downarrow}
3+>| ename:VK_FORMAT_FEATURE_SAMPLED_IMAGE_FILTER_LINEAR_BIT   .4+^.^| {downarrow}
2+>| ename:VK_FORMAT_FEATURE_BLIT_SRC_BIT                      .3+^.^| {downarrow}
1+>| ename:VK_FORMAT_FEATURE_SAMPLED_IMAGE_BIT                 .2+^.^| {downarrow}
s| Format
| ename:VK_FORMAT_D16_UNORM                  | {sym1} | {sym1} |   |   |   |   |   |   | {sym1} |   |   |   |
| ename:VK_FORMAT_X8_D24_UNORM_PACK32        |   |   |   |   |   |   |   |   | {sym2} |   |   |   |
| ename:VK_FORMAT_D32_SFLOAT                 | {sym1} | {sym1} |   |   |   |   |   |   | {sym2} |   |   |   |
| ename:VK_FORMAT_S8_UINT                    |   |   |   |   |   |   |   |   |   |   |   |   |
| ename:VK_FORMAT_D16_UNORM_S8_UINT          |   |   |   |   |   |   |   |   |   |   |   |   |
| ename:VK_FORMAT_D24_UNORM_S8_UINT          |   |   |   |   |   |   |   |   | {sym2} |   |   |   |
| ename:VK_FORMAT_D32_SFLOAT_S8_UINT         |   |   |   |   |   |   |   |   | {sym2} |   |   |   |
14+| ename:VK_FORMAT_FEATURE_DEPTH_STENCIL_ATTACHMENT_BIT feature must: be
supported for at least one of ename:VK_FORMAT_X8_D24_UNORM_PACK32 and
ename:VK_FORMAT_D32_SFLOAT, and must: be supported for at least one of
ename:VK_FORMAT_D24_UNORM_S8_UINT and ename:VK_FORMAT_D32_SFLOAT_S8_UINT.
|====

<<<

[[formats-mandatory-features-bcn]]
.Mandatory format support: BC compressed formats with `VkImageType` ename:VK_IMAGE_TYPE_2D and ename:VK_IMAGE_TYPE_3D
[width="100%",cols="12,^1,^1,^1,^1,^1,^1,^1,^1,^1,^1,^1,^1,^1",options="unbreakable"]
|====
13+>| ename:VK_FORMAT_FEATURE_STORAGE_TEXEL_BUFFER_ATOMIC_BIT .14+^.^| {downarrow}
12+>| ename:VK_FORMAT_FEATURE_STORAGE_TEXEL_BUFFER_BIT        .13+^.^| {downarrow}
11+>| ename:VK_FORMAT_FEATURE_UNIFORM_TEXEL_BUFFER_BIT        .12+^.^| {downarrow}
10+>| ename:VK_FORMAT_FEATURE_VERTEX_BUFFER_BIT               .11+^.^| {downarrow}
9+>| ename:VK_FORMAT_FEATURE_DEPTH_STENCIL_ATTACHMENT_BIT     .10+^.^| {downarrow}
8+>| ename:VK_FORMAT_FEATURE_COLOR_ATTACHMENT_BLEND_BIT        .9+^.^| {downarrow}
7+>| ename:VK_FORMAT_FEATURE_BLIT_DST_BIT                      .8+^.^| {downarrow}
6+>| ename:VK_FORMAT_FEATURE_COLOR_ATTACHMENT_BIT              .7+^.^| {downarrow}
5+>| ename:VK_FORMAT_FEATURE_STORAGE_IMAGE_ATOMIC_BIT          .6+^.^| {downarrow}
4+>| ename:VK_FORMAT_FEATURE_STORAGE_IMAGE_BIT                 .5+^.^| {downarrow}
3+>| ename:VK_FORMAT_FEATURE_SAMPLED_IMAGE_FILTER_LINEAR_BIT   .4+^.^| {downarrow}
2+>| ename:VK_FORMAT_FEATURE_BLIT_SRC_BIT                      .3+^.^| {downarrow}
1+>| ename:VK_FORMAT_FEATURE_SAMPLED_IMAGE_BIT                 .2+^.^| {downarrow}
s| Format
| ename:VK_FORMAT_BC1_RGB_UNORM_BLOCK        | {sym2} | {sym2} | {sym2} |   |   |   |   |   |   |   |   |   |
| ename:VK_FORMAT_BC1_RGB_SRGB_BLOCK         | {sym2} | {sym2} | {sym2} |   |   |   |   |   |   |   |   |   |
| ename:VK_FORMAT_BC1_RGBA_UNORM_BLOCK       | {sym2} | {sym2} | {sym2} |   |   |   |   |   |   |   |   |   |
| ename:VK_FORMAT_BC1_RGBA_SRGB_BLOCK        | {sym2} | {sym2} | {sym2} |   |   |   |   |   |   |   |   |   |
| ename:VK_FORMAT_BC2_UNORM_BLOCK            | {sym2} | {sym2} | {sym2} |   |   |   |   |   |   |   |   |   |
| ename:VK_FORMAT_BC2_SRGB_BLOCK             | {sym2} | {sym2} | {sym2} |   |   |   |   |   |   |   |   |   |
| ename:VK_FORMAT_BC3_UNORM_BLOCK            | {sym2} | {sym2} | {sym2} |   |   |   |   |   |   |   |   |   |
| ename:VK_FORMAT_BC3_SRGB_BLOCK             | {sym2} | {sym2} | {sym2} |   |   |   |   |   |   |   |   |   |
| ename:VK_FORMAT_BC4_UNORM_BLOCK            | {sym2} | {sym2} | {sym2} |   |   |   |   |   |   |   |   |   |
| ename:VK_FORMAT_BC4_SNORM_BLOCK            | {sym2} | {sym2} | {sym2} |   |   |   |   |   |   |   |   |   |
| ename:VK_FORMAT_BC5_UNORM_BLOCK            | {sym2} | {sym2} | {sym2} |   |   |   |   |   |   |   |   |   |
| ename:VK_FORMAT_BC5_SNORM_BLOCK            | {sym2} | {sym2} | {sym2} |   |   |   |   |   |   |   |   |   |
| ename:VK_FORMAT_BC6H_UFLOAT_BLOCK          | {sym2} | {sym2} | {sym2} |   |   |   |   |   |   |   |   |   |
| ename:VK_FORMAT_BC6H_SFLOAT_BLOCK          | {sym2} | {sym2} | {sym2} |   |   |   |   |   |   |   |   |   |
| ename:VK_FORMAT_BC7_UNORM_BLOCK            | {sym2} | {sym2} | {sym2} |   |   |   |   |   |   |   |   |   |
| ename:VK_FORMAT_BC7_SRGB_BLOCK             | {sym2} | {sym2} | {sym2} |   |   |   |   |   |   |   |   |   |
14+| The ename:VK_FORMAT_FEATURE_SAMPLED_IMAGE_BIT,
ename:VK_FORMAT_FEATURE_BLIT_SRC_BIT and
ename:VK_FORMAT_FEATURE_SAMPLED_IMAGE_FILTER_LINEAR_BIT features must: be
supported in pname:optimalTilingFeatures for all the formats in at least
one of: this table, <<formats-mandatory-features-etc>>, or
<<formats-mandatory-features-astc>>.
|====

<<<

[[formats-mandatory-features-etc]]
.Mandatory format support: ETC2 and EAC compressed formats with `VkImageType` ename:VK_IMAGE_TYPE_2D
[width="100%",cols="12,^1,^1,^1,^1,^1,^1,^1,^1,^1,^1,^1,^1,^1",options="unbreakable"]
|====
13+>| ename:VK_FORMAT_FEATURE_STORAGE_TEXEL_BUFFER_ATOMIC_BIT .14+^.^| {downarrow}
12+>| ename:VK_FORMAT_FEATURE_STORAGE_TEXEL_BUFFER_BIT        .13+^.^| {downarrow}
11+>| ename:VK_FORMAT_FEATURE_UNIFORM_TEXEL_BUFFER_BIT        .12+^.^| {downarrow}
10+>| ename:VK_FORMAT_FEATURE_VERTEX_BUFFER_BIT               .11+^.^| {downarrow}
9+>| ename:VK_FORMAT_FEATURE_DEPTH_STENCIL_ATTACHMENT_BIT     .10+^.^| {downarrow}
8+>| ename:VK_FORMAT_FEATURE_COLOR_ATTACHMENT_BLEND_BIT        .9+^.^| {downarrow}
7+>| ename:VK_FORMAT_FEATURE_BLIT_DST_BIT                      .8+^.^| {downarrow}
6+>| ename:VK_FORMAT_FEATURE_COLOR_ATTACHMENT_BIT              .7+^.^| {downarrow}
5+>| ename:VK_FORMAT_FEATURE_STORAGE_IMAGE_ATOMIC_BIT          .6+^.^| {downarrow}
4+>| ename:VK_FORMAT_FEATURE_STORAGE_IMAGE_BIT                 .5+^.^| {downarrow}
3+>| ename:VK_FORMAT_FEATURE_SAMPLED_IMAGE_FILTER_LINEAR_BIT   .4+^.^| {downarrow}
2+>| ename:VK_FORMAT_FEATURE_BLIT_SRC_BIT                      .3+^.^| {downarrow}
1+>| ename:VK_FORMAT_FEATURE_SAMPLED_IMAGE_BIT                 .2+^.^| {downarrow}
s| Format
| ename:VK_FORMAT_ETC2_R8G8B8_UNORM_BLOCK    | {sym2} | {sym2} | {sym2} |   |   |   |   |   |   |   |   |   |
| ename:VK_FORMAT_ETC2_R8G8B8_SRGB_BLOCK     | {sym2} | {sym2} | {sym2} |   |   |   |   |   |   |   |   |   |
| ename:VK_FORMAT_ETC2_R8G8B8A1_UNORM_BLOCK  | {sym2} | {sym2} | {sym2} |   |   |   |   |   |   |   |   |   |
| ename:VK_FORMAT_ETC2_R8G8B8A1_SRGB_BLOCK   | {sym2} | {sym2} | {sym2} |   |   |   |   |   |   |   |   |   |
| ename:VK_FORMAT_ETC2_R8G8B8A8_UNORM_BLOCK  | {sym2} | {sym2} | {sym2} |   |   |   |   |   |   |   |   |   |
| ename:VK_FORMAT_ETC2_R8G8B8A8_SRGB_BLOCK   | {sym2} | {sym2} | {sym2} |   |   |   |   |   |   |   |   |   |
| ename:VK_FORMAT_EAC_R11_UNORM_BLOCK        | {sym2} | {sym2} | {sym2} |   |   |   |   |   |   |   |   |   |
| ename:VK_FORMAT_EAC_R11_SNORM_BLOCK        | {sym2} | {sym2} | {sym2} |   |   |   |   |   |   |   |   |   |
| ename:VK_FORMAT_EAC_R11G11_UNORM_BLOCK     | {sym2} | {sym2} | {sym2} |   |   |   |   |   |   |   |   |   |
| ename:VK_FORMAT_EAC_R11G11_SNORM_BLOCK     | {sym2} | {sym2} | {sym2} |   |   |   |   |   |   |   |   |   |
14+|The ename:VK_FORMAT_FEATURE_SAMPLED_IMAGE_BIT,
ename:VK_FORMAT_FEATURE_BLIT_SRC_BIT and
ename:VK_FORMAT_FEATURE_SAMPLED_IMAGE_FILTER_LINEAR_BIT features must: be
supported in pname:optimalTilingFeatures for all the formats in at least
one of: this table, <<formats-mandatory-features-bcn>>, or
<<formats-mandatory-features-astc>>.
|====

<<<

[[formats-mandatory-features-astc]]
.Mandatory format support: ASTC LDR compressed formats with `VkImageType` ename:VK_IMAGE_TYPE_2D
[width="100%",cols="12,^1,^1,^1,^1,^1,^1,^1,^1,^1,^1,^1,^1,^1",options="unbreakable"]
|====
13+>| ename:VK_FORMAT_FEATURE_STORAGE_TEXEL_BUFFER_ATOMIC_BIT .14+^.^| {downarrow}
12+>| ename:VK_FORMAT_FEATURE_STORAGE_TEXEL_BUFFER_BIT        .13+^.^| {downarrow}
11+>| ename:VK_FORMAT_FEATURE_UNIFORM_TEXEL_BUFFER_BIT        .12+^.^| {downarrow}
10+>| ename:VK_FORMAT_FEATURE_VERTEX_BUFFER_BIT               .11+^.^| {downarrow}
9+>| ename:VK_FORMAT_FEATURE_DEPTH_STENCIL_ATTACHMENT_BIT     .10+^.^| {downarrow}
8+>| ename:VK_FORMAT_FEATURE_COLOR_ATTACHMENT_BLEND_BIT        .9+^.^| {downarrow}
7+>| ename:VK_FORMAT_FEATURE_BLIT_DST_BIT                      .8+^.^| {downarrow}
6+>| ename:VK_FORMAT_FEATURE_COLOR_ATTACHMENT_BIT              .7+^.^| {downarrow}
5+>| ename:VK_FORMAT_FEATURE_STORAGE_IMAGE_ATOMIC_BIT          .6+^.^| {downarrow}
4+>| ename:VK_FORMAT_FEATURE_STORAGE_IMAGE_BIT                 .5+^.^| {downarrow}
3+>| ename:VK_FORMAT_FEATURE_SAMPLED_IMAGE_FILTER_LINEAR_BIT   .4+^.^| {downarrow}
2+>| ename:VK_FORMAT_FEATURE_BLIT_SRC_BIT                      .3+^.^| {downarrow}
1+>| ename:VK_FORMAT_FEATURE_SAMPLED_IMAGE_BIT                 .2+^.^| {downarrow}
s| Format
| ename:VK_FORMAT_ASTC_4x4_UNORM_BLOCK       | {sym2} | {sym2} | {sym2} |   |   |   |   |   |   |   |   |   |
| ename:VK_FORMAT_ASTC_4x4_SRGB_BLOCK        | {sym2} | {sym2} | {sym2} |   |   |   |   |   |   |   |   |   |
| ename:VK_FORMAT_ASTC_5x4_UNORM_BLOCK       | {sym2} | {sym2} | {sym2} |   |   |   |   |   |   |   |   |   |
| ename:VK_FORMAT_ASTC_5x4_SRGB_BLOCK        | {sym2} | {sym2} | {sym2} |   |   |   |   |   |   |   |   |   |
| ename:VK_FORMAT_ASTC_5x5_UNORM_BLOCK       | {sym2} | {sym2} | {sym2} |   |   |   |   |   |   |   |   |   |
| ename:VK_FORMAT_ASTC_5x5_SRGB_BLOCK        | {sym2} | {sym2} | {sym2} |   |   |   |   |   |   |   |   |   |
| ename:VK_FORMAT_ASTC_6x5_UNORM_BLOCK       | {sym2} | {sym2} | {sym2} |   |   |   |   |   |   |   |   |   |
| ename:VK_FORMAT_ASTC_6x5_SRGB_BLOCK        | {sym2} | {sym2} | {sym2} |   |   |   |   |   |   |   |   |   |
| ename:VK_FORMAT_ASTC_6x6_UNORM_BLOCK       | {sym2} | {sym2} | {sym2} |   |   |   |   |   |   |   |   |   |
| ename:VK_FORMAT_ASTC_6x6_SRGB_BLOCK        | {sym2} | {sym2} | {sym2} |   |   |   |   |   |   |   |   |   |
| ename:VK_FORMAT_ASTC_8x5_UNORM_BLOCK       | {sym2} | {sym2} | {sym2} |   |   |   |   |   |   |   |   |   |
| ename:VK_FORMAT_ASTC_8x5_SRGB_BLOCK        | {sym2} | {sym2} | {sym2} |   |   |   |   |   |   |   |   |   |
| ename:VK_FORMAT_ASTC_8x6_UNORM_BLOCK       | {sym2} | {sym2} | {sym2} |   |   |   |   |   |   |   |   |   |
| ename:VK_FORMAT_ASTC_8x6_SRGB_BLOCK        | {sym2} | {sym2} | {sym2} |   |   |   |   |   |   |   |   |   |
| ename:VK_FORMAT_ASTC_8x8_UNORM_BLOCK       | {sym2} | {sym2} | {sym2} |   |   |   |   |   |   |   |   |   |
| ename:VK_FORMAT_ASTC_8x8_SRGB_BLOCK        | {sym2} | {sym2} | {sym2} |   |   |   |   |   |   |   |   |   |
| ename:VK_FORMAT_ASTC_10x5_UNORM_BLOCK      | {sym2} | {sym2} | {sym2} |   |   |   |   |   |   |   |   |   |
| ename:VK_FORMAT_ASTC_10x5_SRGB_BLOCK       | {sym2} | {sym2} | {sym2} |   |   |   |   |   |   |   |   |   |
| ename:VK_FORMAT_ASTC_10x6_UNORM_BLOCK      | {sym2} | {sym2} | {sym2} |   |   |   |   |   |   |   |   |   |
| ename:VK_FORMAT_ASTC_10x6_SRGB_BLOCK       | {sym2} | {sym2} | {sym2} |   |   |   |   |   |   |   |   |   |
| ename:VK_FORMAT_ASTC_10x8_UNORM_BLOCK      | {sym2} | {sym2} | {sym2} |   |   |   |   |   |   |   |   |   |
| ename:VK_FORMAT_ASTC_10x8_SRGB_BLOCK       | {sym2} | {sym2} | {sym2} |   |   |   |   |   |   |   |   |   |
| ename:VK_FORMAT_ASTC_10x10_UNORM_BLOCK     | {sym2} | {sym2} | {sym2} |   |   |   |   |   |   |   |   |   |
| ename:VK_FORMAT_ASTC_10x10_SRGB_BLOCK      | {sym2} | {sym2} | {sym2} |   |   |   |   |   |   |   |   |   |
| ename:VK_FORMAT_ASTC_12x10_UNORM_BLOCK     | {sym2} | {sym2} | {sym2} |   |   |   |   |   |   |   |   |   |
| ename:VK_FORMAT_ASTC_12x10_SRGB_BLOCK      | {sym2} | {sym2} | {sym2} |   |   |   |   |   |   |   |   |   |
| ename:VK_FORMAT_ASTC_12x12_UNORM_BLOCK     | {sym2} | {sym2} | {sym2} |   |   |   |   |   |   |   |   |   |
| ename:VK_FORMAT_ASTC_12x12_SRGB_BLOCK      | {sym2} | {sym2} | {sym2} |   |   |   |   |   |   |   |   |   |
14+|The ename:VK_FORMAT_FEATURE_SAMPLED_IMAGE_BIT,
ename:VK_FORMAT_FEATURE_BLIT_SRC_BIT and
ename:VK_FORMAT_FEATURE_SAMPLED_IMAGE_FILTER_LINEAR_BIT features must: be
supported in pname:optimalTilingFeatures for all the formats in at least
one of: this table, <<formats-mandatory-features-bcn>>, or
<<formats-mandatory-features-etc>>.
|====

ifdef::VK_IMG_filter_cubic,VK_EXT_filter_cubic[]
If cubic filtering is supported,
ename:VK_FORMAT_FEATURE_SAMPLED_IMAGE_FILTER_CUBIC_BIT_EXT must: be
supported for the following image view types:

  * ename:VK_IMAGE_VIEW_TYPE_2D
  * ename:VK_IMAGE_VIEW_TYPE_2D_ARRAY

for the following formats:

  * ename:VK_FORMAT_R4G4_UNORM_PACK8
  * ename:VK_FORMAT_R4G4B4A4_UNORM_PACK16
  * ename:VK_FORMAT_B4G4R4A4_UNORM_PACK16
  * ename:VK_FORMAT_R5G6B5_UNORM_PACK16
  * ename:VK_FORMAT_B5G6R5_UNORM_PACK16
  * ename:VK_FORMAT_R5G5B5A1_UNORM_PACK16
  * ename:VK_FORMAT_B5G5R5A1_UNORM_PACK16
  * ename:VK_FORMAT_A1R5G5B5_UNORM_PACK16
  * ename:VK_FORMAT_R8_UNORM
  * ename:VK_FORMAT_R8_SNORM
  * ename:VK_FORMAT_R8_SRGB
  * ename:VK_FORMAT_R8G8_UNORM
  * ename:VK_FORMAT_R8G8_SNORM
  * ename:VK_FORMAT_R8G8_SRGB
  * ename:VK_FORMAT_R8G8B8_UNORM
  * ename:VK_FORMAT_R8G8B8_SNORM
  * ename:VK_FORMAT_R8G8B8_SRGB
  * ename:VK_FORMAT_B8G8R8_UNORM
  * ename:VK_FORMAT_B8G8R8_SNORM
  * ename:VK_FORMAT_B8G8R8_SRGB
  * ename:VK_FORMAT_R8G8B8A8_UNORM
  * ename:VK_FORMAT_R8G8B8A8_SNORM
  * ename:VK_FORMAT_R8G8B8A8_SRGB
  * ename:VK_FORMAT_B8G8R8A8_UNORM
  * ename:VK_FORMAT_B8G8R8A8_SNORM
  * ename:VK_FORMAT_B8G8R8A8_SRGB
  * ename:VK_FORMAT_A8B8G8R8_UNORM_PACK32
  * ename:VK_FORMAT_A8B8G8R8_SNORM_PACK32
  * ename:VK_FORMAT_A8B8G8R8_SRGB_PACK32

If ETC compressed formats are supported,
ename:VK_FORMAT_FEATURE_SAMPLED_IMAGE_FILTER_CUBIC_BIT_EXT must: be
supported for the following image view types:

  * ename:VK_IMAGE_VIEW_TYPE_2D
  * ename:VK_IMAGE_VIEW_TYPE_2D_ARRAY

for the following additional formats:

  * ename:VK_FORMAT_ETC2_R8G8B8_UNORM_BLOCK
  * ename:VK_FORMAT_ETC2_R8G8B8_SRGB_BLOCK
  * ename:VK_FORMAT_ETC2_R8G8B8A1_UNORM_BLOCK
  * ename:VK_FORMAT_ETC2_R8G8B8A1_SRGB_BLOCK
  * ename:VK_FORMAT_ETC2_R8G8B8A8_UNORM_BLOCK
  * ename:VK_FORMAT_ETC2_R8G8B8A8_SRGB_BLOCK

If cubic filtering is supported for any other formats, the following image
view types must: be supported for those formats:

  * ename:VK_IMAGE_VIEW_TYPE_2D
  * ename:VK_IMAGE_VIEW_TYPE_2D_ARRAY

endif::VK_IMG_filter_cubic,VK_EXT_filter_cubic[]

ifdef::VK_VERSION_1_1,VK_KHR_sampler_ycbcr_conversion[]

To be used with sname:VkImageView with pname:subresourceRange.aspectMask =
ename:VK_IMAGE_ASPECT_COLOR_BIT, <<samplers-YCbCr-conversion,sampler {YCbCr}
conversion>> must: be enabled for the following formats:

[[formats-requiring-sampler-ycbcr-conversion]]
.Formats requiring sampler {YCbCr} conversion for ename:VK_IMAGE_ASPECT_COLOR_BIT image views
[width="100%",cols="18,^3,^1,^1,^1,^1,^1,^1,^1,^1,^1,^1",options="unbreakable"]
|====
11+>| ename:VK_FORMAT_FEATURE_SAMPLED_IMAGE_YCBCR_CONVERSION_CHROMA_RECONSTRUCTION_EXPLICIT_FORCEABLE_BIT  .11+^.^| {downarrow}
10+>| ename:VK_FORMAT_FEATURE_SAMPLED_IMAGE_YCBCR_CONVERSION_CHROMA_RECONSTRUCTION_EXPLICIT_BIT            .10+^.^| {downarrow}
9+>| ename:VK_FORMAT_FEATURE_SAMPLED_IMAGE_YCBCR_CONVERSION_SEPARATE_RECONSTRUCTION_FILTER_BIT             .9+^.^| {downarrow}
8+>| ename:VK_FORMAT_FEATURE_SAMPLED_IMAGE_YCBCR_CONVERSION_LINEAR_FILTER_BIT                              .8+^.^| {downarrow}
7+>| ename:VK_FORMAT_FEATURE_MIDPOINT_CHROMA_SAMPLES_BIT         .7+^.^| {downarrow}
6+>| ename:VK_FORMAT_FEATURE_COSITED_CHROMA_SAMPLES_BIT          .6+^.^| {downarrow}
5+>| ename:VK_FORMAT_FEATURE_TRANSFER_DST_BIT                    .5+^.^| {downarrow}
4+>| ename:VK_FORMAT_FEATURE_TRANSFER_SRC_BIT                    .4+^.^| {downarrow}
3+>| ename:VK_FORMAT_FEATURE_SAMPLED_IMAGE_BIT                   .3+^.^| {downarrow}
2+>| ename:VK_FORMAT_FEATURE_DISJOINT_BIT                        .2+^.^| {downarrow}
s| Format                                                     s| Planes
| ename:VK_FORMAT_G8B8G8R8_422_UNORM                           | 1 |  |        |        |        |        | | | | |
| ename:VK_FORMAT_B8G8R8G8_422_UNORM                           | 1 |  |        |        |        |        | | | | |
| ename:VK_FORMAT_G8_B8_R8_3PLANE_420_UNORM                    | 3 |  | {sym2} | {sym2} | {sym2} | {sym2} | | | | |
| ename:VK_FORMAT_G8_B8R8_2PLANE_420_UNORM                     | 2 |  | {sym2} | {sym2} | {sym2} | {sym2} | | | | |
| ename:VK_FORMAT_G8_B8_R8_3PLANE_422_UNORM                    | 3 |  |        |        |        |        | | | | |
| ename:VK_FORMAT_G8_B8R8_2PLANE_422_UNORM                     | 2 |  |        |        |        |        | | | | |
| ename:VK_FORMAT_G8_B8_R8_3PLANE_444_UNORM                    | 3 |  |        |        |        |        | | | | |
| ename:VK_FORMAT_R10X6G10X6B10X6A10X6_UNORM_4PACK16           | 1 |  |        |        |        |        | | | | |
| ename:VK_FORMAT_G10X6B10X6G10X6R10X6_422_UNORM_4PACK16       | 1 |  |        |        |        |        | | | | |
| ename:VK_FORMAT_B10X6G10X6R10X6G10X6_422_UNORM_4PACK16       | 1 |  |        |        |        |        | | | | |
| ename:VK_FORMAT_G10X6_B10X6_R10X6_3PLANE_420_UNORM_3PACK16   | 3 |  |        |        |        |        | | | | |
| ename:VK_FORMAT_G10X6_B10X6R10X6_2PLANE_420_UNORM_3PACK16    | 2 |  |        |        |        |        | | | | |
| ename:VK_FORMAT_G10X6_B10X6_R10X6_3PLANE_422_UNORM_3PACK16   | 3 |  |        |        |        |        | | | | |
| ename:VK_FORMAT_G10X6_B10X6R10X6_2PLANE_422_UNORM_3PACK16    | 2 |  |        |        |        |        | | | | |
| ename:VK_FORMAT_G10X6_B10X6_R10X6_3PLANE_444_UNORM_3PACK16   | 3 |  |        |        |        |        | | | | |
| ename:VK_FORMAT_R12X4G12X4B12X4A12X4_UNORM_4PACK16           | 1 |  |        |        |        |        | | | | |
| ename:VK_FORMAT_G12X4B12X4G12X4R12X4_422_UNORM_4PACK16       | 1 |  |        |        |        |        | | | | |
| ename:VK_FORMAT_B12X4G12X4R12X4G12X4_422_UNORM_4PACK16       | 1 |  |        |        |        |        | | | | |
| ename:VK_FORMAT_G12X4_B12X4_R12X4_3PLANE_420_UNORM_3PACK16   | 3 |  |        |        |        |        | | | | |
| ename:VK_FORMAT_G12X4_B12X4R12X4_2PLANE_420_UNORM_3PACK16    | 2 |  |        |        |        |        | | | | |
| ename:VK_FORMAT_G12X4_B12X4_R12X4_3PLANE_422_UNORM_3PACK16   | 3 |  |        |        |        |        | | | | |
| ename:VK_FORMAT_G12X4_B12X4R12X4_2PLANE_422_UNORM_3PACK16    | 2 |  |        |        |        |        | | | | |
| ename:VK_FORMAT_G12X4_B12X4_R12X4_3PLANE_444_UNORM_3PACK16   | 3 |  |        |        |        |        | | | | |
| ename:VK_FORMAT_G16B16G16R16_422_UNORM                       | 1 |  |        |        |        |        | | | | |
| ename:VK_FORMAT_B16G16R16G16_422_UNORM                       | 1 |  |        |        |        |        | | | | |
| ename:VK_FORMAT_G16_B16_R16_3PLANE_420_UNORM                 | 3 |  |        |        |        |        | | | | |
| ename:VK_FORMAT_G16_B16R16_2PLANE_420_UNORM                  | 2 |  |        |        |        |        | | | | |
| ename:VK_FORMAT_G16_B16_R16_3PLANE_422_UNORM                 | 3 |  |        |        |        |        | | | | |
| ename:VK_FORMAT_G16_B16R16_2PLANE_422_UNORM                  | 2 |  |        |        |        |        | | | | |
| ename:VK_FORMAT_G16_B16_R16_3PLANE_444_UNORM                 | 3 |  |        |        |        |        | | | | |
ifdef::VK_EXT_ycbcr_2plane_444_formats[]
| ename:VK_FORMAT_G8_B8R8_2PLANE_444_UNORM_EXT                     | 2 |  |        |        |        |        | | | | |
| ename:VK_FORMAT_G10X6_B10X6R10X6_2PLANE_444_UNORM_3PACK16_EXT    | 2 |  |        |        |        |        | | | | |
| ename:VK_FORMAT_G12X4_B12X4R12X4_2PLANE_444_UNORM_3PACK16_EXT    | 2 |  |        |        |        |        | | | | |
| ename:VK_FORMAT_G16_B16R16_2PLANE_444_UNORM_EXT                  | 2 |  |        |        |        |        | | | | |
endif::VK_EXT_ycbcr_2plane_444_formats[]
12+| Format features marked {sym2} must: be supported for
pname:optimalTilingFeatures with elink:VkImageType
ename:VK_IMAGE_TYPE_2D if the sname:VkPhysicalDevice supports the
slink:VkPhysicalDeviceSamplerYcbcrConversionFeatures feature.
|====

Implementations are not required to support the
ename:VK_IMAGE_CREATE_SPARSE_BINDING_BIT,
ename:VK_IMAGE_CREATE_SPARSE_RESIDENCY_BIT, or
ename:VK_IMAGE_CREATE_SPARSE_ALIASED_BIT tlink:VkImageCreateFlags for the
above formats that require <<samplers-YCbCr-conversion,sampler {YCbCr}
conversion>>.
To determine whether the implementation supports sparse image creation flags
with these formats use flink:vkGetPhysicalDeviceImageFormatProperties or
flink:vkGetPhysicalDeviceImageFormatProperties2.

endif::VK_VERSION_1_1,VK_KHR_sampler_ycbcr_conversion[]

ifdef::VK_EXT_fragment_density_map[]
ename:VK_FORMAT_FEATURE_FRAGMENT_DENSITY_MAP_BIT_EXT must: be supported for
the following formats if the <<features-fragmentDensityMap,fragment density
map feature>> is enabled:

  * ename:VK_FORMAT_R8G8_UNORM
endif::VK_EXT_fragment_density_map[]

ifdef::VK_KHR_acceleration_structure[]
ename:VK_FORMAT_FEATURE_ACCELERATION_STRUCTURE_VERTEX_BUFFER_BIT_KHR must:
be supported in pname:bufferFeatures for the following formats if the
<<features-accelerationStructure, pname:accelerationStructure>> feature is
supported:

  * ename:VK_FORMAT_R32G32_SFLOAT
  * ename:VK_FORMAT_R32G32B32_SFLOAT
  * ename:VK_FORMAT_R16G16_SFLOAT
  * ename:VK_FORMAT_R16G16B16A16_SFLOAT
  * ename:VK_FORMAT_R16G16_SNORM
  * ename:VK_FORMAT_R16G16B16A16_SNORM
endif::VK_KHR_acceleration_structure[]

ifdef::VK_KHR_fragment_shading_rate[]
ename:VK_FORMAT_FEATURE_FRAGMENT_SHADING_RATE_ATTACHMENT_BIT_KHR must: be
supported for the following formats if the
<<features-attachmentFragmentShadingRate,
pname:attachmentFragmentShadingRate feature>> is supported:

  * ename:VK_FORMAT_R8_UINT
endif::VK_KHR_fragment_shading_rate[]
