// Copyright 2018-2021 The Khronos Group, Inc.
//
// SPDX-License-Identifier: CC-BY-4.0

If an image is presented to a swapchain created from a display surface, the
mode of the associated display will be updated, if necessary, to match the
mode specified when creating the display surface.
The mode switch and presentation of the specified image will be performed as
one atomic operation.
