Settings: CPU Serttings

- Use multicore features
  Cpu tuner uses a different cpu backend if a multicore cpu is detected. This options allows you to enforce, disable or automatically chose this backend.
- Show Userspace Governor
  Not recommended since to userspace governor does not do any battery saving.
- Min displayed frequency
  The minimum displayed cpu frequency for the maximum cpu frequency. Default is 400 MHz.
- Allowed CPU frequencies
  A list of frequencies (in Hz not MHz) separated by spaces, which are used a cpu frequencies if the system does not report any.
- Default maximum frequency
  This frequency will be used when a system configuration is applied.
- Default minimum frequency
  This frequency will be used when a system configuration is applied.