<?xml version="1.0" encoding="utf-8" ?>
<!DOCTYPE erlref SYSTEM "erlref.dtd">

<erlref>
  <header>
    <copyright>
      <year>2002</year><year>2016</year>
      <holder>Ericsson AB. All Rights Reserved.</holder>
    </copyright>
    <legalnotice>
      Licensed under the Apache License, Version 2.0 (the "License");
      you may not use this file except in compliance with the License.
      You may obtain a copy of the License at
 
          http://www.apache.org/licenses/LICENSE-2.0

      Unless required by applicable law or agreed to in writing, software
      distributed under the License is distributed on an "AS IS" BASIS,
      WITHOUT WARRANTIES OR CONDITIONS OF ANY KIND, either express or implied.
      See the License for the specific language governing permissions and
      limitations under the License.
    
    </legalnotice>

    <title>megaco_codec_mstone1</title>
    <prepared>Micael Karlberg</prepared>
    <responsible>Micael Karlberg</responsible>
    <docno></docno>
    <approved>Micael Karlberg</approved>
    <checked></checked>
    <date>2009-05-27</date>
    <rev>%VSN%</rev>
    <file>megaco_codec_mstone1.xml</file>
  </header>
  <module>megaco_codec_mstone1</module>
  <modulesummary>This module implements a simple megaco codec-based performance tool.</modulesummary>
  <description>
    <p>This module implements the <em>mstone1</em> tool, 
      a simple megaco codec-based performance tool.</p>
    <p>The results, the mstone value(s), are written to stdout.</p>
    <p><em>Note</em> that this module is <em>not</em> included in the runtime part of 
      the application.</p>
  </description>

  <funcs>
    <func>
      <name>start() -> void()</name>
      <name>start(MessagePackage) -> void()</name>
      <name>start(MessagePackage, Factor) -> void()</name>
      <fsummary></fsummary>
      <type>
        <v>MessagePackage = message_package()</v>
        <v>message_package() = atom()</v>
        <v>Factor() = integer() > 0</v>
      </type>
      <desc>
        <p>This function starts the <em>mstone1</em> performance test with all codec configs. 
          <c>Factor</c> (defaults to <c>1</c>) processes are started for every supported 
          codec config. </p>
        <p>Each process encodes and decodes their messages. 
          The number of messages processed in total (for all processes) is the mstone value.</p>
      </desc>
    </func>

    <func>
      <name>start_flex() -> void()</name>
      <name>start_flex(MessagePackage) -> void()</name>
      <name>start_flex(MessagePackage, Factor) -> void()</name>
      <fsummary></fsummary>
      <type>
        <v>MessagePackage = message_package()</v>
        <v>message_package() = atom()</v>
        <v>Factor() = integer() > 0</v>
      </type>
      <desc>
        <p>This function starts the <em>mstone1</em> performance test with only the
          flex codec configs (i.e. <c>pretty</c> and <c>compact</c> with <c>flex</c>). 
          The same number of processes are started as when running the standard
          test (using the <c>start/0,1</c> function).
          Each process encodes and decodes their messages. 
          The number of messages processed in total (for all processes) is the mstone value.</p>
      </desc>
    </func>

    <func>
      <name>start_only_drv() -> void()</name>
      <name>start_only_drv(MessagePackage) -> void()</name>
      <name>start_only_drv(MessagePackage, Factor) -> void()</name>
      <fsummary></fsummary>
      <type>
        <v>MessagePackage = message_package()</v>
        <v>message_package() = atom()</v>
        <v>Factor() = integer() > 0</v>
      </type>
      <desc>
        <p>This function starts the <em>mstone1</em> performance test with only the
          driver using codec configs (i.e. <c>pretty</c> and <c>compact</c> 
          with <c>flex</c>, and <c>ber</c> and <c>per</c> with <c>driver</c> 
          and <c>erlang</c> with <c>compressed</c>). 
          The same number of processes are started as when running the standard
          test (using the <c>start/0,1</c> function).
          Each process encodes and decodes their messages. 
          The number of messages processed in total (for all processes) is the mstone value.</p>
      </desc>
    </func>

    <func>
      <name>start_no_drv() -> void()</name>
      <name>start_no_drv(MessagePackage) -> void()</name>
      <name>start_no_drv(MessagePackage, Factor) -> void()</name>
      <fsummary></fsummary>
      <type>
        <v>MessagePackage = message_package()</v>
        <v>message_package() = atom()</v>
        <v>Factor() = integer() > 0</v>
      </type>
      <desc>
        <p>This function starts the <em>mstone1</em> performance test with codec configs
          not using any drivers (i.e. <c>pretty</c> and <c>compact</c> without 
          <c>flex</c>, <c>ber</c> and <c>per</c> without <c>driver</c> and 
          <c>erlang</c> without <c>compressed</c>). 
          The same number of processes are started as when running the standard
          test (using the <c>start/0,1</c> function).
          Each process encodes and decodes their messages. 
          The number of messages processed in total (for all processes) is the mstone value.</p>
      </desc>
    </func>

  </funcs>

</erlref>

