<?xml version="1.0" encoding="utf-8" ?>
<!DOCTYPE erlref SYSTEM "erlref.dtd">

<erlref>
  <header>
    <copyright>
      <year>1999</year><year>2016</year>
      <holder>Ericsson AB. All Rights Reserved.</holder>
    </copyright>
    <legalnotice>
      Licensed under the Apache License, Version 2.0 (the "License");
      you may not use this file except in compliance with the License.
      You may obtain a copy of the License at
 
          http://www.apache.org/licenses/LICENSE-2.0

      Unless required by applicable law or agreed to in writing, software
      distributed under the License is distributed on an "AS IS" BASIS,
      WITHOUT WARRANTIES OR CONDITIONS OF ANY KIND, either express or implied.
      See the License for the specific language governing permissions and
      limitations under the License.
    
    </legalnotice>

    <title>snmp_user_based_sm_mib</title>
    <prepared></prepared>
    <responsible></responsible>
    <docno></docno>
    <approved></approved>
    <checked></checked>
    <date></date>
    <rev></rev>
    <file>snmp_user_based_sm_mib.xml</file>
  </header>
  <module>snmp_user_based_sm_mib</module>
  <modulesummary>Instrumentation Functions for SNMP-USER-BASED-SM-MIB</modulesummary>
  <description>
    <p>The module <c>snmp_user_based_sm_mib</c> implements the instrumentation 
      functions for the SNMP-USER-BASED-SM-MIB, and functions for configuring 
      the database.
      </p>
    <p>The configuration files are described in the SNMP User's Manual.</p>
  </description>
  <funcs>
    <func>
      <name>configure(ConfDir) -> void()</name>
      <fsummary>Configure the SNMP-USER-BASED-SM-MIB</fsummary>
      <type>
        <v>ConfDir = string()</v>
      </type>
      <desc>
        <p>This function is called from the supervisor at system
          start-up.
          </p>
        <p>Inserts all data in the configuration files into the
          database and destroys all old rows with StorageType
          <c>volatile</c>.  The rows created from the configuration file
          will have StorageType <c>nonVolatile</c>.
          </p>
        <p>All <c>snmp</c> counters are set to zero.
          </p>
        <p>If an error is found in the configuration file, it is
          reported using the function <c>config_err/2</c> of the error
          report module, and the function fails with the reason 
          <c>configuration_error</c>.
          </p>
        <p><c>ConfDir</c> is a string which points to the directory
          where the configuration files are found.
          </p>
        <p>The configuration file read is: <c>usm.conf</c>.
          </p>
      </desc>
    </func>
    <func>
      <name>reconfigure(ConfDir) -> void()</name>
      <fsummary>Configure the SNMP-USER-BASED-SM-MIB</fsummary>
      <type>
        <v>ConfDir = string()</v>
      </type>
      <desc>
        <p>Inserts all data in the configuration files into the
          database and destroys all old data, including the rows with
          StorageType <c>nonVolatile</c>.  The rows created from the
          configuration file will have StorageType <c>nonVolatile</c>.
          </p>
        <p>Thus, the data in the SNMP-USER-BASED-SM-MIB, after this
          function has been called, is the data from the configuration
          files.
          </p>
        <p>All <c>snmp</c> counters are set to zero.
          </p>
        <p>If an error is found in the configuration file, it is
          reported using the function <c>config_err/2</c> of the error
          report module, and the function fails with the reason 
          <c>configuration_error</c>.
          </p>
        <p><c>ConfDir</c> is a string which points to the directory
          where the configuration files are found.
          </p>
        <p>The configuration file read is: <c>usm.conf</c>.
                    <marker id="add_user"></marker>
</p>
      </desc>
    </func>
    <func>
      <name>add_user(EngineID, Name, SecName, Clone, AuthP, AuthKeyC, OwnAuthKeyC, PrivP, PrivKeyC, OwnPrivKeyC, Public, AuthKey, PrivKey) -> Ret</name>
      <fsummary>Add one user</fsummary>
      <type>
        <v>EngineID = string()</v>
        <v>Name = string()</v>
        <v>SecName = string()</v>
        <v>Clone = zeroDotZero | [integer()]</v>
        <v>AuthP = usmNoAuthProtocol | usmHMACMD5AuthProtocol | usmHMACSHAAuthProtocol</v>
        <v>AuthKeyC = string()</v>
        <v>OwnAuthKeyC = string()</v>
        <v>PrivP = usmNoPrivProtocol | usmDESPrivProtocol</v>
        <v>PrivKeyC = string()</v>
        <v>OwnPrivKeyC = string()</v>
        <v>Public = string()</v>
        <v>AuthKey = string()</v>
        <v>PrivKey = string()</v>
        <v>Ret = {ok, Key} | {error, Reason}</v>
        <v>Key = term()</v>
        <v>Reason = term()</v>
      </type>
      <desc>
        <p>Adds a USM security data (user) to the agent config. 
          Equivalent to one line in the <c>usm.conf</c> file.</p>
        <marker id="delete_user"></marker>
      </desc>
    </func>
    <func>
      <name>delete_user(Key) -> Ret</name>
      <fsummary>Delete one user</fsummary>
      <type>
        <v>Key = term()</v>
        <v>Ret = ok | {error, Reason}</v>
        <v>Reason = term()</v>
      </type>
      <desc>
        <p>Delete a USM security data (user) from the agent config.</p>
      </desc>
    </func>
  </funcs>
  
</erlref>

