<?xml version="1.0" encoding="utf-8" ?>
<!DOCTYPE comref SYSTEM "comref.dtd">

<comref>
  <header>
    <copyright>
      <year>2011</year><year>2016</year>
      <holder>Ericsson AB. All Rights Reserved.</holder>
    </copyright>
    <legalnotice>
      Licensed under the Apache License, Version 2.0 (the "License");
      you may not use this file except in compliance with the License.
      You may obtain a copy of the License at
 
          http://www.apache.org/licenses/LICENSE-2.0

      Unless required by applicable law or agreed to in writing, software
      distributed under the License is distributed on an "AS IS" BASIS,
      WITHOUT WARRANTIES OR CONDITIONS OF ANY KIND, either express or implied.
      See the License for the specific language governing permissions and
      limitations under the License.

    </legalnotice>

    <title>snmpc</title>
    <prepared></prepared>
    <responsible></responsible>
    <docno></docno>
    <approved></approved>
    <checked></checked>
    <date></date>
    <rev></rev>
    <file>snmpc_cmd.xml</file>
  </header>
  <com>snmpc(command)</com>
  <comsummary>SNMP MIB compiler frontend</comsummary>
  <description>
    <p>The <c><![CDATA[snmpc]]></c> program provides a way to run
    the SNMP MIB compiler of the Erlang system. </p>
  </description>

  <funcs>
    <func>
      <name>snmpc [options] file.mib | file.bin</name>
      <fsummary>Compile MIBs</fsummary>
      <desc>
        <p><c><![CDATA[snmpc]]></c> compile a SNMP MIB file, 
	see <seeerl marker="snmpc#compile">compile/1,2</seeerl> for 
	more info. </p>
	<p>It can also be used to generate a header file (.hrl) 
	with definitions of Erlang constants for the objects in 
	the MIB, see 
	<seeerl marker="snmpc#mib_to_hrl">mib_to_hrl/1</seeerl>. </p>

	<marker id="options"></marker>
      </desc>
    </func>
  </funcs>

  <section>
    <title>Compiler options</title>
    <p>The following options are supported (note that most of these relate 
    to the compilation of the MIB file):</p>
    <marker id="option_help"></marker>
    <taglist>
      <tag>--help</tag>
      <item>
        <p>Prints help info.</p>
	<marker id="option_version"></marker>
      </item>

      <tag>--version</tag>
      <item>
        <p>Prints application and mib format version.</p>
	<marker id="option_verbosity"></marker>
      </item>

      <tag>--verbosity <em>verbosity</em></tag>
      <item>
        <p>Print debug info. </p>
	<p><c>verbosity</c> = <c>trace</c> | <c>debug</c> | <c>log</c> | <c>info</c> | <c>silence</c></p>
	<p>Defaults to <c>silence</c>.</p>
	<marker id="option_w"></marker>
	<marker id="option_warnings"></marker>
      </item>

      <tag>--warnings | --W</tag>
      <item>
        <p>Print warning messages. </p>
	<marker id="option_wae"></marker>
	<marker id="option_werror"></marker>
      </item>

      <tag>--wae | --Werror</tag>
      <item>
        <p>Warnings as errors. 
	Indicates that warnings shall be treated as errors. </p>
	<marker id="option_odir"></marker>
      </item>

      <tag>--o <em>directory</em></tag>
      <item>
        <p>The directory where the compiler should place the output files.
	If not specified, output files will be placed in the current working
	directory.</p>
	<marker id="option_idir"></marker>
      </item>

      <tag>--i <em>Directory</em></tag>
      <item>
        <p>Specifies the path to search for imported (compiled) MIB files. 
	By default, the current working directory is always included. </p>
	<p>This option can be present several times, each time specifying
	<em>one</em> path. </p>
	<marker id="option_ildir"></marker>
      </item>

      <tag>--il <em>Directory</em></tag>
      <item>
        <p>This option (include_lib), specifies a list of directories to 
	search for imported MIBs. It assumes that the first element in 
	the directory name corresponds to an OTP application. The compiler 
	will find the current installed version. For example, the value 
	["snmp/mibs/"] will be replaced by ["snmp-3.1.1/mibs/"] (or what 
	the current version may be in the system). The current directory 
	and the "snmp-home"/priv/mibs/ are always listed last in the
        include path. </p>
	<marker id="option_sgc"></marker>
      </item>

      <tag>--sgc</tag>
      <item>
	<p>This option (skip group check), if present, disables the 
	group check of the mib compiler. 
	That is, should the OBJECT-GROUP and the NOTIFICATION-GROUP 
	macro(s) be checked for correctness or not. </p>
	<marker id="option_dep"></marker>
      </item>

      <tag>--dep</tag>
      <item>
        <p>Keep deprecated definition(s). 
	If not specified the compiler will ignore deprecated definitions. </p>
	<marker id="option_desc"></marker>
      </item>

      <tag>--desc</tag>
      <item>
        <p>The DESCRIPTION field will be included. </p>
	<marker id="option_ref"></marker>
      </item>

      <tag>--ref</tag>
      <item>
        <p>The REFERENCE field will be included. </p>
	<marker id="option_imp"></marker>
      </item>

      <tag>--imp</tag>
      <item>
        <p>The IMPORTS field will be included. </p>
	<marker id="option_mi"></marker>
      </item>

      <tag>--mi</tag>
      <item>
        <p>The MODULE-IDENTITY field will be included. </p>
	<marker id="option_mc"></marker>
      </item>

      <tag>--mc</tag>
      <item>
        <p>The MODULE-COMPLIANCE field will be included. </p>
	<marker id="option_ac"></marker>
      </item>

      <tag>--ac</tag>
      <item>
        <p>The AGENT-CAPABILITIES field will be included. </p>
	<marker id="option_mod"></marker>
      </item>

      <tag>--mod <em>module</em></tag>
      <item>
        <p>The module which implements all the instrumentation functions. </p>
	<p>The name of all instrumentation functions must be the 
	same as the corresponding managed object it implements. </p>
	<marker id="option_nd"></marker>
      </item>

      <tag>--nd</tag>
      <item>
        <p>The default instrumentation functions will <em>not</em> be
	used if a managed object have no instrumentation function.
	Instead this will be reported as an error, and the compilation 
	aborts. </p>
	<marker id="option_rrnac"></marker>
      </item>

      <tag>--rrnac</tag>
      <item>
        <p>This option, if present, specifies that the row name assign check 
	shall not be done strictly according to the SMI (which allows only 
	the value 1). </p>
	<p>With this option, all values greater than zero is allowed (>= 1). 
	This means that the error will be converted to a warning. </p>
	<p>By default it is not included, but if this option is present 
	it will be. </p>
	<marker id="see_also"></marker>
      </item>

    </taglist>
  </section>

  <section>
    <title>SEE ALSO</title>
    <p><seecom marker="erts:erlc">erlc(1)</seecom>,
    <seeerl marker="compiler:compile">compile(3)</seeerl>,
    <seeerl marker="snmp:snmpc">snmpc(3)</seeerl></p>
  </section>
</comref>

